STRINGTABLE
LANGUAGE 9, 1
{
1, "&OK"
2, "&Cancel"
3, "&Abort"
4, "&Retry"
5, "&Ignore"
6, "&Yes"
7, "&No"
8, "&Close"
9, "&Help..."
23, "Close this dialog."
27, "Error"
28, "Warning"
32, "Yes to &All"
33, "No to All"
34, "&Syntax..."
35, "Continue"
36, "Change..."
37, "eng"
38, "English"
39, "English"
129, "\nCIR\nCIR\nCIR Files (*.cir)\n.cir\nSchematic.Document\nCIR"
130, "\nCKT\nCKT\nCKT Files (*.ckt)\n.ckt\nSpice.Document\nCKT"
131, "\nLBR\nLBR\nLBR Files (*.lbr)\n.ckt\nLibrary.Document\nLBR"
132, "\nMDL\nMDL\nMDL Files (*.mdl)\n.mdl\nModel.Document\nMDL"
150, "\nG2D\nG2D\nG2D Files (*.g2d)\n.ckt\nGraph 2D.Document\nG2D"
151, "\nMCL\nMCL\nMCL Files (*.mcl)\n.ckt\nMonte Carlo.Document\nMCL"
152, "\nG3D\nG3D\nG3D Files (*.g3d)\n.ckt\nGraph 3D.Document\nG3D"
154, "\nFFT\nFFT\nFFT Files (*.fft)\n.ckt\nfft.Document\nFFT"
161, "\nPFM\nPFM\nPFM Files (*.pfm)\n.ckt\nPerformance.Document\nPFM"
190, "Clear All"
210, "Sets all selected text to uppercase.\nUppercase"
211, "Sets all selected text to lowercase.\nLowercase"
219, "Displays current values on the schematic.\nCurrents"
220, "Displays power values on the schematic.\nPowers"
222, "Displays device conditions on the schematic.\nConditions"
224, "Device Voltage"
225, "Device Current"
226, "Device Resistance"
227, "Device Energy"
228, "Device Power"
229, "Device Charge"
230, "Device Capacitance"
231, "Device Flux"
232, "Device Inductance"
233, "Device B Field"
234, "Device H Field"
237, "Node Voltage"
238, "Digital State"
239, "Device Conductance"
240, "Device Impedance"
241, "Device Internals"
258, "%WDid not find any .SUBCKTs to encrypt."
259, "Encrypted %s .SUBCKTs"
263, "Second password entry is not the same as first password entry.\nPlease enter both passwords again."
264, "Missing file name."
296, "Utility for easily deleting common work files.\nCleanup"
302, "Yes: to Save changes for check files.\nNo: Discard all changes.\nCancel: Do nothing."
314, "Applies the display properties of the selected part to other parts of the same type.\nApply Display Attributes"
334, "Prints the values to the screen while the analysis is running.\nPrint values"
337, "When the slider method is set to Log, the Min and Max values must be greater than zero."
375, "This page controls the language that is used for some of the text in the program."
791, "Schematics"
792, "SPICE Files"
794, "Analysis Plots"
795, "3D Plots"
796, "Monte Carlo Histograms"
797, "Performance Plots"
798, "Status Bar"
799, "Go To Function"
800, "Go To X"
801, "Go To Y"
807, "%EFunction '%s' can only be used in an analysis."
808, "%EIllegal Operator. Can't use '%s' for %s with a level of %s\n%s"
809, "Opamp power supplies added."
810, "%EThe function '%s' can only be used for calculations within analysis text."
858, "Globals"
901, "&Monte Carlo"
902, "&Scope"
903, "&Probe"
912, "&Vertical"
913, "&Horizontal"
914, "Dynamic AC"
915, "Dynamic DC"
916, "Find Component..."
960, "Fourier"
999, "Lists the available model levels applicable to the component."
1001, "List of the available font names."
1002, "List of the available styles for the specified font."
1003, "List of the available point sizes for the specified font."
1004, "Specifies whether the font should appear with strikeout marks."
1005, "Specifies whether the font should appear with underlines."
1120, "Shows the security key ID number.\nKey ID"
1121, "Shows the Micro-Cap version number, program date, and RAM memory installed.\nStatistics"
1122, "Sends a screen capture of the entire window to the printer.\nPrint Active Window"
1127, "%EWrong Password."
1128, "%EYou are upgrading from MC%d but this password is only good for an upgrade from MC%d."
1226, "Adds a new model to the list."
1310, "%EAn expression must be entered for the file import command to work."
1311, "%E%s\nNo valid data was found in the specified file."
1312, "%EThe number of data points must equal or exceed the number of optimized variables for LM."
1313, "%ELM is available only when optimizing for Equates."
1348, "Replaces this circuit's properties with those from the Default Properties for New Circuits dialog box."
1349, "Replaces Default Properties for New Circuits with this circuit's properties."
1350, "This restores the internal default settings."
1363, "Browse for file names."
1368, "Sets the border color of the component."
1369, "Sets the fill color of the component."
1371, "Replaces the existing parameters with default values."
1372, "Recalls parameters under the button name."
1377, "Changes the color of the component shape."
1378, "Searches for a specified model parameter name or definition."
1379, "Import PWL data from Excel or CSV file."
1438, "This button calculates the analysis for the next frequency/temperature in the list."
1439, "This stops the analysis at the last calculated frequency/temperature."
1441, "Sets the percentage change used for a component value when using the slider or cursor keys."
1447, "Sets the first value in the display to the Magnitude."
1448, "Sets the first value in the display to the Magnitude in decibels."
1449, "Sets the first value in the display to the real part."
1450, "Turns off the first value in the display."
1451, "Sets the second value in the display to the phase in degrees."
1452, "Sets the second value in the display to the phase in radians."
1453, "Sets the second value in the display to the imaginary part."
1454, "Turns off the second value in the display."
1455, "Defines the temperature at which the analysis is run. Comma separated list."
1456, "Defines the frequency at which the analysis is run. Comma separated list."
1460, "Defines the temperature at which the analysis is run."
1461, "Shows AC values on the schematic."
1462, "Shows DC voltages on the schematic."
1532, "Type"
1533, "Value or Model"
1534, "Qty."
1535, "Power"
1536, "Total Power"
1537, "Cost"
1538, "Total Cost"
1539, "Part"
1540, "Component Memo"
1554, "Translates an MC12 schematic file to an Older version schematic file.\nConvert to Old Version."
1559, "This button calculates the analysis for the previous frequency/temperature in the list."
1587, "If enabled, places text in the schematic describing the analysis settings."
1593, "Changes which component attributes are displayed on the schematic.\nChange Attribute Display"
1614, "Retains parameter edits and lets you change the source name."
1615, "Restores the names and associated parameter values of the buttons."
1616, "Sets the color, voltage, current, resistance, and capacitance of the LED."
1622, "The scale factor (T,G,Meg,K,m,u,n,p,f) to use on the X axis of the plot."
1623, "The scale factor (T,G,Meg,K,m,u,n,p,f) to use on the Y axis of the plot."
1624, "Units (Amps,Volts,...etc) to use on the X axis of the plot."
1625, "Units (Amps,Volts,...etc) to use on the Y axis of the plot."
1626, "Defines the waveform that the Fourier window is operating on."
1627, "Defines the FFT window that will be used in the FFT calculations."
1635, "Smith Chart impedance scale factor."
1654, "Uses the standard FFT calculation method."
1655, "Uses the Fourier Integral calculation method."
1656, "Plots the magnitude: harm(expr)."
1657, "Plots the magnitude in dB: dB(harm(expr))."
1658, "Plots the real harmonics: re(ffts(expr))."
1659, "Plots the THD: THD(harm(expr))."
1660, "Plots the Harmn: harmn(expr)."
1661, "Plots the magnitude in dB: dB(harmn(expr))."
1662, "Plots the imaginary harmonics: im(ffts(expr))."
1663, "Plots the IHD: IHD(harm(expr))."
1664, "Plots the phase: ph(ffts(expr)."
1665, "Frequency to use for THD, IHD, HARMN, DB(HARMN) calculations."
1670, "Sets the upper range that the FFT window operates on."
1671, "Sets the lower range that the FFT window operates on."
1672, "Sets the number of points that the FFT functions will use."
1673, "Includes the DC harmonic when performing an autoscale."
1674, "Defines the number of harmonics that will be used in the autoscale routine."
1675, "Computes FFT Fundamental Frequency Step = 1 / (Upper Time Limit - Lower Time Limit)."
1677, "Sets the lowest level of the Fourier plots. Clips any value below this value producing a plot floor."
1679, "Ignores the phase data when the dB of the harmonic is below this value."
1681, "Plots the negative frequencies of the FFT calculations."
1728, "Enables only one group to be open in the component panel at a time."
1729, "Sets the tab position to the left of the component panel."
1730, "Sets the tab position to the right of the component panel."
1731, "Sets the tab position to the top of the component panel."
1732, "Sets the tab position to the bottom of the component panel."
1733, "Displays the component panel in the schematic editor."
1734, "Displays the list of available sections of the component panel."
1735, "Enables the file bar."
1736, "Places the file bar at the top of the window."
1737, "Places the file bar at the top of the window."
1738, "Enables tabs in the file bar."
1739, "Enables buttons in the file bar."
1740, "Displays the full path of the file in the file tabs."
1741, "Displays the file type icon in the file tabs."
1742, "Displays the Error Window."
1743, "Clears the Error Window prior to attempting a new run."
1744, "Clears the Error Window when the schematic is edited."
1745, "Shows help lines in the Error window."
1748, "Enter a string to show the list of matching commands."
1749, "Displays the current shortcut keys assigned to the command."
1750, "Defines the shortcut sequence used for the selected command."
1751, "Displays the commands currently using the specified shortcut sequence."
1752, "Assigns the specified shortcut sequence to the selected command."
1753, "Removes the defined shortcut sequence for the selected command."
1755, "Sets all shortcuts to their default values."
1756, "Assigns a toolbar icon to the selected command."
1757, "Removes the toolbar icon from the selected command."
1780, "Enables the object for simulation."
1790, "Displays the link assigned to this component in the Component Editor."
1800, "Searches files on the drive for the specified search criteria.\nFind in Files"
1833, "Defines the maximum error that a resistor combination can fall within."
1834, "Defines the maximum number of resistors that can be in parallel for a combination."
1835, "Browses the drives to find other available RES files."
1836, "Defines the file that stores the resistor values used to calculate the combinations."
1837, "Defines the maximum error that a capacitor combination can fall within."
1838, "Defines the maximum number of capacitors that can be in series for a combination."
1839, "Defines the file that stores the capacitor values used to calculate the combinations."
1840, "Browses the drives to find other available CAP files."
1841, "Defines the maximum error that a inductor combination can fall within."
1842, "Defines the maximum number of inductors that can be in parallel for a combination."
1843, "Defines the file that stores the inductor values used to calculate the combinations."
1844, "Browses the drives to find other available IND files."
1845, "Sets the format for the element values in the combination."
1846, "Sets the maximum number of resistors in the combination."
1847, "Sets the maximum number of capacitors in the combination."
1848, "Sets the maximum number of inductors in the combination."
1853, "Defines the Combination attribute with the standard values combination equivalent."
1854, "Sets the Value of the element to the closest standard value match."
1859, "Adds the selected waveform into the current plot window."
1860, "Sets the maximum amount of memory allowed to the waveform buffer."
1861, "Automatically saves waveforms from simulations into the waveform buffer."
1862, "Sets the title for the selected waveform."
1863, "Adds the selected waveform to the analysis limits for plotting on the next run."
1865, "Displays the list of all waveforms available in the waveform buffer."
1866, "Deletes the selected waveform if the Save checkbox next to the name is disabled."
1867, "Deletes all waveforms whose Save checkboxes are disabled."
1868, "%EAdding this waveform costs %s and would exceed the memory allocated for the Waveform Buffer.\nDo you want to delete waveforms and/or increase memory?"
1869, "%EThe memory allocated for the Waveform Buffer is not sufficient.\nPlease increase the memory or delete some waveforms."
1870, "%WAre you sure you want to delete all of the unchecked waveforms in the Waveform Buffer?"
1874, "Sets the default slider percentage step size."
1875, "Sets the default numeric format for the floating sliders."
1876, "Displays fixed sliders for impedances and sources during an analysis."
1877, "Sets the default slider font for the floating sliders."
1878, "Reverts the settings on this page to their default values."
1880, "Sets the initial location for a floating slider to the left of the screen."
1881, "Sets the initial location for a floating slider to the top of the screen."
1882, "Sets the initial location for a floating slider to the right of the screen."
1883, "Sets the initial location for a floating slider to the bottom of the screen."
1884, "Sets the initial location for a floating slider to floating in the window."
1885, "Sets the default file link for a component. Use %s in place of the part name."
1910, "Prints only actual simulation data points."
1911, "Prints regularly spaced data points interpolated from actual simulation data points. The number of printed points is specified in the Number of Points field in the Analysis Limits dialog box."
1936, "Selects all available types."
1937, "Deselects all highlighted types."
1938, "Selects all available models."
1939, "Deselects all highlighted models."
1940, "Selects all available parameters."
1941, "Deselects all highlighted parameters."
1942, "Applies the specified tolerances to the selected parameters."
1943, "Displays the models for all selected types."
1944, "Displays the model types available within the circuit."
1945, "Displays the parameters for all selected models."
1946, "Adds or changes the LOT tolerance for selected parameters when Apply is clicked."
1947, "Leaves the LOT tolerances unchanged for the selected parameters."
1948, "Removes the LOT tolerance from the selected parameters."
1949, "Specifies a lot# for the LOT tolerance as a means for LOT deviations to track one another."
1950, "Specifies the individual distribution to be used for the LOT tolerance."
1951, "Specifies the percentage or absolute LOT tolerance to be assigned to the parameter."
1952, "Adds or changes the DEV tolerance for selected parameters when Apply is clicked."
1953, "Leaves the DEV tolerances unchanged for the selected parameters."
1954, "Removes the DEV tolerance from the selected parameters."
1955, "Specifies a lot# for the DEV tolerance as a means for DEV deviations to track one another."
1956, "Specifies the individual distribution to be used for the DEV tolerance."
1957, "Specifies the percentage or absolute DEV tolerance to be assigned to the parameter."
1958, "Saves the specified tolerances in the parameter list to a set for future applications."
1959, "Displays a list of previously saved tolerance sets for the selected model type."
1960, "Applies the selected tolerance set to the selected models."
1961, "Deletes the selected tolerance set."
1965, "Sets the format used when adding previously unspecified parameter values to a model statement."
2016, "When enabled, all shortcut key references will be specified with the English keyboard names."
2017, "Lists the languages that are available for selection."
2039, "Model"
2041, "Browse"
2042, "Compress"
2045, "Favorites"
2051, "Search"
2052, "Beginning of line"
2053, "Name"
2054, "Memo"
2055, "Name"
2056, "Shape"
2057, "Definition"
2058, "Memo"
2059, "All"
2100, "Text"
2101, "Text Comment"
2102, "Text KeyWord"
2103, "Text Error"
2104, "Text Disabled"
2105, "Text Background"
2106, "Match Color Background"
2107, "Text Encrypted"
2110, "Text Area"
2111, "Text Area Comment"
2112, "Text Area KeyWord"
2113, "Text Area Error"
2114, "Text Area Background"
2115, "Schematic Background"
2116, "Default Grid Text"
2118, "Text Banner"
2119, "Text Banner Background"
2120, "Component"
2121, "Default Attribute Text"
2122, "Wire"
2123, "Bus"
2124, "Digital Path"
2125, "Select"
2126, "Disabled"
2127, "Block Select"
2128, "Select Box"
2129, "Node Highlight"
2130, "Node Number"
2131, "Node Voltage"
2132, "Dynamic AC Display Background"
2133, "Current"
2134, "Power/Condition"
2135, "Pin Connection"
2136, "Digital 0"
2137, "Digital R"
2138, "Digital F"
2139, "Digital 1"
2140, "Digital X"
2141, "Digital Z"
2142, "Match Color Background"
2143, "Grid"
2144, "Title Block Border"
2145, "Graph Paper"
2146, "Anchor"
2147, "Pin Markers"
2150, "Grid"
2151, "General Text"
2152, "Select"
2153, "Select Box"
2154, "Plot All"
2155, "Data Point Labels"
2156, "Tracker"
2157, "Select Color Primary"
2158, "Select Color Secondary"
2159, "Graph Background"
2160, "Baseline Color"
2161, "Window Background"
2162, "Curve 1"
2163, "Curve 2"
2164, "Curve 3"
2165, "Curve 4"
2166, "Curve 5"
2167, "Curve 6"
2168, "Curve 7"
2169, "Curve 8"
2170, "Curve 9"
2171, "Curve 10"
2172, "Label Background"
2173, "Margin Line"
2174, "Margin Arrow"
2175, "Curve Fit Color"
2176, "Anchor"
2177, "Margin Text"
2204, "Fills the button with the selected color."
2205, "Pastes a bitmap in the clipboard into the button."
2265, "Increments/decrements the value of this field"
2266, "Prints every n'th value for all curves. N is the field value."
2300, "This page specifies the color order for waveforms that use the rainbow display."
2301, "Moves the selected color up in the list."
2302, "Moves the selected color down in the list."
2303, "Adds a new entry into the color list."
2304, "Deletes the selected color from the list."
2305, "Displays the list of colors to be used for a rainbow display."
2306, "Sets the color list to its default values."
2309, "Eliminates any values outside of the tolerance band for Gaussian distributions."
2311, "Plot the first harmonic (F2)."
2312, "Plot IM2. (2'nd order intermod products)"
2313, "Plot IM3. (3'rd order intermod products)"
2315, "Sets the harmonic content at F1+F2 to the numerator of the IM2 Intermodulation Distortion ratio."
2316, "Sets the harmonic content at F1-F2 to the numerator of the IM2 Intermodulation Distortion ratio."
2317, "Sets the harmonic content at 2*F2-F1 to the numerator of the IM3 Intermodulation Distortion ratio."
2318, "Sets the harmonic content at 2*F2+F1 to the numerator of the IM3 Intermodulation Distortion ratio."
2319, "Sets the harmonic content at 2*F1-F2 to the numerator of the IM3 Intermodulation Distortion ratio."
2320, "Adds the harmonic content at 2*F1+F2 to the numerator of the IM3 Intermodulation Distortion ratio."
2321, "Includes noise contributions from an AC simulation."
2323, "Sets the harmonic content at F2 to the denominators of the IM2 or IM3 Intermodulation Distortion ratio."
2324, "Sets the IM2, IM3, or H1 denominator to 1.0."
2325, "Marks the point in the plot where the H1 curve drops 1dB below the ideal slope=1 line."
2326, "If an LO source is specified, the frequency slot choices have terms that add FL."
2327, "If an LO source is specified, the frequency slot choices have terms that subtract FL."
2328, "Calculates the point where the H1 curve crosses the IM2 curve if each has its ideal slope of 1 and 2."
2329, "Calculates the point where the H1 curve crosses the IM3 curve if each has its ideal slope of 1 and 3."
2349, "Selects the schematic page for which the color and fonts of the object apply."
2351, "Selects the fundamental frequency as the X-axis variable."
2352, "Selects the input voltage as the X-axis variable."
2353, "Selects the output voltage across the load resistor as the X-axis variable."
2354, "Selects the input power as the X-axis variable."
2355, "Selects the power of the load resistor as the X-axis variable."
2356, "Selects the peak values to be used for the X and Y values."
2357, "Selects the RMS values to be used for the X and Y values."
2365, "Creates text labels for each curve in the Distortion Window."
2366, "Defines the font for all text labels in the plot."
2370, "Selects the THD as the Y-axis variable."
2371, "Selects the THDN as the Y-axis variable."
2372, "Selects the SINAD as the Y-Axis variable."
2373, "Selects the SNR as the Y-Axis variable."
2374, "Selects one of the harmonics as the Y-Axis variable."
2375, "Selects GAIN = H1 / VIN as the Y-Axis variable."
2376, "Selects the phase of H1 as the Y-Axis variable."
2378, "Selects a specific harmonic as the Y-Axis variable."
2380, "Selects the voltage ratio for the Y-Axis variable."
2381, "Selects the power ratio for the Y-Axis variable."
2383, "Selects decibel representation for the X-Axis variable."
2384, "Selects dBm representation for the X-Axis variable."
2385, "Selects a pure number representation for the X-Axis variable."
2386, "Selects a percentage representation for the Y-Axis variable."
2387, "Selects decibel representation for the Y-Axis variable."
2388, "Selects dBm representation for the Y-Axis variable."
2389, "Selects a pure number representation for the Y-Axis variable."
2390, "Sets the selected plot to the Simple designator."
2391, "Sets the selected plot to the Literal designator."
2400, "Sets all plots to the option selected in the Y-axis Type box."
2401, "Sets all plots to the option selected in the Y-axis Designator box."
2402, "Sets all plots to the option selected in the Y-axis Show As box."
2404, "Shows previously saved distortion (and other)plots."
2405, "Lets you select a previously saved distortion plot for comparison plotting."
2406, "Sets all plots to the option selected in the X-axis Show As box."
2447, "Browses through available drives to select a name to save the numeric output file to."
2448, "Groups the sections in the numeric output file by frequency."
2449, "Groups the sections in the numeric output file by input voltage."
2450, "The scale factor (T,G,Meg,K,m,u,n,p,f) to use."
2451, "Specifies numeric format for values."
2452, "Sets the scale factor and format the same for all of the Variables to Print items."
2453, "Creates the numeric output file with the specified settings."
2454, "Automatically creates the numeric output file at the end of each simulation."
2561, "This page controls the use of threads in the program."
2562, "Enables the use of threads in the program."
2563, "Specifies the number of threads that Micro-Cap can create when running. Limited to the number of processors in the system."
2564, "This enables an extra processor to be used for plotting data points when a simulation is running."
2680, "%WUsing PSS with a circuit this large may run very slowly.\nRecommended maximum number of equations is %d. This circuit has %d."
2800, "Display the Info page in the schematic pages."
2801, "Write circuit information to the Info page."
2802, "Display warnings in the Info page."
2803, "Display the System information in the Info page."
2804, "Display symbolic variables in the Info page."
2805, "Display .Array variables in the Info page."
2806, "Display models in the Info page."
2807, "Display the .Measure information in the Info page."
2808, "Display macro and subcircuit information in the Info page."
2809, "Display items that are in the circuit but are not used in the Info page."
2810, "Display the component count in the Info page."
2811, "Show user-defined path names in Info page."
2812, "Don't show paths. Show only file names in Info page."
2813, "Adds simulation progress entries to the Info page."
2841, "Copies object data to all pages."
2903, "Create Model for this Part"
2904, "Translate to SPICE File"
2905, "Create Models for all Parts"
2999, "Finds all models that satisfy the search expression.\nBF>100 finds all devices that have a BF greater than 100."
3000, "This executes the search and fills the model list only with devices that satisfy the search expression."
3002, "The attribute name."
3003, "The attribute value. The drop-down list shows other selectable values from the schematic."
3004, "Displays the name of the attribute on the schematic."
3005, "Displays the value of the attribute on the schematic."
3007, "Available model names. Click to select."
3009, "Shows the pin names for the part on the schematic."
3010, "Shows the MOSFET binning parameters in the model parameter list."
3011, "Selects an lossy transmission line."
3012, "Selects an ideal transmission line."
3013, "Displays the prior part of the current electrical type."
3014, "Displays the next part of the current electrical type."
3015, "Shows the source location of the model statement or subckt."
3016, "Adds a new user-defined attribute."
3017, "Deletes the selected attribute."
3018, "Controls the font and color characteristics for attributes."
3019, "Expands the typing box for attributes with a lot of text."
3021, "Selects one of the characteristic curves for this part."
3022, "Plots the selected characteristic curve."
3023, "Shows calculated current values for the part on the schematic."
3024, "Shows calculated power values for the part on the schematic."
3025, "Shows condition text for the part on the schematic."
3027, "Invokes the IBIS translator for any model whose subcircuit type has been set to one of the IBIS types."
3028, "Displays the first part of the prior electrical type."
3029, "Displays the first part of the next electrical type."
3030, "This describes the syntax of the part's most important attributes, usually PART, VALUE and/or MODEL"
3031, "Sets a define variable used to describe the source parameters."
3032, "This is the magnitude of the signal used in AC analysis."
3034, "This is the phase in degrees of the signal used in AC analysis."
3036, "This is the magnitude of the signal used in DC analysis."
3037, "Plays the WAV file defined for the source."
3039, "This is the %s text. Editing makes the %s text local to this circuit and saves it in the text area."
3040, "Changes the attribute value of all parts of the current electrical type to the attribute value shown."
3055, "The piecewise linear table for the source. Syntax is [Trigger={expr}] t1,v1 t2,v2,...tn,vn"
3056, "Provides scintillating descriptions of all you see around you."
3057, "Controls the display of package pin numbers."
3058, "Controls the display of pin markers."
3059, "Lets you browse for a file name."
3060, "The initial voltage value of the source"
3061, "The initial current value of the source"
3062, "The pulsed voltage value of the source"
3063, "The pulsed current value of the source"
3064, "The time delay before the pulse"
3065, "The rise time of the pulse"
3066, "The fall time of the pulse "
3067, "The width of the pulse"
3068, "The period of the pulse"
3069, "The DC voltage offset of the sine source"
3070, "The DC current offset of the sine source"
3071, "The voltage amplitude of the sine source"
3072, "The current amplitude of the sine source"
3073, "The frequency of the sine source"
3074, "The time delay before the start of the sine source "
3075, "The damping factor in inverse seconds. Actually an inverse exponential time constant."
3076, "The phase shift in the sine wave at Time = 0."
3077, "The initial voltage value of the source"
3078, "The initial current value of the source"
3079, "The pulsed voltage value of the source"
3080, "The pulsed current value of the source"
3081, "The delay time before the rise begins measured from Time = 0"
3082, "The rise time constant"
3083, "The delay time before the fall begins measured from Time = 0"
3084, "The fall time constant"
3085, "The DC voltage offset"
3086, "The DC current offset"
3087, "The peak voltage amplitude"
3088, "The peak current amplitude"
3089, "The carrier frequency"
3090, "The modulation index"
3091, "The modulation frequency"
3092, "The interval between random changes in the source value."
3093, "The maximum amplitude of between random changes in the source value."
3094, "The time when random changes start."
3095, "The time when random changes stop."
3096, "Random number generator seed. Seed must be >0 to produce a repeatable sequence."
3097, "The peak amplitude of the source."
3098, "The time to get to the peak value."
3099, "The width in time at 50% peak amplitude."
3100, "The repetition period of the source."
3104, "\nSyntax: <value> [LOT[/#][/GAUSS|/UNIFORM|/WCASE]=[<tol>[%]] | [-<low>%,<high>%] ]\nExample: 10 Lot=10%\nExample: 10 Lot= -20%,80%"
3105, "\nSyntax: <value> [LOT[/#][/GAUSS|/UNIFORM|/WCASE]=[<tol>[%]] | [-<low>%,<high>%] ] [DEV[/#][/GAUSS|/UNIFORM|/WCASE]=[<tol>[%]]\nExample: 10 Lot=10% Dev=20%"
3106, "Selects the number of model parameter columns in the display."
3108, "When you exit the Attribute dialog box, this displays any edited object (e.g. model statement, macro)."
3170, "This selects the smooth transition version of the switch."
3171, "This selects the hysteresis version of the switch."
3180, "Normal curve with no smoothing."
3181, "Hyperbolic tangent smoothing at the corners."
3182, "Quadratic Bezier curve smoothing at the corners. Fraction is the fraction of the region over which smoothing occurs."
3184, "Fraction (0.0 to 1.0) of the rise or fall time (or PWL region) over which smoothing occurs."
3371, "Enables and sets the order of operating point convergence methods.\nOperating Point Methods"
3402, "Displays the priority of the shape groups to be used in the schematic."
3403, "The user-specified interval between bold grids."
3404, "Increases the priority of the selected shape group."
3405, "Decreases the priority of the selected shape group."
3406, "Enables the RMS calculation for the voltage, current, and power displays in the circuit."
3407, "Enables the average calculation for the voltage, current, and power displays in the circuit."
3408, "Enables the peak calculation for the voltage, current, and power displays in the circuit."
3409, "Enables the calculation of voltages and powers across devices. It does not apply to subcircuits or macros."
3410, "Specifies the number of grids in the schematic that each square in the graph paper grid will use as its length and width."
3415, "Defaults the voltage, current, and power display to show the last data point value."
3416, "Defaults the voltage, current, and power display to show the RMS value."
3417, "Defaults the voltage, current, and power display to show the average point value."
3418, "Defaults the voltage, current, and power display to show the peak value."
3423, "Sets the numeric format for path delays."
3424, "Sets the numeric format for voltage terms printed on the schematic and Dynamic AC and DC numeric output."
3425, "Sets the numeric format for .Warning messages printed on the schematic and in the numeric output."
3426, "Sets the numeric format for calculations produced from formula text."
3427, "Sets the numeric format for current terms printed on the schematic and Dynamic AC and DC numeric output."
3428, "Sets the numeric format for power terms printed on the schematic and Dynamic AC and DC numeric output."
3450, "Add to Buffer..."
3451, "Curve Line"
3452, "Curve Text"
3453, "Hide Waveform"
3454, "Retain..."
3455, "Scales and Formats..."
3456, "Export To..."
3502, "Specifies that the text is to adhere to an absolute screen location."
3503, "Specifies the text is to adhere to a location relative to a curve."
3504, "Specifies the curve to adhere to for relative text."
3620, "%WAre you sure you want to delete the directory?"
3804, "Deletes all text from the cursor position to the end of the line.\nCut to end of line"
3961, "This lets you edit Last Used Files list\nEdit Last Used File List"
3962, "Last file used list."
3963, "Removes the currently selected file name from the list."
3964, "Displays the full file path for each file reference in the File Menu, Window Menu."
3965, "Displays the path variable name in lieu of the full path name."
3966, "Disables printing the path name in window title bars."
4052, "%EMust select exactly 2 columns."
4101, "Performance or Measure function to use."
4103, "Waveform for the performance function."
4105, "Waveform for the performance function."
4107, "Performance function Boolean expression."
4115, "Guesses at a suitable set of parameters for the performance function."
4117, "Expression X"
4118, "Select the .measure that you want."
4119, "Waveform or curve for the performance function to operate on."
4120, "Waveform or curve for the performance function to operate on."
4200, "Lets you select and apply a function to one of the curves.\nGo To Function"
4240, "Enables Parallelogram Drawing mode. Click and drag to add a parallelogram.\nParallelogram Mode"
4250, "Enables Data Drawing mode. Click and drag to add a data.\nData Mode"
4251, "Enables Process Drawing mode. Click and drag to add a process.\nProcess Mode"
4252, "Enables Off-page Connector Drawing mode. Click and drag to add a Off-page Connector.\nOff-page Connector Mode"
4253, "Enables Punch Card Drawing mode. Click and drag to add a Punch Card.\nPunch Card Mode"
4254, "Enables Manual Input Drawing mode. Click and drag to add a Manual Input.\nManual Input Mode"
4255, "Enables Predefined Process Drawing mode. Click and drag to add a Predefined Process.\nPredefined Process Mode"
4256, "Enables Internal Storages Drawing mode. Click and drag to add a Internal Storages.\nInternal Storages Mode"
4257, "Enables Manual Operation Drawing mode. Click and drag to add a Manual Operation.\nManual Operation Mode"
4258, "Enables Document Drawing mode. Click and drag to add a Document.\nDocument Mode"
4259, "Enables Multidocument Drawing mode. Click and drag to add a Multidocument.\nMultidocument Mode"
4260, "Enables Stored Data Drawing mode. Click and drag to add a Stored Data.\nStored Data Mode"
4261, "Enables Delay Drawing mode. Click and drag to add a Delay.\nDelay Mode"
4262, "Enables Summing Junction Drawing mode. Click and drag to add a Summing Junction.\nSumming Junction Mode"
4263, "Enables Or Drawing mode. Click and drag to add a Or.\nOr Mode"
4264, "CollateEnables Collate Drawing mode. Click and drag to add a Collatey.\nCollate Mode"
4265, "Enables Sort Drawing mode. Click and drag to add a Sort.\nSort Mode"
4266, "Enables Preparation Drawing mode. Click and drag to add a Preparation.\nPreparation Mode"
4267, "Enables Terminator Drawing mode. Click and drag to add a Terminator.\nTerminator Mode"
4268, "Enables Punched Tape Drawing mode. Click and drag to add a Punched Tape.\nPunched Tape Mode"
4269, "Enables Sequential Access Storage Drawing mode. Click and drag to add a Sequential Access Storage.\nSequential Access Storage Mode"
4270, "Enables Magnetic Disk Drawing mode. Click and drag to add a Magnetic Disk.\nPunched Magnetic Disk"
4271, "Enables Direct Access Storage Drawing mode. Click and drag to add a Direct Access Storage.\nPunched Direct Access Storage"
4272, "Enables Display Drawing mode. Click and drag to add a Display.\nDisplay Mode"
4273, "Enables Alternate Process Drawing mode. Click and drag to add a Alternate Process.\nAlternate Process Mode"
4274, "Enables Decision Drawing mode. Click and drag to add a Decision.\nDecision Mode"
4275, "Enables Connector Drawing mode. Click and drag to add a Connector.\nConnector Mode"
4276, "Enables Extract Drawing mode. Click and drag to add a Extract.\nExtract Mode"
4277, "Enables Merge Drawing mode. Click and drag to add a Merge.\nMerge Mode"
4298, "Edit Styles..."
4299, "Edit Styles"
4300, "Changes the style of selected item.\nStyle"
5253, "Specifies the pin names of the bus connector."
5254, "Specifies the part name for the bus connector."
5255, "Specifies the grid spacing between pins on the bus connector."
5256, "Specifies the wire node alignments on the bus connector."
5257, "Specifies the bus node position on the bus connector."
5262, "%EAt least one pin name must be specified for the bus."
5355, "%EThis File is not a recognizable format."
5360, "%EObsolete data file, please rerun the simulation."
5365, "%EFiles with this extension are not loadable '%s'"
5400, "Accesses the State Variables Editor.\nState Variables"
5402, "Sets all voltages and currents to 0.0 and all digital levels to X."
5403, "Reads the state variables from a file created by the Write button."
5404, "Writes the state variables to a file."
5405, "Prints the state variables to a text file and a window."
5406, "Creates .IC statements and places them in the text area of the schematic."
5410, "The voltage value on the indicated node"
5411, "The current value on the indicated inductor"
5412, "The digital level on the indicated node"
5414, "Sets the format used for the voltages and currents."
5415, "Creates .NODESET statements and places them in the text area of the schematic."
5490, "%EThe values in the Variable 1 Range field must be positive."
5491, "%WM = m = .001\nIf you want 1e6, then use 1Meg\n\nDo you want to edit this?\n"
5500, "%EA list value is missing after a comma in the expansion list. E.g: '[A,]'\n%s"
5501, "%EA comma or colon may be missing in the expansion list. E.g: '[A B]'\n%s"
5502, "%EThe ending bracket ']' is missing in the expansion list. E.g: '[A,B'\n%s"
5514, "Finds the change in the X expression when the Y expression passes from Low to High."
5515, "Finds the change in the X expression when the Y expression passes from High to Low."
5516, "Finds the N'th local maximum of the X expression."
5517, "Finds the N'th local maximum of the Y expression."
5518, "Finds the N'th local minimum of the X expression."
5519, "Finds the N'th local minimum of the Y expression."
5520, "Finds the N'th local peak to valley change of the Y expression."
5521, "Finds the N'th period of the Y expression. Period is the X difference of successive points passing through the Y average value."
5522, "Finds the N'th frequency of the Y expression. Frequency is the inverse of the X difference of successive points passing through the Y average."
5523, "Finds the N'th X difference of successive points passing through the specified Y Level."
5524, "Finds the largest value of the X expression on the current branch."
5525, "Finds the largest value of the Y expression on the current branch."
5526, "Finds the smallest value of the X expression on the current branch."
5527, "Finds the smallest value of the Y expression on the current branch."
5528, "Finds the X value at the N'th instance where the Y expression equals the specified Y Level."
5529, "Finds the Y value at the N'th instance where the X expression equals the specified X Level."
5530, "Finds the X difference at the N'th instance of the expression Y range."
5531, "Finds the Y difference at the N'th instance of the expression X range."
5532, "Finds the X min to max range within the N'th instance of the specified Y range."
5533, "Finds the Y min to max range within the N'th instance of the specified X range."
5534, "Finds the slope (delta Y / delta X) at the N'th instance of the specified X value."
5535, "Finds the phase margin of expression. DB(expr) and PH(expr) must be plotted or printed."
5536, "Finds the RMS value of the waveform between XMin and XMax."
5537, "Finds the average value of the waveform between XMin and XMax."
5538, "Finds the Gain Margin."
5539, "Finds the Integral of an expression."
5540, "Finds the Peak to Peak value."
5541, "Finds the phase angle between two sinusoidal waveforms in transient analysis."
5550, "%EThe %s function also requires '%s' to be plotted."
5551, "%EThe %s function requires PH(expr) or DB(expr) to be plotted."
5552, "Warning, there is no performance plot because nothing was stepped."
5600, "Absolute current tolerance. Specifies the absolute tolerance to be added to the relative current tolerance."
5601, "This parameter is like ABSTOL but applies only to charge variables."
5602, "Ground shunt capacitance value implicitly placed at each node in the circuit. A value of 0 means no capacitor is present."
5603, "MOSFET default drain area."
5604, "MOSFET default source area."
5605, "MOSFET default length."
5606, "MOSFET default width."
5607, "MOSFET default number of squares for drain resistor"
5608, "MOSFET default number of squares for source resistor"
5609, "MOSFET default drain diode periphery"
5610, "MOSFET default source diode periphery"
5611, "Minimum drive (forcing) resistance for digital IO models."
5612, "Maximum drive (high impedance) resistance for digital models."
5613, "Default maximum error message limit for individual digital constraint devices."
5614, "Default maximum error message limit for all digital devices during each analysis run."
5615, "The minimum digital time step is 1 / DIGFREQ."
5616, "Initial state of flip-flops and latches: 0=clear, 1=set, 2=X."
5617, "Default digital IO level, 1 to 4. Specifies one of four DtoA and AtoD interface circuits."
5618, "Specifies the default digital delay: 1=Min, 2=Typical, 3=Max, 4=Min/Max."
5619, "Specifies scale factor used to calculate unspecified minimum delays from specified typical delays."
5620, "Minimum ratio of drive resistances for one gate to over drive another driving the same node."
5621, "Specifies scale factor used to calculate unspecified maximum delays from specified typical delays."
5622, "Specifies the minimum branch conductance."
5623, "Operating point iteration limit before supply relaxation is attempted."
5624, "DC transfer curve iteration limit for each point of the DC sweep."
5625, "Transient analysis iteration limit for each time point."
5626, "Suppresses simulation error messages in output file for digital devices."
5627, "Minimum relative value required of a pivot in the matrix solver."
5628, "Minimum absolute value required of a pivot in the matrix solver."
5629, "Sets the relative voltage and current tolerance."
5630, "The number of standard deviations in the tolerance band."
5631, "Default model parameter measurement and analysis temperature."
5632, "This is the amount by which the standard LTE formulas are presumed to overestimate the true error."
5633, "Compacts the past history of lossy transmission line input voltages and current."
5634, "Specifies the absolute voltage tolerance to be added to the relative voltage tolerance."
5635, "Controls input and output column width. Must be either 80 or 132."
5636, "Enables private digital libraries."
5637, "Enables private analog libraries."
5638, "Selects Euler integration."
5639, "Selects Gear integration."
5640, "Selects trapezoidal integration."
5641, "Sets the minimum absolute value of the resistance of a resistor or an active device lead resistance, (e.g. BJT RB, RE, and RC)."
5642, "Specifies the resistance to use when adding a resistive path to ground."
5643, "Selects older MC6 style of numeric derivatives rather than the newer algebraic derivatives for behavioral models. This is faster for some circuits."
5644, "Logic threshold for use with the SPICE3 Boolean operators, & (AND), | (OR), and ~ (NOT),IF..."
5645, "Logic ONE for use with the SPICE3 Boolean operators, & (AND), | (OR), and ~ (NOT) ,>, >=,<,<=..."
5646, "Logic ZERO for use with the SPICE3 Boolean operators, & (AND), | (OR), and ~ (NOT),>, >=,<,<=..."
5647, "Restores default values suitable for most circuits."
5648, "Restores default values suitable for high power circuits."
5649, "Writes the current global settings to a .Options statement within the loaded circuit."
5650, "The seed must be >0 to produce a repeatable sequence."
5651, "Ground shunt resistance value implicitly placed at each node in the circuit. A value of 0 means no resistor is present."
5652, "Parallel resistance value implicitly placed across all current sources. A value of 0 means no resistor is present."
5653, "Sets the precision for S and H devices."
5654, "Sets the interpolation order for FFT spectra."
5655, "Selects the number of data points on each side of a data point that must satisfy a performance function search."
5656, "Checks for valid DC paths to ground at each node."
5657, "Checks for loops containing only voltage defined elements such as sources and inductors."
5658, "Generates an error if less than two connections per node."
5659, "Maximum temperature-adjusted diode IS value."
5801, "Selects scientific notation."
5802, "Selects engineering notation."
5803, "Selects decimal notation."
5804, "Select standard notation."
5805, "Sets the number of digits."
5806, "Sets the number of digits."
5900, "Bolds the selected text.\nBold"
5901, "Italicizes the selected text.\nItalic"
5902, "Underlines the selected text.\nUnderline"
5903, "Places a strikethrough through the selected text.\nStrikethrough"
5904, "Sets the selected text as a superscript. (RTF only)\nSuperscript"
5905, "Sets the selected text as a subscript. (RTF only)\nSubscript"
5906, "Sets the color of the selected text.\nFont Color"
5907, "Sets the background color of text.\nText Background Color"
5908, "Sets the background color of the selected text. (RTF only)\nText Highlight Color"
5909, "This color combined with the Font Color will create a gradient color.\nFont Gradient Color"
6201, "Sends an email to Spectrum support."
6300, "Toggles between contour and 3D plot.\nToggle Contour"
6301, "Shows the X view of the 3D plot.\nX View"
6302, "Shows the Y view of the 3D plot.\nY View"
6303, "Shows the Z view of the 3D plot.\nZ View"
6304, "Rotates the 3D plot clockwise about the X axis.\nRotate X Axis"
6305, "Rotates the 3D plot clockwise about the Y axis.\nRotate Y Axis"
6306, "Rotates the 3D plot clockwise about the Z axis.\nRotate Z Axis"
6307, "Rotates the 3D plot counterclockwise about the X axis.\nRotate counterclockwise X Axis"
6308, "Rotates the 3D plot counterclockwise about the Y axis.\nRotate counterclockwise Y Axis"
6309, "Rotates the 3D plot counterclockwise about the Z axis.\nRotate counterclockwise Z Axis"
6404, "Automatically creates the title from the selected performance function or waveform expression."
6405, "Creates a contour plot."
6406, "Adds a background to each axis."
6407, "Adds an axis line to each of the three axes."
6408, "Adds a grid to each axis."
6409, "Adds a numeric scale to each axis."
6410, "Adds constant-valued X and Z lines to the plot."
6411, "Adds a flashing cursor when in Cursor mode."
6422, "Sets the number of patches along the X axis."
6423, "Sets the number of patches along the Z axis."
6425, "Uses no patch color."
6426, "Uses a spectrum of colors from red to violet."
6427, "Uses gray shades only."
6428, "Uses blue shades only."
6429, "Uses red shades only."
6430, "Uses green shades only."
6431, "Uses a spectrum of colors defined by the User Color 1 and User Color 2 objects."
6440, "Text Color"
6441, "Grid Color"
6442, "Isolines Color"
6443, "X Axis Plane Color"
6444, "Y Axis Plane Color"
6445, "Z Axis Plane Color"
6446, "Window Background Color"
6447, "Select Color"
6448, "Select Box Color"
6449, "User Color 1"
6450, "User Color 2"
6451, "Anchor Color"
6600, "This panel lets you enable or disable Did You Know messages."
6601, "This enables the message for the Alt + double-click grid text edit option."
6602, "This enables the message for the distortion analyses."
6603, "This enables the message for the Alt Wire + double-click option."
6604, "This enables the message for the Calculator right-click functions."
6605, "This enables the message about the user created models in the Model program."
6606, "This enables the message describing the user model when one is added."
6607, "This enables the message about the optimization routines available."
6608, "This enables the message about the Smoke Analysis."
6704, "Enables the creation of the Numeric Output file."
6705, "Writes model parameters to the Numeric Output file."
6706, "Writes Monte Carlo and Stepping limits to the Numeric Output file."
6707, "Writes waveform values with enabled Numeric Output buttons to the Numeric Output file."
6708, "Writes operating point information to the Numeric Output file."
6709, "Writes individual component noise contributions at each frequency."
6710, "Writes zero-valued model parameters to the Numeric Output file."
6711, "Writes undefined model parameters to the Numeric Output file."
6712, "Defines an alias for the waveform expression to be used as the column header."
6713, "Displays the list of all waveforms available for numeric output."
6714, "Defines the format that the waveform columns will be placed in."
6715, "Checks all of the waveform checkboxes for numeric output."
6716, "Clears all of the waveform checkboxes for numeric output."
6717, "Increases the order priority of the waveform column for the selected expression."
6718, "Decreases the order priority of the waveform column for the selected expression."
6719, "Writes the main header specified under the Header tab to the Numeric Output file."
6720, "Writes the waveform headers at the top of the waveform value columns to the Numeric Output file."
6721, "Writes the branch header information such as temperature, step, or Monte Carlo run to the Numeric Output file."
6722, "Defines the low X value that the Numeric Output waveform values will be limited to."
6723, "Defines the high X value that the Numeric Output waveform values will be limited to."
6724, "Sets the numeric format for operating point data in the numeric output file."
6726, "Hides all of the waveforms in the list that are not selected for numeric output."
6727, "Specifies the format for the X values of the selected curve in the numeric output."
6728, "Specifies the format for the Y values of the selected curve in the numeric output."
6729, "Writes any measurement calculations specified by .Measure statements to the Numeric Output file."
6730, "When enabled, all duplicated Y Expressions will be included in the numeric output."
6731, "User file name for numeric output."
6732, "Automatic file name for numeric output."
6733, "Include tolerance details"
6801, "Did you know that you can edit the text directly in the schematic by double\nclicking on the text when in Select mode while holding the ALT key down?"
6802, "Did you know that Distortion Analysis has changed since MC9,\nallowing plots of THD, THDN, and SNR vs VOUT, POUT and much more?"
6803, "Did you know that you can select all segments of a wire with ALT + click?"
6804, "Did you know that you can right-click in the calculator box to add functions?"
6805, "Did you know that you can now create a user part which lets you optimize subcircuits, macros, or models of your own creation?"
6806, "You can now select a circuit to optimize and which analysis to use.\nClick on a Parameters '...' button to add a Parameter to optimize.\nAlso you may add more graphs. Double click in the graph title to change it.\nDouble click in the data column title to change the waveform that is being optimized."
6807, "There are now four different optimizer methods: Powell, Hooke, LM, and DE.\nGo to the Model's Optimizations Settings to select which ones to use."
6808, "Did you know that Transient Analysis now has a Smoke / Stress analysis?"
7049, "Smoke Help..."
7202, "Part Name."
7203, "Source Field. (used as a comment only)"
7204, "Memo Field Used in Component Library."
7205, "Author Field.(used as a comment only)"
7230, "Data Sheet Values."
7300, "Measurement Conditions."
7301, "Measurement Conditions."
7303, "Defines the analysis used with the specified circuit file."
7304, "Defines the circuit file that will be used for the optimization."
7305, "Browse for the circuit file that will be used for the optimization."
7306, "Imports data into the data fields from a CSV or numeric output file.\nImport Data"
7307, "When enabled, the optimization will use the Local Optimization Settings over the Global Optimization Settings."
7308, "When enabled, the error difference will be calculated using a log difference rather than a linear difference."
7309, "Copies the status of the Use Local Settings option to all graphs in the file.\nCopy Use Local Settings status to all graphs"
7310, "Copies the status of the Use Local Settings option to all graphs of the same type in the file.\nCopy Use Local Settings status to identical graphs"
7311, "Copies the status of the Use Log Error option to all graphs in the file.\nCopy Use Log Error status to all graphs"
7312, "Copies the status of the Use Log Error option to all graphs of the same type in the file.\nCopy Use Log Error status to identical graphs"
7313, "Exports a summary of the optimized parameters to a text file or an Excel file.\nExport Data"
7320, "Lets you add, edit, or remove parameters to optimize for this graph."
7404, "%EThe measurement condition '%s' already exists for this graph."
7405, "%EThe expression %s vs. %s is not being plotted in the associated circuit file."
7406, "%EToo many data points are being entered through the Fill Data dialog box."
7407, "%ECould not find the original template to add the part:\nFile=%s\nName=%s."
7408, "%EThe file specified in the Circuit field must be a Micro-Cap schematic file (*.CIR)."
7410, "Lets you add, edit, or remove measurement conditions for this graph."
7420, "%ENo parameters have been defined to be optimized in the Parameters section."
7421, "%ENumber of columns in a clipboard paste too big."
7450, "%EUnknown parameter name %s."
7500, "%EFailed to run Excel."
7802, "Numeric format of values shown in the Rated Value column."
7805, "Numeric format of values shown in the Derating Percentages Value column."
7808, "Numeric format of values shown in the Derated for Reliability column."
7811, "Numeric format of values shown in the Derated for Reliabity and Temperature column."
7814, "Numeric format of values shown in the Measured Value column."
7817, "Numeric format of values shown in the Percent of Derated Value column."
7831, "Smoke"
7834, "Adjusts column widths to fit the Smoke window."
7840, "Export Data..."
7853, "Shows an info box describing column titles and parameter names beneath the mouse."
7854, "Shows invalid tests."
7855, "A list of the part names for specifying valid tests."
7856, "A list of the device types for specifying which Smoke parameters to display."
7857, "A list of the Smoke parameters to display for the selected device type."
7858, "Shows the sign (+ -) of measured Smoke parameters."
7859, "Selects all parts"
7860, "Deselects all parts"
7862, "A check mark signifies that the test is valid."
7863, "Sets all parameters to valid or invalid as set in the Default Properties for New Circuits dialog box."
7864, "Sets all parameters to valid."
7865, "Sets all parameters to invalid."
7869, "%WWarning this overwrites many user settings. Are you sure you wish to continue?"
7873, "List of selected library files."
7874, "Adds a library file to the list."
7875, "Removes a library file from the list."
7876, "Lets you select a different file name to replace the currently selected name."
7877, "Moves selected file up one position in the list. Does not affect usage."
7878, "Moves selected file down one position in the list. Does not affect usage."
9000, "Load sample circuit '%s' %s"
9900, "Search sample circuits.\nSearch sample circuits"
10094, "Text File (*.csv)|*.csv|"
10095, "Excel (*.xls;*.xlsx)|*.xls;*.xlsx|"
10096, "Worst Case Tolerance Library (*.TLIB)|*.tlib|"
10097, "Derating Library (*.DLIB)|*.dlib|"
10098, "Title Block (*.TBK)|*.tbk|"
10099, "Waveform audio format (*.Wav)|*.wav|"
10102, "Numeric Output (*.HDNO)|*.HDNO|"
10103, "Numeric Output (*.IDNO)|*.IDNO|"
10104, "All Files (*.*)|*.*|Numeric Output (*.TNO;*.ANO;*.DNO;*.HNO;*.INO)|*.tno;*.ano;*.dno;*.hno;*.ino|CSV (Comma Delimted)(*.CSV)|*.CSV|"
10105, "LTSpice Schematics (*.ASC;*.APP)|*.asc;*.app|"
10106, "Waveform (*.USR)|*.USR|CSV (Comma Delimted)(*.CSV)|*.CSV|Waveform audio format (*.Wav)|*.wav|"
10107, "SPICE Circuit (*.CKT)|*.CKT|"
10108, "SPICE Stim (*.STM)|*.STM|"
10109, "Touchstone File (*.S*P;*.Z*P;*.Y*P;*.G1P;*.G2P;*.H1P;*.H2P;*.T1P;*.T2P;*.A1P;*.A2P)|*.S*P;*.Z*P;*.Y*P;*.G1P;*.G2P;*.H1P;*.H2P;*.T1P;*.T2P;*.A1P;*.A2P|"
10110, "Numeric Output (*.TNO)|*.tno|"
10111, "Numeric Output (*.ANO)|*.ano|"
10112, "Numeric Output (*.DNO)|*.dno|"
10114, "SPICE library (*.LIB)|*.LIB|Model Library (*.LBR)|*.LBR|"
10115, "Script (*.BAT)|*.BAT|"
10118, "Bill Of Materials (*.BOM)|*.bom|"
10119, "SPICE (*.CKT;*.STM)|*.CKT;*.STM|"
10120, "Macro (*.MAC)|*.MAC|"
10121, "Schematic (*.CIR)|*.CIR|"
10122, "SPICE library (*.LIB)|*.LIB|"
10123, "Model Library (*.LBR)|*.LBR|"
10124, "Model Data (*.MDL)|*.MDL|"
10125, "All Files (*.*)|*.*|"
10126, "Component (*.CMP)|*.cmp|MC5 Component (COMP*.MC5)|comp*.mc5|MC4 Component (CS*.MC4)|cs*.mc4|"
10127, "Component (*.CMP)|*.cmp|"
10128, "Component (*.CMP)|*.cmp|MC5 Component (COMP*.MC5)|comp*.mc5|"
10129, "Shape (*.SHP)|*.SHP|MC5 Shape (shape*.mc5)|shape*.mc5|"
10130, "Shape (*.SHP)|*.shp|"
10131, "Monte Carlo (*.TNO;*.ANO;*.DNO;*.SNO)|*.tno;*.ano;*.dno;*.sno|"
10132, "IBIS (*.IBS)|*.IBS|"
10133, "Schematic (*.CIR)|*.CIR|Macro (*.MAC)|*.MAC|"
10134, "Text File (*.txt)|*.txt|"
10138, "Capacitor File (*.CAP)|*.cap|"
10139, "Resistor File (*.RES)|*.res|"
10140, "Inductor File (*.IND)|*.ind|"
10141, "Waveform (*.USR)|*.usr|"
10142, "Package (*.PKG)|*.pkg|"
10143, "Standard Passive Values (*.RES;*.CAP;*.IND)|*.res;*.cap;*.ind|"
10144, "State Variable (*.TOP)|*.top|"
10147, "subckt (*.LIB;*.CKT)|*.lib;*.ckt|"
10148, "Data File (MCAP.DAT,MC5.DAT)|mcap.dat;mc5.dat|"
10149, "JEDEC (*.JED)|*.jed|"
10150, "%EError in command line '%s'."
10151, "Upper Time Limit"
10152, "Lower Time Limit"
10153, "Upper Frequency Limit"
10154, "Lower Frequency Limit"
10155, "%EThe number of data points must be a power of 2 chosen from the set {8,16,32,64,128,256,512,1024,2048,4096,8192...1048576}."
10156, "%ELower Time Limit must be less than the Upper Time Limit"
10157, "%EUpper Frequency Limit must be greater than zero"
10188, "This page lets you edit the names of the component palettes and toggle them on or off."
10189, "This page lets you set which icons are displayed in the main tool bar."
10190, "This page lets you add or edit font styles used in the program."
10191, "This page controls the appearance and position of the Component panel"
10192, "This page lets you add, edit, or delete shortcut key combinations."
10193, "This page lets you adjust the settings used when trying to calculate combination or single values of RLC parts."
10194, "This page controls the initial font, format, position, and step size of sliders."
10195, "This page controls the appearance and position of the Window tabs."
10196, "This page controls the Error Window."
10200, "The name of the selected style."
10201, "Adds a new style to the list."
10202, "Deletes the selected style."
10203, "Sets a predefined style that will be used for the text."
10401, "%EUnknown identifier '%.200s'."
10402, "%EUnknown identifier '%s' in '%.200s'."
10403, "%EOperand expected in '%.200s'."
10404, "%EIllegal constant '%s' in '%.200s'."
10405, "%EFound unexpected ')' in '%.200s'."
10406, "%EMissing ').' in '%.200s'."
10407, "%EOperator expected '%.200s'."
10408, "%EIllegal node name '%.200s' in '%.200s'."
10409, "%EFormula too complex in '%.200s'."
10410, "%EMissing expression in '%.200s'."
10411, "%EMissing expression."
10412, "%EGlobal designators can only have references to a single type in the statement.\nText:\t%s"
10413, "%ECan't find label '%s' in %s(...)"
10414, "%ECan't find device between nodes %s and %s in %s(...)."
10415, "%EMore than one device found between nodes %s and %s in %s(...)."
10416, "%EIllegal expression using %s(%s)."
10417, "%EExpecting '(' to follow '%s' in '%.200s'."
10418, "%EExpression not allowed in function '%.200s'."
10419, "%ENot enough parameters found in function '%.200s'."
10420, "%EToo many parameters found in function '%.200s'."
10421, "%ECan't use expression '%s' in Harmonic Distortion analysis."
10422, "%ECan't use '%s' in function '%s' on arg. no. '%s'\nfor expression %.200s."
10423, "%ECan't nest case."
10424, "%EMissing or invalid expression."
10425, "%ECan only use expression '%s' in analysis limit dialog box."
10426, "%ECan't use expression '%s' in AC analysis."
10427, "%ECan't use expression '%s' in DC analysis."
10428, "%ECan't use expression '%s' in Transient analysis."
10429, "%ECan't Mix %s."
10430, "%ETable is missing last Yn parameter."
10431, "%ENesting to deep."
10432, "%ECan not calculate '%s' at this time. '%.200s'."
10433, "%EIllegal index variable '%s' in Series '%s'."
10434, "%ECan't calculate '%s' at this time."
10435, "%ECan't find waveform '%s' in '%s'."
10436, "%ECan't use '%s' \nfor expression %.200s."
10437, "%EThe second derivative parameter must be just one variable, not an expression."
10438, "%EFor the %s function, the plotted X expression must be 'F' and the plotted Y expression must be of the form  'db(expr)' or 'ph(expr)'."
10439, "%ELast(expr,n) n must be a constant integer and greater than or equal to zero."
10440, "%ECondition missing ':'."
10441, "%ECondition missing '?'."
10442, "%EThe current for the device in the expression %s is not available to be used directly."
10443, "%EAn attempt was made to access the array variable %s outside its bounds."
10444, "%EA stack overflow occurred in an array variable. It probably contains a self-reference."
10445, "%EThe argument of the RNDI function is the time interval between random values and must be a positive, non-zero constant, like 10ns."
10446, "%ENot enough indexes found in the reference to .array '%.200s'.\nDimensions needed %s."
10447, "%EToo many indexes found in the reference to .array '%.200s'.\nDimensions needed %s."
10448, "%EOnly positive integers are allowed for dimension specifications for .Array '%s'."
10449, "%EThe Array element has exceeded the maximum number of dimensions limit."
10450, "%EThe Array reference produces an expression that is too complex."
10451, "%EA dimension value is missing within the .Array statement."
10452, "%ECan't use '%s' within a Der operator."
10453, "%EIllegal index variable '%s' in Prod '%s'."
10454, "%EAC current and power variables are not available for devices of type EKV, BSIM3, or BSIM4."
10455, "%ETransient/Distortion charge and capacitance variables are not available for devices of type EKV."
10456, "%ECan't use expression '%s' in Intermodulation Distortion analysis."
10457, "%EThe designator for the branch selection operator (@) must be greater than 0."
10458, "%EBranch selection operators (@) cannot be nested."
10459, "%EThe branch selection operator (@) cannot be used with a '%s' function."
10460, "%EThe nonlinear core expression %s(%s) is not available for this inductor."
10461, "%ECan't use %s with an Array."
10462, "%EExpected to find an array in %s"
10463, "%EThe wrong number of parameters are specified in the measurement call."
10464, "%EThe variables referenced in a .Measure statement can not be changed during a run."
10465, "%ECan't use expression '%s' in Stability analysis."
10466, "%ECan not do math with Add() Function."
10467, "Not Available"
10496, "%EPlease select the name of the load resistor."
10497, "%EA value must be specified in the Number of Harmonics in THD field."
10498, "%EA source must be specified in the Input Source Name field."
10499, "%EThe source specified in the Input Source Name field is not a valid sine source."
10500, "%ECircuit must have a Voltage Source or Current Source component with type of Sin or a Sine Source."
10501, "%WThe Max Simulation Cycles field must have a minimum value of 4."
10502, "F1 must be less than F2."
10503, "%EF1 must be greater than zero."
10504, "%EAt least one Numerator must be selected to plot IM2."
10505, "%EAt least one Numerator must be selected to plot IM3."
10506, "%EAt least one Denominator must be selected to plot IM2 or IM3."
10507, "%ECan't find the specified load resistor."
10508, "%EPlease select the name of the source resistor."
10509, "%ECan't find the specified Source Resistor."
10510, "%EThe source specified in the Name of LO Source field is not a valid sine source."
10511, "%EA source must be specified in the Name of LO Source field."
10512, "\nEnable expressions must be made up of just Checks and Booleans."
10582, "Name of source resistor."
10592, "%EThe symbolic derivative has exceeded the specified size limit."
10595, "*** Warning any changes made to this page will be overwritten when an analysis is entered."
10596, " is 'Used'"
10597, " is 'Not Used'"
10598, " on page '%s'"
10599, " found in '%s' on page '%s'"
10600, " from page '%s'"
10601, " found in '%s'"
10602, "Automatically added for the A to D interface."
10603, "%sA/D interface added between %s and new node %s due to digital part %s."
10604, "Main found in '%s'"
10605, "'%s' included"
10606, "Part '%s' called from '%s' calls %s '%s'"
10607, "Not Found"
10608, "Components:"
10609, "Files Used:"
10610, "Analog Nodes = %d"
10611, "Digital Nodes = %d"
10612, "Passed Value"
10613, "System:"
10614, "Data Points:"
10615, "Timings:"
10616, "Warnings:"
10621, "%EMissing vn value in PWL."
10622, "%ENeed at least two values for '%s'."
10623, "%WStimulus not supported in PWL."
10624, "%EMissing FOR value in PWL."
10625, "%EExpecting FOR or FOREVER in PWL."
10626, "%EENDREPEAT before REPEAT in PWL"
10627, "%EMissing ENDREPEAT in PWL."
10629, "%WMissing Value after TIME_SCALE_FACTOR."
10630, "%EMissing Value after VALUE_SCALE_FACTOR."
10631, "%ETime must be in ascending order."
10632, "%EEmpty REPEAT ENDREPEAT block in PWL."
10633, "%ETIME_SCALE_FACTOR can not be zero."
10634, "%EWIDTH must be positive."
10635, "%EIllegal value '%.1000s'."
10636, "%EIllegal value '%s' in spice source.\nValue must be greater than 0."
10791, "%EBad controlling node '%s' in source."
10792, "%EToo many dimensions in source."
10793, "%EMissing controlling node in source."
10794, "%EBad label or too few labels in source."
10795, "%EToo many coefficients in source."
10798, "%EExpressions used in poly coefficients require curly brackets '{' '}'."
10799, "%ECan't find the source '%s'."
10800, "%EVALUE syntax can be used on E and G devices only."
10802, "%EError in coupling device. Inductor %s not found."
10803, "%EError in coupling device. Inductor %s found more than once."
10804, "%EError in coupling device. Too many inductors."
10806, "%EError in coupling device. Missing K value."
10808, "%EError in coupling device. Must have more than one inductor name."
10809, "%EError in coupling device. Cross linked %s %s."
10810, "%EError in coupling device. '%s' '%s' already coupled."
10811, "%EError in coupling device. Missing inductor names."
10818, "%EMismatched braces.\nMissing '%c' in table source."
10819, "%EMismatched braces.\nExtra '%c' in table source."
10820, "%E.Spice commands not allowed in a .Subckt."
10821, "%EThe .EndSpice statement must be located in the same file as the .Spice statement."
10822, "%EThe .EndSpice not allowed in a .Subckt."
10823, "%EThere is no corresponding .EndSpice statement for the specified .Spice statement."
10824, "%E.EndSpice found with no matching .Spice."
10825, "%EA .Spice statement is not allowed to be nested within another .Spice statement."
10826, "%ECan't find the voltage source specified in the REF attribute: '%s'."
10827, "%WThe F and S variables are only available for use in the transmission line in an AC analysis.\nIn other analysis modes the F variable is set to zero."
10828, "%WPart names have been changed.\n%s"
10829, "%EK devices may not reference inductors with nonlinear flux or inductance expressions."
10831, "%EThe circuit is missing a ground."
10833, "%ESyntax in table source."
10834, "%EMissing model statement '%s'."
10835, "%EIllegal switch VALUE attribute %s."
10836, "%EK value must be >= -1.0 and <= 1.0."
10837, "%EThe Charge attribute expression must have V(%s) in its expression or else the Capacitance attribute must be defined."
10838, "%EThe SPICE circuit is missing a ground node."
10839, "%EAlready have a DC value."
10840, "%EArea must be positive."
10841, "%EMust specify part name."
10842, "%ELess than two connections at analog node %s."
10843, "%EThe Flux attribute expression must have I(%s) in its expression or else the Inductance attribute must be defined."
10844, "%EUnknown keyword %s."
10845, "%EOnly one of the magnitude keywords MAG, DB, or R_I may be used in a Laplace Table source."
10846, "%EOnly one of the phase keywords DEG or RAD, may be used in a Laplace Table source."
10847, "%EMismatched parentheses.\nMissing '%c' in table source."
10848, "%ENumber of turns must be >=1.0"
10849, "%EMissing Data in Table Source."
10850, "%ECan't mix R_I with other keywords."
10851, "%WFraction must be in the range of 0.01 to 0.5"
10852, "%EMissing I/O model statement '%s'."
10853, "%EVoltage source loop found."
10854, "%EMissing voltage source in W Switch."
10855, "%ENo connections on O Device analog node '%s'."
10856, "%ENode %s has no DC path to ground."
10857, "%EMismatched parentheses.\nExtra '%c' in table source."
10858, "%EThe Modella model must use a PNP4 or PNP4T definition."
10859, "%EIllegal transmission line model parameters. Format is '<Z0=value> <[TD=val2] | [F=freq[NL=nlen]]>'."
10860, "%EHidden node %s is missing."
10861, "%WNode %s has no DC path to ground.\nResistor added."
10862, "%WNodes %s have no DC path to ground.\nResistors added."
10863, "%ENodes %s have no DC path to ground."
10864, "%EEither SAMPLE EXPR or PERIOD must be specified."
10865, "%ECan't find an inductor across switch input nodes."
10866, "%WPart and node have the same name."
10867, "%EIllegal transmission line model parameters. NL and TL must  not be zero if TD is not defined."
10869, "%WThe Temp parameter in the device attributes is not available.\nUse the T_ABS parameter within the model statement instead."
10870, "%ECan't use variables that change during an analysis (like time or V(10)) in a Laplace source."
10871, "%EBoth numbers in an asymmetric tolerance must have a percent sign. e.g. -20%%,+80%%"
10872, "%EFirst number in an asymmetric tolerance must have be negative. e.g. -20%%,+80%%"
10873, "%ESecond number in an asymmetric tolerance must be positive. e.g. -20%%,+80%%"
10874, "%ENegative tolerances can only be used in asymmetric tolerances. e.g. -20%%,+80%%"
10875, "%EThe Chosen interpolation method is invalid."
10887, "%ECircuit contains a component which has a NULL definition."
10888, "%EThis component is not available in the demo version."
10889, "%EIllegal use of reserved variable or symbol, '%s'."
10891, "%EThe system clock is probably incorrect. Please check it."
10892, "%ETD must be greater than 1e-16."
10893, "%EMissing value for 'CLOCK FREQUENCY'."
10894, "%EMissing value for 'INPUTEXPR'."
10895, "%ECan't have a .if <VarExpr> in a library file referenced by Micro-Cap.  A .if <Const> is valid."
10896, "%EDuplicate definition."
10897, "%EIllegal character in label '%s'."
10898, "%EDuplicate definition of parts."
10899, "%EIllegal character in label '%s'.\nDo you want to rename parts?"
10900, "%EIllegal character in label '%s'."
10901, "%EMissing model statement '%s' L=%g W=%g. Found Similar Matches."
10902, "%EMicro-Cap does not support CHEBYSHEV."
10903, "%ECan't find subckt %s."
10904, "%ENode %s from subckt %s does not match any defined pin name for this part."
10905, "%EUnknown command."
10906, "%WDuplicate definition of parts.\n%s"
10907, "%EToo many .includes."
10908, "%EMissing nodes."
10909, "%EToo many nodes passed to subckt '%s'."
10910, "%EUnknown component %s."
10911, "%WCan't use DISTO in print/plot statement."
10912, "%E%s can't be connected to an analog device."
10913, "%EIllegal number of gates."
10914, "%EIllegal pin count."
10915, "%EMissing PWR node in part."
10917, "%EIllegal analysis type %s."
10918, "%EMissing .ENDS for .SUBCKT %s."
10919, "%EToo few nodes passed to subckt '%s'."
10920, "%EMissing GND node in part."
10922, "%EIllegal number '%s'."
10923, "%ECan't use 0 for a digital node name."
10924, "%ENode not defined."
10925, "%EExpecting a digital state but found '%s'."
10926, "%EInductor not defined."
10927, "%EExpecting a value but found '%s'."
10928, "%ELabel name too long '%s'."
10929, "%EDuplicate definition for %s %s."
10930, "%ENot a SUBCKT param %s."
10931, "%E.Ends statement Found outside of a .Subckt."
10932, "%E%s device has an analog node where a digital node was expected.\nNode: %s"
10933, "%E%s device has a digital node where an analog node was expected.\nNode: %s"
10934, "%EMissing values in an .Array statement. Syntax is .ARRAY NAME v1,...vn . Ex. .ARRAY RCAR 1K,2K,3K"
10935, "%EMissing array name in an .Array statement. Syntax is .ARRAY NAME v1,...vn . Ex. .ARRAY CVAL .01u,.1u"
10936, "%EThe NAME in a %s statement is already used in another statement."
10937, "%EFound unexpected '%s' within the Array element."
10938, "%EMissing a '}' after '%s' within the Array element"
10939, "%EExpecting a '{' before '%s' within the Array element."
10940, "%EExpecting a ',' before '%s' within the Array element."
10941, "%EExpecting a ')' before '%s'\nThe dimension list for an array must be in the form (n1,n2,n3) where n are integers."
10942, "%ECan't have more than one .TR statement."
10943, "%EMissing values."
10944, "%ETime values must be in increasing order."
10945, "%EMaximum time step values must be > 0."
10946, "%ETime values must be >= 0."
10947, "%EIncorrect .Path format. The keyword DATA, LIB or DOC should follow .Path."
10950, "%EIllegal character in .Watch %c."
10953, "%ECan't ground pin %s."
10956, "%EMissing $ENCRIPTED_END for $ENCRIPTED_START."
10960, "%EThe user path name '%s' does not exist."
10961, "%EThe user path name is a reserved name. It must be fixed before you can exit the dialog box.\nDo you want the name to be fixed automatically?"
10962, "%EThe specified user path name already exists. It must be fixed before you can exit the dialog box.\nDo you want the name to be fixed automatically?"
10963, "%EThe user path name contains an illegal character. It must be fixed before you can exit the dialog box.\nDo you want the name to be fixed automatically?"
10964, "%EFile name to big to create .inx"
10968, "%WUsing the Leave or Retrace option disables threads and may produce slower run times."
10970, "%WModel attribute is ignored when a time-varying expression is used for RESISTANCE."
10971, "%WModel attribute is ignored when a time-varying expression is used for INDUCTANCE or FLUX."
10972, "%WModel attribute is ignored when a time-varying expression is used for CAPACITANCE or CHARGE."
10974, "%ECan't have more than one .RELTOL statement."
10980, "%EThe operating system was unable to create a thread."
11021, "%EExtra text '%s' found in a .Measure statement."
11022, "%EA Param measure can not use the From or To keywords."
11023, "%EThe .Measure '%s' is recursive."
11024, "%EThe .Measure statement does not have a function assigned."
11025, "%EThe .Measure statement can only have one '%s' for a TRIG or a TARG keyword."
11026, "%EA .Measure can only have a single CROSS, RISE, FALL, or AT keyword for a TRIG or TARG measure function."
11027, "%ECan only have one '%s' in a .Measure statement."
11028, "%EMissing '%s' for '%s' in the .Measure statement."
11029, "%EA .Measure using a FIND/WHEN function can only have a single CROSS, RISE, FALL, or AT keyword."
11030, "%EA .Measure using a FIND/WHEN function can only have a single CROSS, RISE, FALL, or AT keyword."
11031, "%ECan't have '%s' with an AT."
11032, "%EThe .Measure statement can only have one '%s' for a FIND/WHEN function."
11033, "%EThe .Measure statement can not have a FIND with a DERIVATIVE function."
11034, "%EThe .Measure statement can not have a FIND after a WHEN."
11035, "%ECould not find a value."
11036, "%EOnly .Measure statements are allowed in a .BEGIN_MEASURE / .END_MEASURE block."
11037, "%EThe .BEGIN_MEASURE is missing the corresponding .END_MEASURE."
11038, "%EThe name specified in the .BEGIN_MEASURE line must be present in the block."
11039, "%EThe .END_MEASURE is missing the corresponding .BEGIN_MEASURE."
11040, "%EDid not find any .Measure in the Measure Block that match this analysis."
11100, "Lets you specify one or more default paths (folders) for DATA (circuits, output), LIBRARY (model libraries), and PICTURE (graphic picture files).\nPath"
11101, "This text field sets the default path for circuit files, numeric output, text files, probe files, Monte Carlo files, filter impedance files, User Source files, digital stimulus files, PLA files, sensitivity output files, PCB netlists, and Bill of Materials netlists."
11102, "This text field sets the default path for where the library files or macro files will be stored.  When entering an analysis, if Micro-Cap can't find a model in the local circuit, it will use this path to find the Nom.lib file or any files referenced in a .lib or .inc that are not specified with a path.  It will also search this path for any macro files used within the circuit.  Multiple paths must be separated with a semicolon."
11103, "This text field sets the default path where any picture files will be stored.  When a picture file is created through Micro-Cap or inserted into a schematic, this is the default path it will use."
11104, "This text field sets the default path for documentation files.  This path will be used when accessing the Micro-Cap manuals via the Help menu.  It also sets the default path for documents that have been defined for a component in the Link field of the Component Editor."
11105, "Lets you browse for the data path"
11106, "Lets you browse for the model library path"
11107, "Lets you browse for the graphics path"
11108, "Lets you browse for the document path"
11109, "The preferred paths section lets you store and manipulate paths so that it is easy to change between two different sets of paths."
11110, "This command adds a new preferred path using the paths that are currently defined."
11111, "This command updates the selected preferred path name with the paths currently defined."
11112, "This command deletes the selected preferred path."
11113, "The initial path in the Open File dialog box will be set to the path defined in the appropriate path field in the upper part of this dialog box.  If multiple paths are listed in the field, the first path will be chosen."
11114, "The initial path in the Open File dialog box will be set to the last path from which a similar file was opened.  Data file, library file, and graphic file types will all have their own last path stored."
11115, "The initial path in the Open File dialog box will be set to the same path as the current active file open in Micro-Cap."
11116, "This field lists the defined variable names that can be used where path names are required. For example, User sources, PWL file names."
11117, "This invokes the User Path dialog box which lets you define new path names and associated paths."
11118, "This lets you edit selected user paths."
11119, "This lets you delete selected user paths."
11120, "When enabled, the search operation also looks in any subdirectories that the paths in any of the Path fields may have"
11121, "This lets you specify paths which do not exist at the time of creation, but may later. For example, USB or CD drives."
11122, "This places .Path command statements into the currently active circuit which will localize the path information for that circuit.  The .Path dialog box that is invoked from this button lets you select which paths are to be localized."
11151, "%EMissing value for '%s'."
11152, "%EBad '%s'."
11153, "%EParameter count mismatch or .parameters statement not found."
11154, "%EBad parameters '%s'."
11155, "%EMultiple .Parameters statements have been found in the macro."
11156, "%WPurely numeric grid text or pin names have been used and might be confused with node numbers."
11157, "%EPin '%s' not defined."
11158, "%ERecursive macro found '%s'."
11159, "%WFile %s has been edited and must be saved before generating an Index file.\nDo you want to save the file ?"
11170, "%EExpecting '(' to follow '%s'."
11171, "%EStatement too complex."
11172, "%EMissing identifier in %s."
11173, "%EParameter count mismatch."
11174, "%EDuplicate statement '%s'."
11175, "%EIllegal character in %s identifier"
11176, "%EMissing LOT keyword in .define statement."
11177, "%EUse of LOT='%%' with a define statement requires that the expression be constant during the run."
11178, "%EIllegal identifier in %s statement."
11179, "%EThe LOT keyword is not available for use with a define with parameters."
11180, "%EMissing '}' in %s."
11181, "%EStatement is Recursive."
11182, "%EMismatched parentheses in %s %s"
11183, "%EMismatched braces in %s %s"
11200, "File"
11201, "Edit"
11202, "Component"
11203, "Windows"
11204, "Options"
11205, "Analysis"
11206, "Box"
11207, "Mode"
11208, "View"
11209, "Scope"
11210, "Cursor"
11211, "Design"
11213, "Help"
11220, "Component name not found."
11230, "%EPlease select the name of the loop gain probe."
11231, "%ECan't find the specified loop gain probe."
11232, "%ECircuit must have a Loop Gain Probe component."
11350, "%EAn unexpected .ELSE has been found."
11351, "%EAn unexpected .ELIF has been found."
11352, "%EAn unexpected .ENDIF has been found."
11353, "%EA .ENDIF statement is missing for a .IF condition."
11354, "%EToo many nested .IF statements are present."
11400, "Creates a new schematic, SPICE, model library, or document file.\nNew"
11401, "Schematic File (.cir)"
11402, "Macro File (.mac)"
11403, "General Text File (.txt)"
11404, "SPICE File (.ckt)"
11405, "Text Library File (.lib)"
11406, "Binary Library File (.lbr)"
11407, "Model File (.mdl)"
11408, "Script File (.bat)"
11409, "Worst Case Tolerance Library (*.tlib)"
11410, "Derating Library (*.dlib)"
11542, "Numeric format for the Nominal Value"
11544, "Numeric format for the Tolerances"
11546, "Numeric format for the Parameters"
11548, "Numeric format for the Variances"
11550, "Numeric format for the Sensitivity"
11552, "Numeric format for the (%%)"
11554, "Numeric format for the Outputs"
11556, "Numeric format for the Percent Outputs"
11851, "%EError in Pulse source. The requirement that P5>=P4>=P3>=P2>=P1 is violated."
11852, "%EIllegal use of '%s'."
11854, "%EOnly one of the temperature parameters T_REL_GLOBAL, T_REL_LOCAL or T_ABS may be defined in a model."
11855, "%EIllegal model type '%s'."
11856, "%EIn GaAsFET model, VMAX must be less than VBI."
11857, "%ERecursive AKO in Model statement %s."
11858, "%ECan't find AKO Model %s."
11859, "%EMust specify model name and type."
11861, "%EBad value '%s' for '%s'."
11863, "%E<%s #> must be in range of 0 to 99."
11864, "%EThe VON and VOFF parameters for the S Switch model must be different."
11865, "%EThe ION and IOFF parameters for the W Switch model must be different."
11866, "%WMissing ')'."
11867, "%EIllegal parameter name %s in model."
11891, "%WThe AC signal magnitudes of all sources in this circuit are zero."
11895, "%EMethod must be followed by either GEAR or TRAP."
11896, "%EMissing value for '%s'."
11897, "%EBad value following %s."
11898, "%WIgnoring .options that are in Macro/Subckt."
11900, "%EExpecting '%s'."
11901, "%EExpecting '%s' to follow '%s'."
11902, "%EExpecting '%s' but found '%s'."
11903, "%EExtra text '%.200s' found."
11904, "%WExtra text '%.200s' found."
11905, "%EUnknown command found '%s' in stim."
12001, "%ECan't read from import file while it is being written to."
12003, "%EIllegal import expression."
12005, "%EImport must have T or F in Transient."
12007, "%EMissing '('."
12008, "%ECan't open import input file '%s'."
12009, "%ECouldn't find import waveform '%s' vs. '%s' or bad data in file '%s'."
12010, "%ECouldn't find %s in import waveform '%s'\nin file '%s'."
12011, "%EMissing data for column %s in import waveform '%s'\nin file '%s'."
12012, "%ECouldn't find %s in import waveform '%s'\nin file '%s'\nimport file had extra values '%s'."
12013, "%EThat name is not in the Waveform Buffer list."
12101, "Name of currently selected shape."
12104, "List of all shapes contained in the Shape library."
12105, "Scrolls the drawing area vertically."
12106, "Scrolls the drawing area horizontally."
12107, "Drawing area for creating or editing a shape."
12110, "Snaps objects placed in drawing area to the grid points.\nGrid Snap"
12111, "Close Shape Editor."
12113, "Adds a new shape.\nAdd Shape"
12114, "Deletes the current shape or group."
12115, "Invokes the Object Editor."
12116, "Reverts to the saved shape."
12118, "Creates a new file and adds it to the Shape library.\nNew File"
12119, "Adds an existing file to the Shape library.\nOpen File"
12120, "Removes selected file from the Shape library.\nRemove File"
12121, "Saves Shape library as a new name.\nSave File As"
12122, "Translates the selected shape file to an older Micro-Cap shape format.\nTranslate"
12123, "Add a new shape group\nAdd Group"
12124, "Searches for a specified shape name.\nFind"
12125, "Creates a duplicate of the selected shape and assigns it a generic name."
12126, "Saves Shape library file.\nSave"
12127, "Reverts to the disk version\nRevert"
12130, "Flips the selected objects about the X-axis.\nFlip X"
12131, "Flips the selected objects about the Y-axis.\nFlip Y"
12132, "Creates a mirror image of the selected schematic region.\nMirror"
12133, "Rotates the selected schematic region.\nRotate"
12151, "Pastes the selected object stored in the Clipboard List.\nPaste from Clipboard List"
12174, "Allows editing the Clipboard List. The Clipboard List is a secondary clipboard that can hold images, analysis limits, text \nEdit Clipboard List"
12189, "Copies an Images to the Clipboard List\nCopies an Image To Clipboard List"
12190, "Left-aligns one or more selected pieces of attribute or grid text. Must select one piece as the anchor (CTRL+click).\nAlign Left"
12191, "Center equalizes the X coordinate of all selected objects.\nAlign Center"
12192, "Right-aligns one or more selected pieces of attribute or grid text. Must select one piece as the anchor (CTRL+click).\nAlign Right"
12193, "Top-aligns one or more selected pieces of attribute or grid text. Must select one piece as the anchor (CTRL+click).\nAlign Top"
12194, "Middle equalizes the Y coordinate of all selected objects.\nAlign Middle"
12195, "Bottom-aligns one or more selected pieces of attribute or grid text. Must select one piece as the anchor (CTRL+click).\nAlign Bottom"
12196, "Sets the align commands to affect only grid text and attribute text of selected parts. If un-checked the commands affect all selected objects.\nAlign Attribute Text"
12197, "Copy formula to clipboard"
12199, "Allows you localize (save in a text page) a file.\nLocalize a File"
12200, "Adds a new schematic page to the schematic.\nAdd schematic Page"
12201, "Adds a new text page to the schematic.\nAdd Text Page"
12203, "Adds or modifies tolerances for models within the circuit.\nTolerances"
12204, "Pastes the image stored in the clipboard.\nPaste Image"
12205, "Copies items to the Clipboard List\nCopy To Clipboard List"
12207, "Deletes a range of pages from the active schematic.\nDelete Page"
12211, "Adds a new macro section into the circuit file.\nAdd Macro Section"
12214, "List of objects contained in the shape."
12226, "Deletes current object."
12228, "X coordinate of object."
12229, "Y coordinate of object."
12252, "Delete Point"
12253, "Add Point"
12270, "&Group"
12271, "&File"
12272, "&Name"
12273, "Assign Component Name to %s."
12274, "Display %s Attribute."
12275, "Display Macro Parameter Names and Values."
12289, "Opens the Component Editor.\nComponent Editor"
12291, "Name of component."
12292, "Shape of component. Click on the arrow for a list of shapes."
12293, "Definition of component. Click on the arrow for a list of definitions."
12294, "Number of Components in Library."
12296, "Pin configuration of component."
12298, "Pin configuration of component."
12299, "Hierarchical display of Component library."
12300, "Integrates all the steps required to add a new part to the libraries.\nAdd Part Wizard"
12301, "Adds a Part to the current group.\nAdd Part"
12302, "Adds a group to the list.\nAdd Group"
12303, "Deletes a component or group.\nDelete"
12304, "Merges the currently displayed library with one selected from the disk.\nMerge"
12305, "User palette number the component appears on (if any)."
12307, "Copies the Name field to the %s attribute when the part is placed in a schematic."
12308, "Displays the PART name when the component is placed in a schematic."
12309, "Displays the %s name when the component is placed in a schematic."
12310, "Displays the MODEL name when the component is placed in a schematic."
12313, "Removes selected file from the Component library.\nRemove File"
12314, "Copies the current component to the clipboard for a subsequent paste or replace operation.\nCopy"
12315, "Adds a new component and copies all fields except Name from a template previously copied to the clipboard.\nPaste"
12327, "The memo field is used for documentation only."
12329, "Enables the display flag for all macro parameter names and values when the part is initially placed in a schematic."
12331, "If enabled, this flag tells Micro-Cap to display pin text when the part is initially placed in a schematic."
12332, "Sets the Display Pin Numbers flag to On."
12333, "Zoom-out on text placement and pin placement windows.\nZoom Out"
12334, "Zoom-in on text placement and pin placement windows.\nZoom In"
12335, "Sets the cost and power fields for multiple components at one time.\nSet Cost and Power"
12338, "Saves Component library file.\nSave"
12339, "Reverts to the disk version\nRevert"
12340, "Adds an existing file to the Component library.\nOpen"
12341, "Creates a new file in the Component library.\nNew"
12342, "Clears all components from the Component palettes.\nClear Palettes"
12344, "The default cost used in the Bill of Materials report."
12346, "The default power used in the Bill of Materials report."
12347, "Imports subckts from a SPICE model file by matching existing parts with similar pin names.\nImport Wizard"
12348, "Creates a copy of the component library in a previous Micro-Cap format.\nTranslate"
12349, "Displays the subckt, macro, or model statement for the part.\nInfo"
12350, "Saves Component library as a new name.\nSave File As"
12351, "Replaces all fields except Name with a template previously copied to the clipboard.\nReplace with template"
12352, "Undoes the last action.\nUndo"
12353, "Reverses the previous Undo command.\nRedo"
12354, "Sorts the part names.\nSort"
12355, "Creates a part list.\nParts List"
12356, "Pins: Click to add pins for subckts, macros, logic expressions, pin delays, and constraints."
12357, "Text positioning: Click and drag in window to move text."
12358, "Text positioning: Click and drag in window to move text."
12360, "Assigns a file link to component.  The link can be either a URL or a local path."
12363, "Sets the type of subcircuit model used.  It should be set to Standard for all models besides ones using IBIS files."
12370, "This option sets the display flag for the %s attribute.  The %s attribute is the name of the model statement that characterizes the electrical behavior of the part."
12371, "This option sets the display flag for the %s attribute."
12373, "This option sets the display flag for all macro parameter names and values."
12374, "Moves one or more parts from the current group to another group.\nMove Parts"
12380, "Tests the assigned file link from the Link field."
12411, "This command finds a specified component type.\nFind Component"
12450, "Click on a name to select the page. Double-click to edit the name."
12454, "Click on a name to select the section. Double-click to edit the name."
12460, "Controls which model type to display."
12461, "Displays all model names of the selected type from the current library."
12462, "Tells you something about the displayed part."
12463, "Shows the model name of the displayed part."
12465, "Adds a new model name to the current file."
12466, "Deletes the displayed model name from the current file."
12467, "Merges a library file from disk with the current library file."
12468, "Copies a model name from the current library to another(or the same) library."
12469, "Places parts in alphanumeric order and removes duplicates."
12470, "Finds a specified parameter name."
12501, "%ECircuit wire can't be coincident with a macro box boundary."
12502, "%WYou are attempting to create a macro by the name of '%s',\nand there is already a component of that name in the library.\nDo you want to overwrite it?"
12503, "%WYou are attempting to create a SUBCKT by the name of '%s',\nand there is already a component of that name in the library.\nDo you want to overwrite it?"
12504, "%EYou are attempting to create a macro by the name of '%s',\nand that name is in use in an open circuit."
12505, "%ESelect Box to Small."
12506, "Replaces the active window file with the disk version of it.\nRevert"
12507, "%EYou are attempting to create a SUBCKT by the name of '%s',\nand that name is in use in an open circuit."
12508, "Accesses the Backup and Restore dialog box where you can create backups or restore from a backup.\nBackup And Restore"
12513, "Exit Micro-Cap."
12516, "%EMacro file name can't be same as source file name."
12517, "%EMacro file's extension must be CIR or MAC."
12530, "%EThere is already a file with this name in memory that is in a different format."
12531, "%EThe user supplied Numeric Output file name '%s' is illegal."
12611, "When enabled, this option places the component name into the %s attribute when the component is placed in a schematic. This option disables the Attribute dialog box because the electrical characteristics for the part have already been defined."
12613, "Component Wizard"
12614, "Enter the name of the file containing the subckt."
12615, "Enter the name of the file containing the model statement."
12616, "Enter the name of the macro file"
12617, "%EMust have a name."
12626, "%EName '%s' not found in library '%s'."
12640, "$NAME\tThis prints the circuit name."
12641, "$NAMEEXT\tThis prints the circuit name with its extension."
12642, "$MC\tThis prints the version of Micro-Cap."
12643, "$DATE\tThis prints the current date."
12644, "$TIME\tThis prints the current time."
12645, "$USER\tThis prints the user's name."
12646, "$COMPANY\tThis prints the user's company."
12647, "$PAGE\tThis prints the page number."
12648, "$PAGENAME\tThis prints the name of the page."
12649, "$MAXPAGE\tThis prints the largest page number."
12650, "$SECTION\tThis prints the section number."
12651, "$SECTIONNAME\tThis prints the name of the section."
12652, "$MAXSECTION\tThis prints the largest section number."
12653, "$SHEET\tThis prints the  sheet number."
12654, "$MAXSHEET\tThis prints the largest sheet number."
12655, "$ANALYSIS\tThis prints the analysis type."
12656, "$DATESAVED\tThis prints the date that the file was last saved."
12657, "$TIMESAVED\tThis prints the time that the file was last saved."
12658, "$PATH\tThis prints the path of the file."
12801, "Enables a single title block per schematic page."
12809, "List of keywords that can be used."
12810, "Selects the title block to place in the schematic."
12812, "Sets the values that will be placed in for each parameter string."
12813, "Selects where the title block will be placed on the schematic page."
12814, "Keeps the aspect ratio of the title block when it is being resized."
12815, "Reverts the title block to its original size."
12913, "Localizes / refreshes model data by copying it from the libraries to the circuit text area.\nLocalizes model data by copying it to the circuit text area."
12985, "Enables display of devices without a SMOKE attribute."
13017, "Component Import"
13018, "%EMust provide a file name."
13090, "%WThis will clear all palettes. Are you sure you want to continue?"
13181, "%EStimulus pin count does not match format statement."
13182, "%EEmpty loop."
13183, "%ENo Label."
13184, "%EUNTIL must be followed by GT,GE,LT or LE."
13185, "%EExpecting GOTO, INCR, DECR or a value to follow time value."
13186, "%EIllegal Goto statement."
13190, "%EIllegal digit <format array>."
13191, "%EToo many labels."
13192, "%EInvalid value '%s'."
13193, "%EWidth too large."
13194, "%ETime must be in ascending order."
13195, "%EREPEAT nesting too deep."
13196, "%EExpecting <n> TIMES or FOREVER to follow REPEAT."
13197, "%EIllegal repeat statement."
13198, "%EENDREPEAT without a matching REPEAT."
13199, "%EREPEAT without a matching ENDREPEAT."
13200, "%EMissing <format array>."
13201, "%EMissing 'BY'."
13202, "%EMissing <time>."
13203, "%EMissing <label name>."
13204, "%EMissing 'TIMES'."
13206, "%ELABEL not allowed in REPEAT."
13207, "%ETIMESTEP must be > 0."
13221, "%EMust specify LOGIC:."
13222, "%ECan't assign value to input '%s'."
13223, "%ECan't assign expression to '%s'."
13225, "%EExpecting '%s' but found '%s' after value '%s'."
13226, "%EIllegal variable '%s'."
13227, "%EUnknown format '%s' in Constraint."
13228, "%EMust specify Enable HI|LO for TRISTATE:."
13229, "%EMust specify BOOLEAN:, PINDLY:, TRISTATE:, SETUP_HOLD:, WIDTH:, FREQ:, or GENERAL:"
13230, "%EMust specify BOOLEAN:, SETUP_HOLD:, WIDTH:, FREQ:, or GENERAL:"
13231, "%ENode '%s' must be an input node."
13232, "%EIllegal range '%s' value for DATA()."
13233, "%ECan't assign '%s' to ENABLE."
13234, "%ERadix flag must be 'B','O', or 'X'."
13235, "%EIllegal value '%c' in program data."
13236, "%EHave not defined number of fuses."
13237, "%EIllegal default fuse state field."
13238, "%EMissing fuse address."
13239, "%EOnly one QF allowed."
13240, "%EToo many fuses."
13241, "%EAddress %d has not been defined.\nEither define with K or L, or default with F."
13242, "%ENo data."
13243, "%EIllegal <temporary value> in LOGICEXP."
13244, "%EIllegal <enable node> in TRISTATE."
13245, "%EIllegal <output node> in PINDLY."
13246, "%EIllegal <node> in CONSTRAINT."
13247, "%EIllegal <input node> following DATA in CONSTRAINT."
13248, "%EIllegal <Boolean variable>."
13249, "%EIllegal address %d."
13250, "%EPLA file has too much data."
13252, "%EMissing %s signal name."
13253, "%ETIMESCALE must appear on separate line."
13254, "%ENumber of signal names not equal to number of values %s."
13255, "%ENode %s not found in STIM file %s."
13256, "%EToo many signals in header, exceeded %d max."
13257, "%EExpecting '=' to follow 'TIMESCALE'."
13258, "Either the required blank line separating the header from the data is missing and or the data itself is missing."
13260, "%W%d digital warning message%s.\nSee Numeric Output window."
13271, "%ECan't find a model named '%s'."
13274, "%ECan't step parameter."
13275, "%ECan't find a model parameter named '%s'."
13276, "%EMissing a model parameter."
13277, "%ECan't find a component named '%s'."
13278, "%ECan't find the parameter '%s' for component '%s'."
13279, "%EMore than %d cases in stepping settings."
13281, "%EIllegal Step value."
13282, "%EIllegal From value."
13283, "%EIllegal To value."
13284, "%ECan't step '%s' more than once."
13285, "%ECan't find a define named '%s'."
13286, "%EWhen using simultaneous stepping all cases must have the same number of steps."
13287, "%EMissing list values."
13290, "&List"
13291, "Next"
13298, "%EThe Demo could not start.\nThe Mouse or Keyboard hook was not installed"
13299, "%EThe System is out of timers try closing all open programs before running the demo."
13306, "%EMenu can't be right aligned when running demo."
13370, "Circuit"
13371, "Analog       Total   Rejected       Total       Run     Setup      Load     Solve   Device     DoIO    Trunc    Break"
13372, " Nodes  Iterations  Solutions   Solutions      Time      Time      Time      Time     Time     Time     Time     Time\n"
13373, "Total run time                 %s\n"
13374, "Total elapsed time             %s\n"
13375, "Total setup time               %s\n"
13376, "Total load time                %s\n"
13377, "Total solve time               %s\n"
13378, "Total Update Device time       %s\n"
13379, "Total DoIO time                %s\n"
13380, "Total Truncate time            %s\n"
13381, "%EShape name already used."
13383, "Delete current shape?"
13384, "%E%s has already been used. Please enter new name."
13385, "%ECan't Delete a shape that is being used as a root shape."
13386, "Remove '%s' shape file from the list?\n\nThe shapes within the file will no longer be available to use in the schematic."
13387, "Specifies no lead at the pin for the Block shape."
13388, "Specifies a clock lead at the pin for the Block shape."
13389, "Specifies an inverted lead at the pin for the Block shape."
13390, "Specifies an inverted clock lead at the pin for the Block shape."
13391, "Specifies a standard lead at the pin for the Block shape."
13392, "%WThis group contains shapes that are used as roots.\nYou must delete any shapes that use these roots first."
13394, "%WThis group contains shapes that will be lost if the group is deleted.\nDo you still want to delete the group?"
13395, "Total Add Breakpoints time     %s\n"
13398, "%WTemperature TC1 coefficient is outside the normal range."
13399, "%WTemperature TC2 coefficient is outside the normal range."
13503, "%WMicro-Cap may assign nodes differently than MC4.\nCheck the X and Y expressions in the analysis limits."
13505, "%EAttempted to load an MC4 macro circuit which has not yet been saved in Micro-Cap format. Load the macro circuit with Micro-Cap and save it."
13506, "%EEncrypted File is Corrupt."
13507, "%WComponent has no shape linked to it."
13508, "%WThe file %s on the disk has been changed.\nDo you want to overwrite it with your changes ?"
13509, "Incorrect password. Access denied."
13510, "%EThat file name is already in use.\n%s."
13511, "Revert to the disk version ?"
13512, "%WFile '%s' has been saved in MC%d format.\nIt may have lost critical data."
13513, "%WExtra or unknown data was found.\nfile %s\n\n%s."
13514, "%ECannot rename a section with the same name as another section."
13515, "%ECannot rename a page with the same name as another page in its section."
13516, "%WThe file %s has been modified outside of Micro-Cap.\nDo you want to reload it?"
13517, "%WThe file %s has been modified outside of Micro-Cap.\nDo you want to reload it and lose changes made in Micro-Cap?"
13518, "%W%s already exists.\nDo you want to replace it?"
13519, "%ETried reading past the end of the file '%s'."
13520, "%EThe data within the Probe/Retrieve file does not match the format expected '%s'."
13530, "%ESource not found."
13535, "%EOutput Start Time must be less than the Maximum Run Time."
13536, "%EMaximum Run Time must be greater than zero."
13537, "%EOutput Start Time must be greater than or equal to zero."
13541, "%EIllegal temperature."
13542, "%EInternal time step too small in transient analysis."
13544, "%WThis run will require %g periods of at least one pulse source!\nPlease check the time range.\nDo you wish to continue?"
13546, "%WThe time range and maximum time step specified will require more than 10,000,000 time steps.\nDo you wish to continue?"
13547, "%ECan't find expression in %s."
13548, "%WFound %d data points out of %d."
13549, "%WFile must be converted to use. Do you wish to convert it?"
13550, "%WThe source %s contains duplicate X values within its table data."
13551, "%WThe User Source does not have a time dependent waveform.  The transient value will be set to 0V."
13552, "%WWith the time range specified, this circuit's STIM will require more than 1,000,000 time steps.\nDo you wish to continue?"
13553, "%EMust have at least one Schematic Page and one Text Page per Section."
13554, "%WWith the time range specified, this circuit's PWL will require more than 1,000,000 time steps.\nDo you wish to continue?"
13555, "%WPage '%s' is not empty.\nDeleting will delete all elements in the page.\nDelete anyhow?"
13556, "Save changes in '%s'?"
13557, "%EPaste region is outside drawing area."
13558, "%WSection '%s' is not empty.\nDeleting will delete all elements and pages in the Section.\nDelete anyhow?"
13561, "%EIllegal node name."
13570, "%ECoordinates out of range."
13572, "%EWhen a model parameter uses the TEMP temperature variable, you can't use a variable in the Temperature field."
13575, "%ECan't plot noise with other expressions."
13577, "%EThe high limit and low limit must be non-zero when using log stepping."
13578, "%EThe high limit must be < 1e30.  The high must be greater than the low."
13579, "%EThe Frequency Range step method must be set to Linear or List when the range is <=0."
13580, "%EThe High and Low values in the Noise Frequency Range must be greater than 0."
13581, "%ECan't open a Fourier, Performance, 3D, or Monte Carlo window when the Temperature field uses a time-varying variable."
13582, "%EMissing ')'."
13583, "%EFormat error."
13584, "%EUnknown model parameter."
13585, "%EIn log stepping, from and to must have the same sign."
13586, "%EIn log stepping, step can not be 0.0 or 1.0 and must be positive."
13587, "%EIn log stepping, from or to can not be 0.0."
13588, "%EThe Temperature value is too small.  It must be greater than -273.15C."
13589, "One or more branches failed to run. Check Numeric Output window for errors."
13590, "Check Numeric Output window for warnings."
13592, "Left Cursor"
13593, "Right Cursor"
13594, "F"
13595, "G"
13596, "Gamma"
13597, "Z"
13598, "Complex"
13599, "Mag Ang"
13612, "Left"
13613, "Right"
13614, "Delta"
13615, "Slope"
13616, "%EError Illegal state."
13619, "%WAre you sure you want to remove this file.\n%s"
13620, "%EFor an IBIS subcircuit, the number of pins and names of the pins must match the following for each type:\n\nInput: In\nInput with Supplies: In,Vcc,Vee\nOutput: In,En,Out\nOutput with Supplies: In,En,Vcc,Vee,Out."
13621, "%EComponent name already used."
13622, "%ECan't delete a component that is used in an open circuit."
13623, "%WThis group contains components.  Do you still want to delete the group?"
13624, "%EA STIM must have at least 1 node and no more than 32."
13625, "%WThe pin names of this component may not be changed."
13627, "%EIllegal input node."
13628, "%EIllegal output node quantity."
13629, "%WThe file '%s' uses an older file format.\nIt must be saved with a different file name before continuing.\nMicro-Cap will use the newly saved file."
13630, "%EFor bandpass filters, PB must be less than SB."
13631, "%EThese specifications require a filter of order %d.\nThe filter order must be between 2 and %d."
13632, "%EFilters using the Bessel function are limited to order 10."
13633, "%EIn a low pass filter the stopband frequency (Fs)\nmust be greater than the passband frequency (Fc)."
13634, "%EIn a high pass filter the passband frequency (Fc) \nmust be greater than the stopband frequency (Fs)."
13635, "%EFor bandpass filters, PB/2 must be less than Fc."
13636, "%ELow-pass and high-pass KHN filters must have a gain >= -5 dB."
13637, "%EHigh-pass Sallen-Key filters must have a gain >= 0 db."
13638, "%EThe gain is too high in this filter."
13639, "%EFor notch filters, PB/2 must be less than Fc."
13640, "%EKHN, Acker-Mossberg, and Tow-Thomas notch filters are limited to order 20 or lower."
13641, "%EThe gain is too low in this filter."
13642, "%ESallen-Key bandpass filters of this order are limited to gains<=70db."
13643, "%EOne stage of this filter has an illegal Q of %g. The Q must be greater than 0.4."
13644, "%EThe passband frequency (PB) and the stopband frequency (SB)\nmust be less than the center frequency (FC)."
13645, "%EFor notch filters, the passband frequency (PB)\nmust be greater than the stopband frequency (SB)."
13646, "%EThe Q/gain choices produce negative resistances. Raise the Q or lower the gain."
13647, "%EThe order for this filter is too high."
13648, "%EThe choice of a Sallen-Key or MFB circuit and a negative passband gain requires\na capacitance of less than %g, which is too low.  Try raising the gain or changing the circuit."
13650, "%EPassive Chebyshev filters are limited to odd orders."
13651, "%EThe file %s is missing.\nPlease restore it before using the filter routines."
13652, "%EThe macro name you've chosen is already being used by another part. Please choose a new name."
13653, "%EThe macro name you've chosen belongs to a macro with a pin count other than 2. Please choose a new macro name."
13654, "%EThe macro name you've chosen belongs to a macro with the wrong pin labels. Please choose a new macro name."
13655, "%WThe macro file %s already exists.\nDo you want to overwrite it?"
13656, "%ECircuit for macro is same as main circuit."
13657, "%EYou must enter a macro name."
13659, "%EObsolete state variables file."
13660, "This command translates the voltages, currents, and states\nin this editor into %s statements and places them in the\ntext area of the current circuit.\nDo you wish to continue?"
13661, "%ENSUB must be >= NI in MOSFET model."
13662, "%ETOX must be > 0.0 in the MOSFET model."
13680, "%Wk1 should be specified with k2 in model '%s'.\n"
13681, "%Wk2 should be specified with k1 in model '%s'.\n"
13682, "%Wnsub is ignored because k1 or k2 is given in model '%s'.\n"
13683, "%Wxt is ignored because k1 or k2 is given in model '%s'.\n"
13684, "%Wvbx is ignored because k1 or k2 is given in model '%s'.\n"
13685, "%Wvbm is ignored because k1 or k2 is given in model '%s'.\n"
13686, "%Wgamma1 is ignored because k1 or k2 is given in model '%s'.\n"
13687, "%Wgamma2 is ignored because k1 or k2 is given in model '%s'.\n"
13688, "%EFor bandpass filters, SB/2 must be less than Fc."
13689, "%EFor notch filters, SB/2 must be less than Fc."
13690, "Warning %s temperature adjusted PHI (or PB, VJ, VJE, or VJC) went negative at temperature=%f.\n"
13691, "Check model parameter value and or the operating temperature.\n"
13781, "%ECan't use '%s' variable in '%s'."
13782, "Get Function"
13801, "%EMust select an expression to plot."
13802, "%EWaveforms in the same graph must have the same log/linear option."
13803, "%EIllegal range."
13804, "%EWaveforms in same graph must have the same Plot Type."
13807, "%EDifferent X expressions for the same graph."
13810, "%ECan't plot FFT/IFT function for X expr."
13811, "%EX expression must be F or T when Y expression is an FFT/IFT."
13812, "%EX expression must be T when Y expression is an FS or RES"
13813, "%ECan't plot digital function for X expression."
13815, "%ECan't plot digital variables in AC."
13816, "%ECan't plot digital variables in Stability."
13817, "%WIf Y expression uses FFT, FFTS, FS, HARM, HARMN, THD, THDN, or IHD, then the X expression should contain F else it should NOT contain F."
13818, "%WIf Y expression uses an IFT, or IFTS operator then the X expression should contain T."
13850, "Properties for %s"
13860, "%EIllegal Address value (32 is the max)."
13899, "A circuit for %s with the following properties will be built when you return to the schematic:\n%s"
13901, "Percent displayed %6.2f"
13903, "Low"
13904, "Mean"
13905, "High"
13906, "Sigma"
13912, "Grid Spacing"
13913, "Range Low"
13914, "Range High"
13924, "Number of Runs %d"
13926, "Bar Count"
13930, "Font Color"
13931, "Grid Color"
13932, "Bar Front Color"
13933, "Bar Top/Side Color"
13934, "Graph Background Color"
13935, "Window Background Color"
13936, "Select Color"
13937, "Select Box Color"
13938, "Anchor Color"
13951, "Individual run statistics"
13952, "There were no Monte Carlo failures in the numeric output file for this circuit."
13953, "%WNo Monte Carlo 'Report When' cases were found in the file."
13956, " Low=%s Mean=%s High=%s Standard Deviation=%s\n"
13960, "Transient"
13961, "AC"
13962, "DC"
13963, "Harmonic Distortion"
13964, "Intermodulation Distortion"
13965, "Stability"
13966, "Dynamic AC"
13967, "Dynamic DC"
13968, "Transfer Function"
13969, "DC OP Worst Case"
13970, "&Transient"
13971, "&AC"
13972, "&DC"
13973, "&Harmonic Distortion"
13974, "&Intermodulation Distortion"
13975, "Stability"
13980, "Transient Analysis"
13981, "AC Analysis"
13982, "DC Analysis"
13983, "Harmonic Distortion Analysis"
13984, "Intermodulation Distortion Analysis"
13985, "Stability Analysis"
13986, "Dynamic AC"
13987, "Dynamic DC"
13991, "Running Transient Analysis."
13992, "Running AC Analysis."
13993, "Running DC Analysis."
13994, "Running Harmonic Distortion Analysis"
13995, "Running Intermodulation Distortion Analysis"
13996, "Running Stability Analysis"
14000, "%EThe high and low values in the Noise Frequency Range must be non-zero."
14002, "Name of currently selected title block."
14003, "List of all title block contained in the Title Block library."
14004, "Drawing area for creating or editing a Title Block."
14005, "Close Title Block Editor."
14006, "Enables Include Title Block mode. Lets you include another Title Block in the current Title Block.\nInclude Title Block mode"
14007, "Adds a new title block.\nAdd Title Block"
14008, "Deletes the current title block or group."
14009, "Reverts to the saved title block."
14010, "Creates a new file and adds it to the Title Block library.\nNew File"
14011, "Adds an existing file to the Title Block library.\nOpen File"
14012, "Removes selected file from the Title Block library.\nRemove File"
14013, "Saves Title Block library as a new name.\nSave File As"
14014, "Translates the selected title block file to an older Micro-Cap title block format.\nTranslate"
14015, "Add a new title block group\nAdd Group"
14016, "Searches for a specified title block name.\nFind"
14017, "Creates a duplicate of the selected title block and assigns it a generic name."
14018, "Saves Title Block library file.\nSave"
14019, "List of objects contained in the title block."
14051, "%ECan't read the version(%s) of %s."
14061, "%ENo Model Name Given."
14062, "Delete Part %s"
14063, "Quit Micro-Cap?"
14064, "%WIf you change the level parameter you will lose the old model data.\nDo you wish to proceed?"
14070, "%E%s=%g Value must be greater than zero."
14071, "%E%s=%g Value must be greater than or equal to zero."
14072, "%E%s=%g Value must be >=0 and <=1."
14073, "%E%s=%g Value must be >=0 and <=3."
14074, "%E%s=%g Value must be >=1 and <=3."
14075, "%E%s=%s Value must be \"0\",\"1\",\"R\",\"F\",\"X\",\"Z\",\"\"."
14076, "%ELEVEL must be 1......"
14077, "%ELEVEL must be 1,2 or 3"
14078, "%ELEVEL must be ........\nThermal definitions must use a Thermal model."
14079, "%ELEVEL must be .....\nNon-Thermal definitions can not use a Thermal model."
14080, "%ELEVEL must be 1, 2, 21, 500 or 501"
14081, "%ELEVEL must be 21 or 501.\nThermal definitions must use a Thermal model."
14082, "%ELEVEL must be 1, 2 or 500.\nNon-Thermal definitions can not use a Thermal model."
14083, "%ELEVEL must be 1,2"
14084, "%ELEVEL must be 1, 2, 4 or 200."
14085, "%E%s=%g Value must be >=1 and <=4."
14086, "%WNB must be positive. Setting NB to its default value."
14091, "Scale Range Must be in the range of 1 to 600."
14092, "%EUnable to start print job."
14093, "%ENo Printer detected."
14100, "%ESecurity key internal error=%d."
14101, "%EBad data on key."
14102, "This key '%s' was reported lost or was exchanged and not returned from %s.\nPlease contact Spectrum Software for more information."
14103, "HaspCode Illegal return code."
14104, "This key '%s' has expired."
14105, "%EThe number of stations activating the program is larger than authorized."
14106, "%EError in hardware key\nThis might be an older HASP3 key that is no longer accessible and needs to be exchanged.\nContact Spectrum Software."
14107, "Trouble Shooting the Security key..."
14181, "%ERLCG, RL, GL, and GC lossy transmission lines are not supported."
14182, "%EInternal lossy transmission line error-cannot find delayed time point. Contact Spectrum Software."
14183, "%ELossy transmission line length missing."
14184, "%EInternal lossy transmission error-auxiliary index is incorrect. Contact Spectrum Software."
14185, "%EIn lossy transmission lines, at least two of R,L,G,C must be specified and nonzero."
14190, "%EFailed to converge in specified number of iterations at time=%g."
14191, "%EFailed to converge during AC analysis Function source iterations."
14192, "%EFailed to converge at %g."
14193, "%EFailed to converge during the DC operating point."
14220, "Unassigned component button."
14225, "Save a Waveform to the Buffer"
14226, "Retain"
14282, "Hides the selected waveform"
14301, "Save or recall waveforms\nSave or recall waveforms"
14302, "Opens the Waveform Buffer which lets you recall or delete waveforms stored within the buffer.\nWaveform Buffer"
14303, "Saves the selected waveform to the Waveform Buffer"
14403, "Saves the selected waveform to the Waveform Buffer and places its name in the Analysis Limits for future simulations."
14500, "%ENlx = %g is less than -Leff."
14501, "%ETox = %g is not positive."
14502, "%ENch = %g is not positive."
14503, "%ENsub = %g is not positive."
14504, "%ENgate = %g Ngate is not positive."
14505, "%ENgate = %g Ngate is too high."
14506, "%EXj = %g is not positive."
14507, "%EDvt1 = %g is negative."
14508, "%EDvt1w = %g is negative."
14509, "%E(W0 + Weff) = 0 causing divided-by-zero."
14510, "%EDsub = %g is negative"
14511, "%E(B1 + Weff) = 0 causing divide-by-zero."
14512, "%Eu0 at current temperature = %g is not positive."
14513, "%EDelta = %g is less than zero."
14514, "%EVsat at current temperature = %g is not positive."
14515, "%EPclm = %g is not positive."
14516, "%EDrout = %g is negative."
14519, "%EClc = %g is negative."
14520, "%WLeff = %g may be too small."
14521, "%WLeff for CV = %g may be too small."
14522, "%WWeff = %g may be too small."
14523, "%WWeff for CV = %g may be too small."
14524, "%WNlx = %g is negative."
14525, "%WTox = %g is less than 10A."
14526, "%WNch = %g may be too small."
14527, "%WNch = %g may be too large."
14528, "%WNsub = %g may be too small."
14529, "%WNsub = %g may be too large."
14530, "%WNgate = %g is less than 1.E18cm^-3."
14531, "%WDvt0 = %g is negative."
14532, "%W(W0 + Weff) may be too small."
14533, "%WNfactor = %g is negative."
14534, "%WCdsc = %g is negative."
14535, "%WCdscd = %g is negative."
14536, "%WEta0 = %g is negative."
14537, "%Weff= %g may be too small."
14538, "%WA2 = %g is too small. Set to 0.01."
14539, "%WA2 = %g is larger than 1. A2 is set to 1 and A1 is set to 0."
14540, "%WRdsw = %g is negative. Set to zero."
14541, "%WRds at current temperature = %g is negative. Set to zero."
14542, "%WVsat at current temperature = %g may be too small."
14543, "%WPdibl1 = %g is negative."
14544, "%WPdibl2 = %g is negative."
14545, "%WCgdo = %g is negative. Set to zero."
14546, "%WCgso = %g is negative. Set to zero."
14547, "%WCgso = %g is negative. Set to zero."
14548, "%EThe effective channel length is %g. It must be positive."
14549, "%EThe effective channel width is %g. It must be positive."
14550, "%EThe effective channel length for C-V is %g. It must be positive."
14551, "%EThe effective channel width for C-V is %g. It must be positive."
14552, "%EToxm = %g is not positive."
14553, "%WNoff = %g is too small."
14554, "%WNoff = %g is too large."
14555, "%WVoffcv = %g is too small. It must be in the range -.5 to +.5."
14556, "%WVoffcv = %g is too large. It must be in the range -.5 to +.5."
14557, "%WMoin = %g is too small. It should be in the range 5 to 25."
14558, "%WMoin = %g is too large. It should be in the range 5 to 25."
14559, "%WAcde = %g is too small. It should be in the range .4 to 1.6."
14560, "%WAcde = %g is too large. It should be in the range .4 to 1.6."
14561, "%ELintnoi = %g is too large - Leff for noise is negative."
14562, "%ENGATE = %g. It must be positive."
14570, "Lets you add a new Performance window.\nAdd Performance"
14573, "Lets you select an existing Performance window."
14583, "Displays a list of the open Performance Plot windows.\nPerformace windows"
14600, "Lets you add a new 3D window.\nAdd 3D"
14603, "Lets you select an existing 3D window."
14613, "Displays a list of the open 3D windows.\n3D windows"
14620, "Selects the variable for the X axis."
14621, "Selects the variable for the Y axis."
14622, "Selects the variable for the Z axis."
14650, "Lets you add a new Fourier window.\nAdd Fourier"
14652, "Lets you select an existing Fourier window."
14662, "Displays a list of the open Fourier windows.\nFourier windows"
14669, "Displays a list of options for the sliders.\nSlider"
14670, "Add a floating slider to the screen.\nAdd Slider"
14672, "Displays the selected floating slider in the window."
14682, "Displays a list of the open Slider windows.\nSlider windows"
14701, "%EYour request exceeds the HASP HL memory range."
14702, "%EYou have requested an unknown ‘PROGRAM NUMBER FEATURE’."
14703, "%EYour system is out of memory."
14704, "%EThere are too many open handles."
14705, "%EAccess to feature is denied."
14706, "%EThe legacy decryption function cannot work on the feature."
14707, "%EThe HASP HL key is no longer available."
14708, "%EDecrypted data length is too short to execute the function call."
14709, "%EYou have passed an invalid handle to the function."
14710, "%ESpecified fileid is not recognized by the API."
14711, "%EThe installed driver is too old to execute the function."
14712, "%EA real-time clock (rtc) is not available."
14713, "%EGeneric error from host system call."
14714, "%EThe required driver is not installed."
14715, "%EUnrecognized file format for update."
14716, "%EThe function cannot be executed in this context."
14717, "%EThe binary data passed to the function does not contain an update."
14718, "%EThe HASP HL license you requested to update has not been found."
14719, "%EThe required XML tags not found. Contents in the binary data are missing or invalid."
14720, "%EThe update request is not supported by the HASP HL key."
14721, "%EThe update counter is not set properly."
14722, "%EYou have passed an invalid vendor code."
14723, "%EThe used hardware does not support the encryption type."
14724, "%EThe passed time value is beyond the supported value range."
14725, "%EReal-time clock battery has run out of power."
14726, "%EAcknowledge data requested by the update ack_data parameter is NULL."
14727, "%EProgram is running remotely on a Terminal Server."
14728, "%EThe type of feature requested is not implemented."
14729, "%EUnknown algorithm used in V2C file."
14730, "%EThe signature verification operation has failed."
14731, "%EThe requested feature is no longer available."
14732, "%ETrace log is not enabled"
14750, "%EObject not initialized correctly."
14751, "%EParsed parameter is incorrect."
14752, "%ELogging in twice to the same object."
14753, "%ELogging out twice from the same object."
14754, "%EError related to incorrect use of system or platform."
14755, "%EThe requested type of feature is not implemented."
14860, "%EThe file %s should be present in the path specified in the Document field in the Path dialog box.\nIf not present, the file can be downloaded from www.spectrum-soft.com."
14861, "%WMust restart Micro-Cap after an Install in order to load a PDF file.\nExit and rerun Micro-Cap"
14862, "Welcome to Micro-Cap.\nPlease exit the program and rerun from the Start menu, the desktop icon,\nor DOS prompt to insure that all features are properly initialized.\n\nDo you want to Exit Micro-Cap?"
14923, "Flips the order of the Z axis values in the 3D plot."
14930, "Lets you add a new Harmonic Distortion window.\nAdd Harmonic Distortion"
14932, "Lets you select an existing Harmonic Distortion window."
14942, "Displays a list of the open Harmonic Distortion windows.\nHarmonic Distortion windows"
14960, "Lets you add a new Intermodulation Distortion window.\nAdd Intermodulation Distortion"
14962, "Lets you select an existing Intermodulation Distortion window."
14972, "Displays a list of the open Intermodulation Distortion windows.\nIntermodulation Distortion windows"
15000, "%WThe number of Monte Carlo runs has been changed to the upper limit of %s."
15001, "%EMonte Carlo population exceeded"
15002, "%EInsufficient memory."
15003, "%EFloating point '%s'."
15007, "%EError in loading file %s."
15008, "%EError in writing file %s."
15009, "%EBad format in loading file '%s'."
15010, "%EInvalid File name. '%s'"
15015, "%EThe OPAMP '%s', has a negative value for C2."
15016, "%EIn the OPAMP '%s', Ibias must be > Ioff/2."
15017, "%EIn the OPAMP '%s', SRP must be > 4*PI*gbw*VT."
15018, "%EIn the OPAMP '%s', ZoDC must be greater than ZoAC."
15019, "%EIn the OPAMP '%s', which has NPN inputs, SRP must be >= SRN."
15020, "%EIn the OPAMP '%s', which has PNP or JFET inputs, SRN must be >= SRP."
15022, "%EFile not found '%s'."
15023, "%ECannot access '%s'."
15024, "%ESecurity key missing. Please replace the key. (Error=1000)"
15025, "%ESecurity key missing. Please replace the key."
15026, "%WCircuit '%s' contains illegal coordinates."
15027, "%EIn the OPAMP '%s', SRN must be > 4*PI*gbw*VT."
15028, "%EIn the OPAMP '%s', Vcc must be >= VPS."
15029, "%EIn the OPAMP '%s', Vee must be <= VNS."
15032, "%EIllegal digital state on DtoA input."
15033, "%ECan't find X or 0 states in AtoD model."
15034, "%ECan't find X or 0 states in DtoA model."
15035, "%EIllegal state character in model statement."
15038, "%EMust specify filename."
15040, "%EMissing parameter."
15047, "%EMissing Quotes in %s."
15048, "%EMissing Quote(s)."
15049, "%WNo items found matching '%s'."
15050, "%EIn the OPAMP '%s', PD must be larger than %s."
15051, "%EMatrix is singular."
15053, "%EUnknown"
15080, "%EComponent(s) not found.\n%s"
15082, "Insufficient memory."
15084, "%EPSS can not be run with circuits containing digital elements."
15099, "%EFloating point 'math error'"
15100, "%EFloating point 'invalid operation'"
15101, "%EFloating point 'denormal'"
15102, "%EFloating point 'division by zero'"
15103, "%EFloating point 'overflow'"
15104, "%EFloating point 'underflow'"
15105, "%EFloating point 'inexact'"
15106, "%EFloating point 'unemulated'"
15107, "%EFloating point 'neg sqrt()'"
15108, "%EFloating point 'stack overflow'"
15109, "%EFloating point 'stack underflow'"
15111, "%EFloating point Unknown error"
15112, "%EFloating point 'Multiple Faults'"
15113, "%EFloating point 'Multiple Traps'"
15120, "%EThis waveform format is not supported."
15140, "%EInstances must be >0 and their product can not exceed 1024."
15159, "%EMemory Access Violation."
15200, "%1 from %2"
15201, "Connected to %1"
15202, "Resolving name: %1"
15203, "Resolved name to %1"
15204, "Connecting to %1"
15205, "Redirecting to %1"
15206, "Getting file information"
15207, "An error occurred while attempting to download the file, Error:%1"
15208, "An error occurred connecting to the server, Error:%1"
15209, "Failed to receive a valid response from the server"
15210, "Failed to receive a valid HTTP response from the server, Error:%1"
15211, "An error occurred while downloading the file, Error:%1"
15212, "%1% of %2 completed"
15213, "Retrieving the files for %1"
15214, "%1 of %2"
15215, "%1 sec"
15216, "%1 min"
15217, "%1 min %2 sec"
15218, "%1 Bytes"
15219, "%1 KB"
15221, "%1 MB"
15223, "%1 (%2 copied)"
15224, "%1 Bytes/Sec"
15225, "%1 KB/Sec"
15226, "An error occured while opening the file to be downloaded, Error:%1"
15227, "Aborting transfer"
15240, "%1 GB"
15251, "This procedure will:\n\tLet you save any changed files.\n\tDownload the latest program from the web.\n\tDownload the English Resource.\n"
15252, "\tDownload the %s Resource\n"
15253, "\tExit Micro-Cap.\n\tRerun the new version.\nThe old version will be saved under the names:\n\t"
15254, "This procedure will download:\n\t%s\n\t%s"
15255, "This procedure will download:\n\t%s\n\t%s\n\t%s\n\t%s\n\t%s\n"
15256, "This procedure will download:\n\tAll of the Micro-Cap sample circuits\n\tthat are specified in the Help -> Sample Circuit Menu\n"
15257, "This procedure will:\n\tDownload New libraries files\n\tUpdated nom.lib\n\tUpdate Standard.cmp with new items\n\tUpdate Standard.shp with new items\n"
15312, "Accesses the global optimization error criteria.\nGlobal Optimization Settings"
15313, "Accesses the local optimization error criteria.\nLocal Optimization Settings"
15314, "Scales the plot automatically.\nAuto Scale"
15316, "Lets you edit the minimum, initial value, and maximum model parameter values.\nModel Defaults"
15317, "Creates a new Model data file.\nNew Model Data File"
15318, "Opens an existing model data file.\nOpen Model Data File"
15319, "Merges the current data file with one from the disk.\nMerge"
15320, "Sorts the data file using the NAME field.\nSort"
15321, "Deletes a line of data in the Numeric data fields.\nDelete Data"
15322, "Changes polarity of a part. For example, from NPN to PNP.\nChange Polarity"
15323, "Toggles between SI (Tesla-A/m) and CGS (Gauss-Oersted) units.\nToggle between SI and CGS units."
15324, "Model"
15325, "Edits the properties of the current graph.\nEdit Graph"
15329, "Adds a part to the current model file.\nAdd Part"
15330, "Adds a diode.\nAdds a diode"
15331, "Adds a NPN.\nAdds a NPN"
15332, "Adds a PNP.\nAdds a PNP"
15333, "Adds a NMOS.\nAdds a NMOS"
15334, "Adds a PMOS.\nAdds a PMOS"
15335, "Adds a NJFET.\nAdds a NJFET"
15336, "Adds a PJFET.\nAdds a PJFET"
15337, "Adds an opamp.\nAdds an opamp"
15338, "Adds a core.\nAdds an core"
15339, "Lets you manually change the plot scale.\nManual Scale"
15340, "Deletes the displayed part from the open model file.\nDelete Part"
15341, "Shows a list of all parts in the file. Can cut, copy, paste, or delete.\nParts List"
15342, "Imports an array of numeric values from the clipboard.\nClipboard Data Import"
15343, "Shows the previous part.\nPrevious Part"
15344, "Shows the next part.\nNext Part"
15345, "Shows the first part in the data file.\nFirst Part"
15346, "Shows the last part in the data file.\nLast Part"
15347, "Shows the previous graph.\nPrevious Graph"
15348, "Shows the next graph.\nNext Graph"
15349, "Shows the first graph of the current part.\nFirst Graph"
15350, "Shows the last graph of the current part.\nLast Graph"
15351, "Shows all graphs at once.\nShow all Graphs"
15352, "Shows only one graph at a time.\nShow one Graph"
15364, "Initializes the model parameters for the displayed graph of the part.\nInitializes"
15365, "Optimizes the model parameters to fit the supplied data points.\nOptimizes"
15366, "Initializes each part in the data file.\nInitializes All"
15367, "Optimizes each part in the file without initialization.\nOptimizes All"
15369, "Initializes all of the graphs for this part.\nInitialize All Graphs"
15370, "Optimizes all of the graphs for this part.\nOptimize All Graphs"
15371, "Fills in X or Z data values into the approprate table column.\nFill Data"
15376, "Creates a model for the current part.\nCreate Model for this Part"
15377, "Creates models for all parts in the model file.\nCreate Models for all Parts"
15383, "Adds a User created part.\nAdds a User part"
15384, "Adds a new graph window to the user created part.\nAdd Graph"
15385, "Sets the order of the graph windows for the user created part.\nOrder Graph"
15386, "Deletes the selected graph window.\nDelete Graph"
15387, "Opens the template library to select a user created part.\nTemplate Library"
15388, "Saves the existing user created part to the template library.\nSave Part to Template library"
15389, "Edits the list of parts in the current template library.\nEdit Template Library"
15390, "Adds the specified user created part."
15400, "Lets you step a model parameter to view the effect on the curve.\nStep"
15415, "%WThe file %s already exists.\nDo you want to overwrite it?"
15416, "%s successfully merged into %s\nMerged parts placed at the end of the list in this file."
15425, "Creates SPICE file with the extension .LIB.\nAdd These Parts to the Component Library"
15498, "Graph Properties"
15502, "Left justify the header in the numeric output, State Variables output, or Monte Carlo statistics file."
15503, "Center the header in the numeric output, State Variables output, or Monte Carlo statistics file."
15504, "Right justify the header in the numeric output, State Variables output, or Monte Carlo statistics file."
15505, "Set tab delimiter for the numeric output, State Variables output, or Monte Carlo statistics file."
15506, "Set semicolon delimiter for the numeric output, State Variables output, or Monte Carlo statistics file."
15507, "Set comma delimiter for the numeric output, State Variables output, or Monte Carlo statistics file."
15508, "Set space delimiter for the numeric output, State Variables output, or Monte Carlo statistics file."
15509, "Set other delimiter for the numeric output, State Variables output, or Monte Carlo statistics file."
15510, "Set other delimiter for the numeric output, State Variables output, or Monte Carlo statistics file."
15514, "Shows the numeric output header as it will appear when the file is created."
15678, "Lets you change the window's properties.\nProperties"
15679, "Lets you change the initial properties for graphic objects.\nGraphic Object Properties"
15684, "Controls the pattern of the selected waveform."
15685, "This selects the style used to mark data points. Data points are shown only if Scope / View / Data Points is enabled."
15688, "This selects one of two curve styles, Normal or Popsicle."
15690, "Sets the default numeric format for analysis tags."
15693, "Sets the numeric format for formula text."
15695, "Curve Line"
15696, "Curve Text"
15697, "Background"
15698, "Foreground"
15701, "Chooses the waveform to save to the user file."
15702, "Saves the waveform to the user file."
15703, "Deletes the waveform from the user file."
15705, "Defines the name of the waveform to be saved."
15706, "Browses for user files."
15707, "User file name."
15708, "Number of interpolated datapoints to print to the numeric output file."
15709, "Prints actual (rather than interpolated) data points to the numeric output file."
15710, "Sets the sample rate for the selected waveform."
15711, "Sets the number of bits for the selected waveform."
15712, "Starts playing the selected waveform."
15713, "Stops playing the selected waveform."
15714, "Sets the maximum range for the selected waveform."
15715, "Automatically saves the selected waveforms."
15716, "Sets the format that will be used in the corresponding file."
15718, "Sets the file type that will be exported by selecting the extension of the file."
15719, "Calculates an autorange that will be used for the WAV file output."
15726, "Add a new plot."
15727, "Delete highlighted plot."
15811, "Apply Display Properties of %1 to all %2"
15812, "Apply Display Properties..."
15813, "Label Time Points..."
15814, "Label Frequency Points..."
15815, "Label Input Sweep Points..."
15900, "This page controls the auto save features."
15901, "Automatically saves the circuit to disk prior to running an analysis."
15902, "Automatically saves the circuit to disk on a specified time interval."
15903, "Time interval between automatic circuit saves."
16001, "Displays all possible curves for the object clicked on.\nAll"
16002, "Deletes all curves from the Window.\nDelete all Plots"
16003, "Places analog and digital curves in separate plot groups.\nSeparate Analog and Digital"
16004, "Displays one curve only.\nOne Curve"
16005, "Displays multiple curves.\nMany Curves"
16006, "Saves all possible curves for plotting.\nSave All"
16007, "Saves only states, voltages, and currents for plotting.\nSave V and I Only"
16008, "Displays voltage curves.\nVoltage"
16009, "Displays current curves.\nCurrent"
16010, "Displays energy curves.\nEnergy"
16011, "Displays power curves.\nPower"
16012, "Displays resistance curves.\nResistance"
16013, "Displays charge curves.\nCharge"
16014, "Displays capacitance curves.\nCapacitance"
16015, "Displays flux curves.\nFlux"
16016, "Displays inductance curves.\nInductance"
16017, "Displays B field waveforms.\nB"
16018, "Displays H field waveforms.\nH"
16019, "Sets time as Y-axis variable.\nTime"
16021, "Sets voltage as X-axis variable.\nVoltage"
16022, "Sets current as X-axis variable.\nCurrent"
16023, "Sets Energy as X-axis variable.\nEnergy"
16024, "Sets power as X-axis variable.\nPower"
16025, "Sets resistance as X-axis variable.\nResistance"
16026, "Sets charge as X-axis variable.\nCharge"
16027, "Sets capacitance as X-axis variable.\nCapacitance"
16028, "Sets flux as X-axis variable.\nFlux"
16029, "Sets inductance as X-axis variable.\nInductance"
16030, "Sets B Field as X-axis variable.\nB"
16031, "Sets H Field as X-axis variable.\nH"
16032, "Sets time as X-axis variable.\nTime"
16033, "Displays conductance curves.\nConductance"
16034, "Displays impedance curves.\nImpedance"
16035, "Displays input noise waveform.\nInput noise"
16036, "Displays output noise waveform.\nOutput noise"
16037, "Sets frequency as Y-axis variable.\nFrequency"
16038, "Calculates magnitude of waveform.\nMagnitude"
16039, "Calculates magnitude in dB of waveform.\nMagnitude in dB"
16040, "Calculates phase of waveform.\nPhase"
16041, "Calculates group delay of waveform.\nGroup Delay"
16042, "Calculates real part of waveform.\nReal"
16043, "Calculates imaginary part of waveform.\nImaginary"
16046, "Displays conductance curves.\nConductance"
16047, "Displays impedance curves.\nImpedance"
16048, "Sets input noise as X-axis variable.\nInput Noise"
16049, "Sets output noise as X-axis variable.\nOutput Noise"
16050, "Sets frequency as X-axis variable.\nFrequency"
16051, "Calculates magnitude of X-axis variable.\nMagnitude"
16052, "Calculates magnitude in dB of X-axis variable.\nMagnitude in dB"
16053, "Calculates phase of X-axis variable.\nPhase"
16054, "Calculates group delay of X-axis variable.\nGroup Delay"
16055, "Calculates real part of X-axis variable.\nReal"
16056, "Calculates imaginary part of X-axis variable.\nImaginary"
16063, "Displays Y-axis in linear scale.\nLinear scale Y"
16064, "Displays Y-axis in log scale.\nLog scale Y"
16065, "Draws X-axis with a linear scale.\nLinear scale X"
16066, "Draws X-axis with a log scale.\nLog scale X"
16067, "Pauses the analysis...can be restarted from the same point.\nPause"
16068, "Runs the analysis.\nRun"
16069, "Stops the analysis...can't be restarted from the same point.\nStop"
16070, "Calculates the next data point in animation analysis mode.\nResume"
16071, "Accesses the Analysis Limits dialog box.\nLimits"
16078, "Selects plot group 1.\nGroup 1"
16079, "Selects plot group 2.\nGroup 2"
16080, "Selects plot group 3.\nGroup 3"
16081, "Selects plot group 4.\nGroup 4"
16082, "Selects plot group 5.\nGroup 5"
16083, "Selects plot group 6.\nGroup 6"
16084, "Selects plot group 7.\nGroup 7"
16085, "Selects plot group 8.\nGroup 8"
16086, "Selects plot group 9.\nGroup 9"
16087, "Places each new waveform in its own plot group.\nGroup individual"
16088, "Lets you delete selected waveforms from window.\nDelete Curves"
16089, "Lets you enter a Y expression to plot. X expressions are implicit but may be edited from the F10 dialog box.\nAdd Curve"
16090, "Plot number field must be a number from 1 to 19."
16093, "Stage"
16094, "Default"
16095, "Bode"
16096, "Step"
16097, "Impulse"
16098, "Circuit"
16099, "Gain"
16100, "Invokes the Active Filter Designer.\nActive Filters"
16470, "Invokes the Passive Filter Designer.\nPassive Filters"
16484, "%EIinternal API error"
16500, "Enables X and Y data for cursor mode trackers.\nTracker Cursor"
16501, "Enables X/Y intercept trackers.\nTracker Intercept"
16502, "Enables a tracker at the mouse position.\nTracker Mouse"
16503, "Enables branch data for cursor mode trackers.\nTracker Cursor: Branch Info"
16601, "Adds or updates local (within the circuit) model statement parameters using originals from the model libraries."
16602, "Adds or updates local (within the circuit) subckts using originals from the model libraries."
16603, "Adds missing but does not update existing model statements, subckts, or macros in the local circuit."
16604, "Updates existing and adds missing model statements, subckts, or macros in the local circuit."
16605, "When enabled, the Localize Models command only applies to components that are selected in the schematic."
16606, "Adds or updates local (within the circuit) macro sections using originals from the macro files."
16609, "%ESelected parts can only be localized in a single section at a time."
16610, "Localizes (embeds) the standard resistor sizes file if used by the circuit."
16611, "Localizes (embeds) the standard inductor sizes file if used by the circuit."
16612, "Localizes (embeds) the standard capacitor sizes file if used by the circuit."
16613, "Localizes (embeds) any digital stimulus (STM) file if used by the circuit."
16614, "Localizes (embeds) any User source (USR) file if used by the circuit."
16615, "Localizes (embeds) any JED digital (JED) file if used by the circuit."
16616, "Localizes (embeds) any Touchstone (S2P) file if used by the circuit."
16617, "Localizes (embeds) any image file if used by the circuit."
16618, "Localizes (embeds) mcap.inc"
16711, "Page"
16712, "P"
16713, "X Expression"
16714, "Y Expression"
16715, "X Range"
16716, "Y Range"
16717, ">"
16801, "For Limit Field:"
16811, "Default"
16812, "Set as Default"
16900, "Worst Case"
16902, "Worst Case\nWorst Case"
16903, "Performs a DC OP worst case analysis on the active circuit.\nDC OP Worst Case"
16904, "Computes sensitivity and includes it in the output file."
16905, "Computes the RSS (root-sum-squared) measure of output function change and prints it in the output file."
16906, "Computes the extreme high and low measures of output function change and prints them in the output file."
16907, "Computes the EVA solution using the internal optimizer. It is more accurate but slower than the standard EVA."
16908, "Computes the Monte Carlo analysis measure of output function change and prints it in the output file."
16909, "Shows the selected input variable parameters and their tolerances."
16911, "Estimates DV from sensitivity rather than computing it directly by running another analysis."
16912, "Lets user specify one or more output expressions. Right-click for options."
16913, "Calculates the specified measures of output function change."
16914, "Causes the windows to be tiled. Otherwise the windows remain unchanged."
16916, "Clicking on an item in this list causes the output to be sorted numerically by the selected item."
16918, "Creates an Excel output file in addition to a text file output."
16920, "Shows analysis plots and histograms. The analysis is usually faster when it is off."
16921, "Includes the RSS table in the output"
16922, "Includes the EVA table in the output"
16923, "Includes the Monte Carlo detail in the output"
16924, "Includes the Worst Case Change table in the output"
16925, "Includes the Worst Case Value table in the output"
16926, "Includes the Worst Case Percent Change table in the output"
16927, "Copy tolerances selected below to all devices of the same type and parameter name"
16928, "Copy selected table entry to all devices of the same type and parameter name"
16930, "Variable"
16931, "Name"
16932, "Tolerance"
16933, "Output"
16934, "Sensitivity"
16935, "Sensitivity(%/%)"
16936, "RSS Variance Low"
16937, "RSS Variance High"
16938, "Value"
16940, "By Extreme Value Low"
16941, "By Extreme Value High"
16942, "By Root Sum Squared Low "
16943, "By Root Sum Squared High"
16944, "By Monte Carlo Analysis Low"
16945, "By Monte Carlo Analysis High"
16946, "Nominal"
16948, "RSS Min Tol%"
16949, "RSS Max Tol%"
16950, "EVA Min Tol%"
16951, "EVA Max Tol%"
16952, "RSS Parameter Low"
16953, "RSS Parameter High"
16954, "EVA Parameter Low"
16955, "EVA Parameter High"
16956, "Low"
16957, "High"
16958, "%EMust have at least one component with initial LOT tolerances specified in order to run Worst Case Analysis."
16959, "%EEnter a performance function here like PEAK_Y(V(OUT),1,1)"
16960, "%ECan't step temperature while using Worst Case Analysis."
16961, "%WAll tolerances are zero so worst case output suspended."
16962, "%EEnter an expression here like V(OUT)"
16969, "%ECan't use the second DC transfer variable in Worst Case (must be set to None)."
16970, "%EEither Neg or Pos must be left blank or 0."
16971, "%EIf the main parameter is zero, then all tolerances must be absolute. Percentage tolerances cannot be used with a zero-valued parameter."
16972, "Initial"
16975, "Adds a new bias tolerance type."
16976, "Deletes the selected bias tolerance type."
16977, "Shows and lets you edit the selected bias tolerance type."
17012, "Sets the value and scale numeric formats."
17014, "Includes numeric data in saved graphic images of histograms."
17015, "Sets the upper limit in the histogram to the value of the highest column."
17051, "Recreates circuits that failed a Monte Carlo run.\nLoad MC File"
17070, "Move Item Up"
17071, "Move Item Down"
17072, "Cut Item"
17073, "Delete Item"
17074, "Copy Item"
17075, "Paste Item"
17076, "Insert Item"
17098, "Run Options"
17099, "State Variables"
17102, "Incorrect expressions in X or Y fields are tinted red but not plotted."
17105, "Sets the ranges to auto at the beginning of each run."
17106, "Runs the analysis."
17107, "Adds another curve line."
17108, "Deletes the curve line where the cursor is."
17109, "Expands the text field where the cursor is."
17110, "Accesses the Stepping dialog box."
17112, "Defines whether simulation is saved to or retrieved from disk."
17113, "Defines the starting position of the simulation if operating point is off."
17114, "Determines the method for calculating the spot of the next data point."
17115, "Calculates an operating point in starting the analysis."
17116, "Calculates only an operating point."
17117, "Defines the method for sweeping the second variable."
17118, "Defines the method for stepping the temperature."
17120, "Selects the method for stepping the amplitude."
17121, "Automatically resizes the analysis limits dialog box."
17122, "Expands the list of all waveforms created by the specified waveform subset."
17123, "Selects linear, log, or list stepping for the F2 level."
17125, "Controls the graph page the curve will be present in."
17126, "Controls the graph group the curve will be present in."
17127, "Defines the expression for the X-axis[,Alias][;Comment]."
17128, "Defines the expression for the Y-axis[,Alias][;Comment]. Click the right mouse button for a variable menu."
17129, "Defines the range of the X-axis. Format is <high>[,<low>[,<grid spacing>[,<bold grid spacing>]]][;<comment>]."
17130, "Defines the range of the Y-axis. Format is <high>[,<low>[,<grid spacing>[,<bold grid spacing>]]][;<comment>]."
17150, "Defines the model parameter for the first swept variable."
17151, "Defines the model parameter for the second swept variable."
17155, "Retains waveforms from previous runs during this analysis session."
17157, "Assigns SMPTE standard values for F1, F2, F1/F2 Level Ratio, and F2 Level."
17158, "A fixed time step will be used during the simulation based on the Maximum Time Step value."
17159, "Calculates a Periodic Steady State to use at the start of the simulation."
17160, "Assigns CCIF standard values for F1, F2, F1/F2 Level Ratio, and F2 Level."
17161, "Assigns DIN standard values for F1, F2, F1/F2 Level Ratio, and F2 Level."
17168, "Accesses the Periodic Steady State dialog box in order to modify the PSS settings."
17170, "Shows Monte Carlo statistics.\nStatistics"
17171, "Deletes all text, markers, or shapes.\nDelete All Objects"
17172, "Automatically scales the X and Y axes.\nAuto Scale"
17175, "Replots using the current range limits from the Analysis Limits dialog box.\nRestore Limit Scales"
17176, "Creates an envelope enclosing all branches of the selected waveform.\nEnvelope"
17177, "Removes all of the accumulated waveforms from the analysis plot page on the next run.\nClear Accumulated Plots"
17178, "Automatically scales the Y axes over the visible X regions.\nAuto Scale Visible Region"
17180, "Shows the Watch window where you can watch expressions values.\nWatch"
17181, "Allows single-stepping through data point values on a schematic.\nAnimate"
17182, "Opens the Breakpoints dialog box.\nBreakpoints"
17183, "Shows the Error Window.\nError Window"
17184, "Finds a data point with a specific X value.\nGo to X"
17185, "Finds a data point with a specific Y value.\nGo to Y"
17186, "Places a tag at the left cursor.\nTag Left Cursor"
17187, "Places a tag at the right cursor.\nTag Right Cursor"
17188, "Places a horizontal tag between the left and right cursors.\nTag Horizontal"
17189, "Places a vertical tag between the left and right cursors.\nTag Vertical"
17190, "Forces all of the cursors from each graph to track.\nAlign Cursors"
17194, "Forces both cursors to track on the same curve.\nKeep Cursors on Same Branch"
17195, "This lets you select and color a left and right branch for each curve.\nGo To Branch"
17196, "Go To Branch."
17198, "Show Smoke display.\nShow Smoke display"
17200, "Copies the cursor table values to the clipboard.\nCopy Cursor Values to Clipboard"
17206, "Copy the front window to the clipboard as a bitmap.\nCopy to Clipboard (BMP)"
17207, "Copies the selected schematic region multiple times in X and/or Y directions.\nStep Box"
17208, "Creates a mirror image of the selected schematic region.\nMirror"
17209, "Rotates the selected schematic region.\nRotate"
17210, "Flips the selected schematic region about the X-axis.\nFlip X"
17211, "Flips the selected schematic region about the Y-axis.\nFlip Y"
17213, "Searches for the specified object.\nFind"
17215, "Cuts wires at the select box boundaries.\nDelete Cut Wire"
17216, "Exit analysis.\nExit analysis"
17217, "Repeats the last Find command.\nRepeat"
17218, "Conducts a search and replace.\nReplace"
17219, "Copies the selected region to the clipboard in BMP format.\nCopy selected to Clipboard (BMP)"
17221, "Copies the entire window to the clipboard in WMF Placeable Format.\nCopy selected to Clipboard (WMF)"
17222, "Saves the window to an Image file.\nSaves Window to Image File     (for emf,wmf it's the whole window for bmp it visable part)"
17223, "Copies the entire window to the clipboard in EMF format.\nCopy selected to Clipboard (EMF)"
17224, "Create a macro component from the boxed area.\nMake Macro"
17227, "Copies the entire Circuit page to the clipboard in BMP format.\nCopy Circuit Page to Bitmap"
17228, "Saves color choice and SPICE type in a SPICE file."
17230, "Performs a transfer function analysis on the active circuit.\nTF"
17238, "Places the cursor between corresponding braces.\nGo to Brace"
17239, "Disables the selected circuitry for simulation.\nDisable"
17240, "Enables the selected circuitry for simulation.\nEnable"
17280, "Normalizes the selected curve using the maximum point in the curve.\nNormalize max"
17281, "Normalizes the curve at the cursor position.\nNormalize"
17282, "Normalizes the selected curve using the minimum point in the curve.\nNormalize min"
17291, "Opens the numeric output file.\nNumeric Output"
17292, "Shows the analysis Window.\nAnalysis"
17293, "Exit analysis.\nExit analysis"
17298, "Lets you enable a region with a formula.\nEnable with a formula"
17302, "Restores the default tool bar buttons and their arrangement.\nDefault Main Tool Bar"
17303, "Maximizes the Micro-Cap window over multiple monitors.\nMaximize over Multiple Monitors"
17304, "Overlaps the analysis and schematic windows.\nOverlap"
17305, "Maximizes the active window.\nMaximize"
17306, "Lets you activate, close, or save any of the loaded files.\nWindows"
17307, "Windows..."
17309, "Opens the Shape Editor.\nShape Editor"
17314, "Automatically checks all model parameters of parts in the model library against standard limit values.\nCheck Model Library Parameters"
17317, "Displays the circuit centered on the chosen flag.\nGo to Flag"
17320, "Navigates to the schematic level right above the current macro level.\nUp"
17322, "Opens the Title Block Editor for creating or editing title blocks.\nTitle Block Editor"
17323, "E&xit"
17330, "Accesses the Calculator.\nCalculator"
17366, "Lets you add a new Monte Carlo histogram.\nAdd Monte Carlo"
17371, "Lets you select an existing Monte Carlo histogram."
17381, "Displays a list of the open Monte Carlo windows.\nMonte Carlo windows"
17400, "Displays attribute text on the schematic.\nAttribute Text"
17401, "Flags unconnected pins with a yellow triangle.\nUnconnected Pins Warnings"
17402, "Displays grid text on the schematic.\nGrid Text"
17403, "Displays node numbers on the schematic.\nNode Numbers"
17404, "Displays node voltages or states on the schematic.\nNode Voltages"
17405, "Displays connection points on the schematic.\nPin Connections"
17406, "Creates a border for each sheet in the schematic.\nBorder for each Sheet"
17407, "Show the title block for the schematic.\nShow Title Block"
17408, "Displays a Cross-hair Cursor on the schematic.\nCross Cursor"
17409, "Creates a one border for the schematic.\nOne Border"
17410, "Sets the measurement type of the voltage, current, and power displays.\nVoltage, Current, and Power Measurement"
17411, "Displays the voltage, current, and power displays of the last calculated data point.\nLast"
17412, "Displays the voltage, current, and power displays of the RMS value.\nRMS"
17413, "Displays the voltage, current, and power displays of the average value.\nAverage"
17414, "Displays the voltage, current, and power displays of the peak value.\nPpeak"
17420, "Displays a grid on the schematic.\nGrid"
17421, "Displays no grid.\nGrid None"
17422, "Normal grid.\nNormal Grid"
17423, "Normal grid with bold marks every 5 grids.\nGrid Bold 5"
17424, "Normal grid with bold marks every 6 grids.\nGrid Bold 6"
17425, "Normal grid with bold marks at an interval specified on the Circuit Properties dialog box.\nGrid Bold User"
17426, "Displays a graph paper grid in the schematic background.\nGraph Paper"
17430, "Bold Grids User (%d)"
17450, "Changes the color of selected item.\nColor"
17451, "Changes the style of selected item.\nStyle"
17452, "Changes the font of selected item.\nFont"
17453, "Displays all possible digital paths.\nAll Paths"
17454, "Renames all component names using standard conventions.\nRename Components"
17455, "Renames all symbolic names that conflict with node text by adding an underscore character.\nRename Defines"
17456, "This resets all of the display values to their original positions.\nReset Node Positions"
17457, "Calculates the standard values needed to come close to the current value of the impedance elements.\nFit to Standard Value"
17460, "Selects options for a Monte Carlo run.\nMonte Carlo Options"
17461, "Specifies a the number of Monte Carlo runs."
17462, "Selects a normal or Gaussian distribution."
17463, "Selects a linear distribution."
17464, "Selects a worst case distribution."
17465, "Boolean condition statement that specifies when to add an exception report to the numeric output."
17466, "Shows available performance functions."
17467, "Enables Monte Carlo runs."
17468, "Disables Monte Carlo runs."
17469, "Defines the seed for the random number generator within Monte Carlo. Seed must be >0 to produce a repeatable sequence."
17470, "Runs the first simulation with no toleranced parameters."
17471, "Invokes the Tolerance dialog box to easily add tolerances to circuit parameters."
17481, "Places the seed value used in the previous run into the Seed field."
17500, "Automatically scales the Circuit to fit the page.\nAuto Scale"
17501, "Removes all splitters that have been placed in the window\nRemove Splitters"
17502, "Evenly spaces out all splitters in the window.\nSpace Splitters Evenly"
17503, "Splits the window vertically.\nSplit vertically"
17504, "Zoom-in on active window.\nZoom In"
17505, "Zoom-out on active window.\nZoom Out"
17506, "Places the panel in the schematic view.\nPanel"
17507, "Splits the window horizontally.\nSplit horizontally"
17508, "Toggles the component panel size between the users last size and an auto size.\nToggels Panel Size"
17509, "Enables the window tabs bar.\nWindow Tabs"
17541, "Toggles display of User palette 1.\nUser palette 1"
17542, "Toggles display of User palette 2.\nUser palette 2"
17543, "Toggles display of User palette 3.\nUser palette 3"
17544, "Toggles display of User palette 4.\nUser palette 4"
17545, "Toggles display of User palette 5.\nUser palette 5"
17546, "Toggles display of User palette 6.\nUser palette 6"
17547, "Toggles display of User palette 7.\nUser palette 7"
17548, "Toggles display of User palette 8.\nUser palette 8"
17549, "Toggles display of User palette 9.\nUser palette 9"
17561, "Enables Select mode. Click on an object to select it or drag to select a region.\nSelect Mode"
17562, "Enables Component mode. Click in the schematic to add the selected device.\nComponent Mode"
17563, "Enables Text mode. Click text.\nText Mode"
17564, "Enables Orthogonal Wire mode. Click and drag to add a wire at 0, 90, 180, 270 degrees.\nWire Mode"
17565, "Enables Diagonal Wire mode. Click and drag to add a wire at any angle.\nDiagonal Wire Mode"
17566, "Enables Bus mode. Click in the schematic to create the bus connection.  Use Wire mode to draw the bus wire.\nBus Mode"
17567, "Activates Component Help mode. Click on a component to see its parameter syntax.\nHelp Mode"
17568, "Enables Line Drawing mode. Click and drag to add a line.\nLine Mode"
17569, "Enables Ellipse Drawing mode. Click and drag to add an ellipse.\nEllipse Mode"
17570, "Enables Rectangle Drawing mode. Click and drag to add a rectangle.\nRectangle Mode"
17571, "Enables Diamond Drawing mode. Click and drag to add a diamond.\nDiamond Mode"
17572, "Enables Arc Drawing mode. Click and drag to add an arc.\nArc Mode"
17573, "Graphical left brace. Click and drag to add a brace.\nLeft Brace Mode"
17574, "Graphical right brace. Click and drag to add a brace.\nRight Brace Mode"
17575, "Graphical left and right brace pair. Click and drag to add a brace pair.\nBrace Pair Mode"
17576, "Enables Scale mode for analysis Window.\nScale Mode"
17577, "Enables Cursor mode for analysis Window.\nCursor Mode"
17578, "Enables Pie Drawing mode. Click and drag to add a pie.\nPie Mode"
17579, "Enables Flag mode. Click in the schematic to plant a flag.\nFlag Mode"
17580, "Enables Info mode. Click on a component to show its model, timing, or subcircuit description.\nInfo Mode"
17581, "Enable Horizontal Measure mode. Click and drag to measure horizontal delta.\nHorizontal Tag Mode"
17582, "Enable Vertical Measure mode. Click and drag to measure vertical delta.\nVertical Tag Mode"
17583, "Enable Tag mode. Click on the plot to add a data point tag.\nTag Mode"
17584, "Enables Point-to-end Path mode. Click on a gate to show its possible paths.\nPoint to End Paths Mode"
17585, "Enables Point-to-point Path mode. Click on two gates to show paths between.\nPoint to Point Paths Mode"
17586, "Invokes a menu of graphical objects for placement in the window.\nGraphics"
17587, "Enables Picture mode. Click to add a picture.\nImport Picture Mode"
17588, "Enables Closed Polygon mode. Click for points and double click to close.\nClosed Polygon"
17590, "Enables Probe mode. Click in the schematic to display the associated waveform.\nProbe"
17591, "Enables Function Tag mode. Click in the plot to place a function tag.\nFunction Tag Mode"
17592, "Enables File Link mode.  Click on a component to view its linked file.\nFile Link Mode"
17593, "Enables Region Enable mode.  Drag in the schematic to create a boolean defined enable region.\nRegion Enable"
17594, "Enables Title Block mode.  Click in the schematic to place a title block.\nTitle Block Mode"
17595, "Enables Star Drawing mode.  Click and drag to add a star.\nStar Mode"
17596, "Enables Check mode. Click in the schematic to add a Check Box.\nCheck Box Mode"
17597, "Enables Triangle mode. Click in the schematic to add a Check box.\nTriangle Mode"
17598, "Enables Spreadsheet mode. Click in the schematic to add a spreadsheet.\nSpreadsheet Mode"
17600, "Enables Open Polygon mode. Click for points and double click to end.\nOpen Polygon"
17601, "Enables Include Shape mode. Lets you include another shape in the current shape.\nInclude Shape Mode"
17602, "Enables Pan mode. Click and drag in the drawing area to pan.\nPan"
17603, "Enables Block mode. Click and drag to create a general Block symbol.\nBlock"
17604, "Enables Text mode. Click in drawing area to add text.\nText"
17605, "Enables the seven segment primitive drawing mode.\nSeven Segment"
17606, "Enables the digital LED primitive drawing mode.\nDigital LED"
17607, "Enables the animated switch primitive drawing mode.\nSwitch"
17608, "Enables the SPST switch primitive drawing mode.\nSPST Switch"
17609, "Enables the SPDT switch primitive drawing mode.\nSPDT Switch"
17610, "Enables the DPST switch primitive drawing mode.\nDPST Switch"
17611, "Enables the traffic light primitive drawing mode.\nTraffic Light"
17612, "Enables the animated meter primitive drawing mode.\nMeter"
17613, "Enables the analog bar primitive drawing mode.\nAnalog Bar"
17614, "Enables the relay primitive drawing mode.\nRelay"
17615, "Enables the analog LED primitive drawing mode.\nAnalog LED"
17616, "Enables the analog LED Circle primitive drawing mode.\nAnalog LED Circle"
17617, "Enables the motor primitive drawing mode.\nMotor"
17618, "Enables the current arrow drawing mode.\nCurrent Arrow"
17619, "Bring object to the front.\nBring To Front"
17620, "Send object to the back.\nSend To Back"
17621, "Selects the next object in a stack of overlapping objects.\nNext Object"
17622, "Runs transient analysis on the active circuit.\nTransient"
17623, "Runs AC analysis on the active circuit.\nAC"
17624, "Runs DC analysis on the active circuit.\nDC"
17625, "Runs transient analysis in Probe mode.\nProbe Transient"
17626, "Runs AC analysis in Probe mode.\nProbe AC"
17627, "Runs DC analysis in Probe mode.\nProbe DC"
17628, "Runs AC analysis and displays AC voltage, current, and power values on the schematic.\nDynamic AC"
17629, "Runs DC analysis and displays DC voltage, current, and power values on the schematic.\nDynamic DC"
17630, "Runs transient analysis and computes harmonic distortion using FFT functions.\nHarmonic Distortion"
17631, "Runs transient analysis and computes intermodulation distortion using FFT functions.\nIntermodulation Distortion"
17632, "Runs AC analysis and computes the phase and gain margins.\nStability"
17669, "Toggles between the drawing and text area.\nToggle Area"
17670, "Shuttles text between the schematic and a text page.\nMove Text"
17672, "Toggles between Select mode and the other most recent mode.\nToggle Mode"
17675, "Toggles the Vertical waveform selection in a Probe analysis.\nToggle Selection Mode"
17680, "The Status Bar"
17690, "Run a script stored in the loaded batch file.\nRun Script"
17750, "%EThere is an environment variable with an illegal setting."
17751, "Shows the Contents screen of the Help system.\nHelp Contents"
17752, "Search for Help On.\nHelp Search"
17753, "Product Support.\nProduct Support"
17754, "Provides a list of helpful tips.\nTips"
17755, "Shows a list of Micro-Cap 12's major new features.\nNew features"
17756, "Micro-Cap copyright notice.\nAbout"
17757, "Invokes the help topic for a selected SPICE keyword.\nSpice Help"
17759, "The Help file failed to load.\nDo you want to try and load it from the web?"
17802, "Don't change the mode at the end of the run."
17820, "Runs all of the demos.\nGeneral Demo"
17821, "Demonstrates the use of 3D plots.\n3D Plots Demo"
17822, "Demonstrates adding new parts to the model libraries.\nAdding New Parts Demo"
17823, "Demonstrates the use of mixed-mode circuits.\nAnalog and Digital Demo"
17824, "Demonstrates the use of the analyses.\nDemo analyses"
17825, "Demonstrates the use of the animation mode.\nDemo animation"
17826, "Demonstrates the use of the Dynamic DC analysis.\nDemo DC"
17827, "Demonstrates the use of the Filter Designer.\nDemo Filter"
17828, "Demonstrates the use of the FFT capabilities.\nDemo FFT"
17829, "Demonstrates the use of the Monte Carlo analysis.\nDemo Monte Carlo"
17830, "Demonstrates the use of performance plots.\nDemo performance"
17831, "Demonstrates the use of the probe analysis feature.\nDemo Probe"
17832, "Demonstrates how to create a schematic.\nDemo schematic"
17833, "Demonstrates Worst Case Analysis.\nDemo Worst Case Analysis"
17834, "Demonstrates the use of the stepping feature.\nDemo Stepping"
17836, "Demonstrates the use of the Transfer Function analysis.\nDemo Transfer Function"
17837, "Demonstrates the use of circuit optimizer.\nDemo Optimizer"
17838, "Demonstrates the use of RF tools, including S-Parameter two-ports and Smith charts.\nDemo RF"
17839, "Demonstrates the use of the Dynamic AC analysis.\nDemo Dynamic AC"
17840, "Demonstrates the use of the IBIS translator.\nDemo IBIS"
17841, "Demonstrates Stability Analysis\nDemo Stability Analysis"
17842, "Demonstrates the use of the .measure command\nDemo .measure command"
17850, "Provides help in downloading the latest version of the program.\nUpdate"
17851, "Accesses the User's Guide.\nUser's Guide"
17852, "Accesses the Reference Manual.\nReference Manual"
17853, "Loads the Spectrum Software website.\nWeb"
17854, "Register your copy of Micro-Cap online.\nRegistration"
17873, "Sets the outline color of the selected objects.\nLine"
17874, "Sets the fill color of the selected objects.\nFill"
17877, "Sets the fill color of the selected object."
17878, "Sets the outline color of the selected object."
17881, "Left Click to select the curve: Right Click for the Waveform Menu"
17882, "Left Click to select the curve"
17883, "Left Click to place the Left Cursor on the curve: Right Click to place the Right Cursor on the curve"
17884, "Text page for notes and action statements such as .DEFINE .MODEL and .SUBCKT."
17885, "The Info page shows the name and location of the models used in the analysis."
17886, "Text area"
17887, "Drawing area"
17888, "Wait"
17889, "Splitter: Double click to add or remove."
17892, "Tool bar"
17894, "Scroll bar"
17895, "Processing nodes."
17896, "Rewiring."
17898, "Hit %s to continue."
17899, "Double-click in the window for more options."
17900, "Double-click in the window for more options. Drag with the right mouse button to rotate the surface."
17901, "Use the cursor Up Arrow and Down Arrow keys to increment the part value."
17902, "Processing macros."
17903, "Processing subcircuits %s %s."
17904, "Remapping nodes."
17905, "Processing digital components."
17906, "Checking for voltage loops."
17907, "Scan for AtoD interface."
17908, "Processing device expressions."
17909, "Clearing arrays."
17910, "Click on a node or a part."
17911, "Click mouse to add additional vertices, or ESC to close the polygon."
17912, "Adding break points."
17913, "Select one or more batteries, resistors, capacitors, or inductors. Cursor keys change the values."
17914, "Select one or more batteries or resistors. Cursor keys change the values."
17915, "Processing K Devices."
17916, "Equation setup."
17917, "Process limits."
17918, "Alloc Graphs Arrays."
17919, "Setup .IC."
17920, "Updating Spice file."
17921, "Updating Secondary Windows."
17927, "Component Palette."
18001, "Closes this dialog box and saves any changes you have made."
18002, "Closes this dialog box without saving any changes you have made."
18009, "Invokes the help topic.\nHelp"
18012, "Saves all changes you have made without closing this Dialog box."
18022, "Changes the font."
18030, "Line"
18031, "Ellipse"
18032, "Rectangle"
18033, "Diamond"
18034, "Arc"
18035, "Pie"
18036, "Vertical Tag"
18037, "Point Tag"
18038, "Function Tag"
18039, "Horizontal Tag"
18040, "Picture"
18041, "Polygon"
18042, "Text"
18043, "{"
18044, "}"
18045, "{}"
18046, "Region Enable"
18047, "Title Block"
18048, "Star"
18049, "Triangle"
18050, "Marker"
18051, "Spreadsheet"
18052, "Parallelogram"
18053, "Data"
18054, "Process"
18055, "Off-page Connector"
18056, "Punch Card"
18057, "Manual Input"
18058, "Predefined Process"
18059, "Internal Storages"
18060, "Manual Operation"
18061, "Document"
18062, "Multidocument"
18063, "Stored Data"
18064, "Delay"
18065, "Summing Junction"
18066, "Or"
18067, "Collate"
18068, "Sort"
18069, "Preparation"
18070, "Terminator"
18071, "Punched Tape"
18072, "Sequential Access Storage"
18073, "Magnetic Disk"
18074, "Direct Access Storage"
18075, "Display"
18076, "Alternate Process"
18077, "Decision"
18078, "Connector"
18100, "Accesses the Stepping dialog box.\nStepping"
18101, "The part, model, or variable name"
18102, "The attribute or model parameter to be stepped."
18103, "The starting value"
18104, "The ending value"
18105, "The step value"
18106, "Steps in a linear fashion. New = Old + Step Value"
18107, "Steps in a log fashion. New = Old * Step Value "
18108, "Steps through the listed values."
18109, "Selects simple (non-model) components."
18110, "Selects models."
18111, "Selects symbolic variables, created by .define or .param statements)"
18112, "This selects temperature for stepping in Dynamic DC."
18113, "Enables stepping of the parameters shown on the panel."
18114, "Disables stepping of the parameters shown on the panel."
18116, "Steps all variables simultaneously."
18117, "Steps variables in nested loops"
18122, "This selects the start or next step value."
18123, "This ends the stepping process."
18124, "Suggests suitable From, To and Step values based upon the current value."
18125, "Enables stepping of the parameters on all panels."
18126, "Disables stepping of the parameters on all panels."
18179, "Extract"
18180, "Merge"
18202, "Weight (thickness) of the border"
18204, "The solid color or the top color of the gradient"
18205, "The gradient bottom color"
18206, "Default border color"
18209, "The number of instances of the text in the horizontal direction"
18210, "The distance between instances of the text in the horizontal direction"
18211, "The number of instances of the text in the vertical direction"
18212, "The distance between instances of the text in the vertical direction"
18213, "Allows insertion of special characters from menus.\nInsert special characters"
18221, "The text angle in degrees. Horizontal text = 0 degrees"
18230, "Specifies the text as Pin Text which displays only when the mouse hovers above the pin icon."
18231, "Treats all text between the specified delimiters [ ] as a formula to be computed."
18232, "Specifies the formula delimiters. Typical delimiters are [ ] and { }."
18234, "Specifies that the text is to be RTF (Rich Text Format). This let's you control the font and color of individual characters."
18235, "Helps to build some command statements such as .Measure, .Define, .Help, .Warning., or .Parameters\nBuild Command"
18237, "This is the vertical text anchor point. Text will hangs from either Bottom or Top"
18238, "This is the horizontal text anchor point. Text will hangs from either Center, Left or Right"
18239, "This enables the grid snap feature. If enabled, the text anchor point snaps to the nearest grid."
18240, "Specifies the thickness of the text outline."
18241, "Increments/decrements the value of this field"
18370, "Name"
18371, "Path"
18376, "Fits a linear or polynomial equation to a specified waveform.\nCurve Fit"
18400, "Marks the actual analysis data points.\nData Points"
18401, "Produces ruler tick marks for the analysis grid.\nRuler"
18402, "Applies tokens to the waveforms.\nTokens"
18403, "Adds major grid lines to the horizontal axis.\nHorizontal Axis Grids"
18404, "Adds major grid lines to the vertical axis.\nVertical Axis Grids"
18405, "Adds minor grid lines to any log axis.\nMinor Log Grids"
18406, "Adds a zero-valued baseline.\nBaseline"
18407, "Draws a \"+\" at the intersection of the horizontal and vertical grids, if they are enabled.\nPlus Mark"
18408, "Adds minor grid lines to any log axis in a 2/5/10 format.\nMinor Log Grids 2 5"
18409, "Labels minor grid lines when they are displayed in the analysis.\nLabel All Minor Grids"
18410, "Accesses option, limit, and control parameters.\nGlobal Settings"
18411, "Accesses a list of preference items.\nPreferences"
18412, "Displays the contents of the MCAP.INC text file which contains definitions available to all circuits.\nMCAP.INC"
18413, "This page lets you edit the colors available to Micro-Cap."
18414, "Loads a library of .Measure statements that can be used in any circuit file.\nMeasure.lib"
18415, "Displays a horizontal line marking the crossover for the phase or gain margin in Stability analysis.\nMargin Line"
18416, "Displays an arrow showing the phase or gain margin in Stability analysis.\nMargin Arrow"
18417, "Displays Phase and Gain Margin text on the Open plot."
18418, "Displays Phase and Gain Margin text on the Nyquist plot."
18419, "Lets you review or edit new circuit properties, for example color, font, and numeric format.\nDefault Properties For New Circuits"
18420, "Loads the NOM.LIB file from the LIBRARY folder.\nNOM.LIB"
18421, "Loads the logs files\nLogs"
18431, "Opens the Tool bar menu.\nMain Tool Bar"
18432, "Displays this Status bar for quick information.\nStatus Bar"
18438, "Default Properties For New Circuits"
18440, "Adds a horizontal cursor.\nHorizontal Cursor"
18451, "%d Digit Scientific"
18452, "%d Digit Engineering"
18453, "%d Digit Decimal"
18454, "%d Digit Default"
18470, "This page lets you edit the font used within the status bar."
18471, "Displays the threads count in the Status Bar."
18472, "Displays coordinates of the window in the Status Bar."
18473, "Displays the time in the Status Bar."
18485, "Selects a 2D or a 3D histogram."
18500, "Translates an LBR binary model library to an LIB text file model library containing model statements.\nConvert to SPICE Library"
18502, "Translates an LIB text file model library to an LBR binary model library containing model parameters.\nConvert to Binary Library"
18505, "This lets you migrate selected files from an earlier version of Micro-Cap.\nMigrate"
18506, "Creates a Bill of Materials for the circuit.\nBill of Materials"
18507, "Prints the active window to the printer directly skipping the Print Preview.\nPrint Window"
18508, "Saves the file in encrypted format. If protected, a user defined password must be supplied to open the file.\nProtect File"
18509, "Creates SPICE compatible models from IBIS files.\nIBIS"
18510, "Converts Touchstone files to other Touchstone parameter formats.\nTouchstone Files"
18511, "Creates PCB netlists.\nPCB netlists"
18512, "Prints the selected region using the current screen scale.\nPrint Select Region"
18650, "Close All\nClose All"
18670, "Advances to the next simulation data point in Cursor mode.\nNext Simulation Data Point"
18671, "Advances to the next rounded and interpolated data point in Cursor mode.\nNext Interpolated Data Point"
18672, "Advances to the local high in Cursor mode.\nPeak"
18673, "Advances to the local low in Cursor mode.\nValley"
18674, "Advances to the global high in Cursor mode.\nHigh"
18675, "Advances to the global low in Cursor mode.\nLow"
18676, "Advances to the inflection point in Cursor mode.\nInflection"
18677, "Finds the highest point on all curves.\nGlobal High"
18678, "Finds the lowest point on all curves.\nGlobal Low"
18685, "Finds the data point with the smallest Y value of all branches of the selected curve at the current cursor position.\nBottom"
18686, "Finds the data point with the largest Y value of all branches of the selected curve at the current cursor position.\nTop"
18687, "Labels branches of a curve with their stepped or case number values.\nLabel Branches"
18688, "Lets you specify data points to be labeled.\nLabel Data Points"
18689, "Adds a marker (vertical or horizontal line, or circle) to the plot area containing the selected wavefrom.\nMarker"
18699, "Lets you control the number of data points saved.\nReduce Data Points"
18711, "%E%s's Initial value must be greater than or equal to its Low value."
18712, "%E%s's High value must be greater than its Low value."
18713, "%E%s's Initial value must be less than or equal to its High value."
18809, "Sets the initial background pattern of graphical objects."
18810, "Sets the initial line pattern of graphical objects."
18811, "Sets the initial line thickness of graphical objects."
18822, "Applies the Border/Line color, weight, and pattern choices to analysis text,\nin addition to graphical objects and tags."
18823, "Applies the Fill color and pattern choices to analysis text,\nin addition to graphical objects and tags."
18830, "This enables the grid snap feature. If enabled, the object snaps to the nearest grid."
19001, "Description: Mandatory model name\nSyntax: <name>\nExamples: IRF710, 2N2222A, OP-02"
19002, "Description: Optional model name\nSyntax: [name]\nExample: RMODEL"
19003, "Description: Primary inductance, secondary inductance, coupling coefficient.\nSyntax: <Primary Inductance>, <Secondary Inductance>,<Coupling Coefficient>\nExample: 1m,10m,.98"
19004, "Description: Smoke\nSyntax: [name]\nExample: LOW_POWER"
19005, "Description: Multiplier, length (m), width (m), drain and source areas (m*m) and peripheries (m), number of drain, source, gate, and body squares, OFF keyword, initial conditions.\nSyntax: [M=val] [L=val] [W=val] [AD=val] [AS=val] [PD=val] [PS=val] [NRD=val] [NRS=val] [NRG=val] [NRB=val] [OFF] [IC=vds[,vgs[,vbs]]]\nExample: M=2 L=100u W=100u IC=6,2,.5"
19006, "Description: List of inductor names that are coupled.\nSyntax: <L1 L2...<Ln>>\nExample: L1 L2 L3"
19007, "Description: Required coupling value\nSyntax: <coupling value>\nExample: .999"
19008, "Description: Subcircuit name\nSyntax: <subckt name>\nExample: OP01"
19009, "Description: File name\nSyntax: [file name]\nExample: OP02.LIB"
19010, "Description: List of parameter names with optional default values\nSyntax: <<name>=<value>>*\nExample: L=1u C=2p Gain=20"
19011, "Description: List of text parameter names with optional default values\nSyntax: <<name>=<text value>>*]\nExample: MYFILE.OUT"
19012, "Description: File Name"
19013, "Description: Macro name\nSyntax: %s\nExample: CLIP"
19014, "Description: This attribute defines the nonlinear function expression.\nSyntax: <expr>\nExample: 1.5+2*sin(2*PI*1E6*t)+25*IB(Q1)"
19015, "Description: This attribute defines the nonlinear function expression.\nSyntax: <expr>\nExample: 1.5+2*sin(2*PI*1E6*t)+25*IB(Q1)"
19016, "Description: Two or more ordered pairs describing the transducer input/output characteristic curve\nSyntax: <<input value>,<output value>>\nExample: (0,0) (1.5,3) (10,26)"
19017, "Description: Set of frequency, magnitude, and phase values\nSyntax: <<frequency value>,<magnitude value>,<phase value>>*\nExample: (0,1,90) (1k,3,120) (3k,2.6,88)"
19018, "Description: This attribute defines the Laplace expression.\nSyntax: <expression using S variable>\nExample: 1/(1+.001*s+1E-8*s*s)"
19019, "Description: Polynomial keyword, pin names, coefficients\nSyntax: [POLY(<n>)] NC1+ NC1- [NC2+...][P0 P1...]\nExample: POLY(2) 10 0 5 0 0 0 0 0 1"
19020, "Description: Polynomial keyword, source names, coefficients\nSyntax: [POLY(<n>)] VN1 [VN2...][P0 P1...]\nExample: POLY(3) V1 V2 V3 0 1 1 1"
19021, "Description: Timing model name\nSyntax: <name>\nExample: DLY_TTL"
19022, "Description: I/O model name\nSyntax: <I/O model name>\nExample: IO_HC"
19023, "Description: Digital delay selector. 0=DIGMNTYMX 1=Min 2=Typ 3=Max 4=Worst Case\nSyntax: <value>\nExample: 2"
19024, "Description: Interface subckt select value\nSyntax: <value>\nExample: 0"
19025, "Description: Digital power node name\nSyntax: <node name>\nExample: $G_DPWR"
19026, "Description: Digital ground node name\nSyntax: <node name>\nExample: $G_DGND"
19027, "Description: Digital stimulus format array\nSyntax: <format array>\nExamples: 11 (two binary outputs), 44 (four hex output)"
19028, "Description: Symbolic name for the array of digital values shown in the Edit window.\nSyntax: <command>\nExample: See samples in Help under Stimulus Generators."
19029, "Description: Scale factor to multiply the time clock values specified using the 'c' character to get real time.\nSyntax: <value>\nExample: 1ns"
19030, "Description: Logic string used extensively in model text files. Rarely used in schematics.\nSyntax: <logic text>\nExample: g3bar = {~G3}"
19031, "Description: Pin delay text used extensively in model text files. Rarely used in schematics.\nSyntax: <text>\nExample: DPWR DGND Y_O W_O ENAB D0 D1"
19032, "Description: Constraint text used extensively in model text files. Rarely used in schematics.\nSyntax: <text>\nExample: DPWR DGND DCBAR D0 D1 D2 D3 D4 D6 D7 SCBAR S2"
19033, "[<B|O|X>$<initialization data>$]"
19034, "Description: Optional PLA data. Overridden by file data, if FILE attribute is specified.\nSyntax: [<radix flag>$<program data>$]\nExample: B$01 01 10 11 01 11 01 10 01"
19035, "<controlling voltage source name>"
19036, "Description: Signal names for the FSTIM device\nSyntax: <stimulus file signal name>*]\nExample: B0 B1 B2 B3"
19037, "Description: Optional text \nSyntax: [text]\nExample:"
19039, "[IS=Initial state]"
19040, "Description: This is the value or expression for the resistance, plus optional temperature coefficients.\nSyntax: <value | expression> [LOT[/#][/GAUSS|/UNIFORM|/WCASE]=[<tolvalue>[%]] | [<lowtolval>%,<hightolval>%]] [TC=<TC1>[,<TC2>]]\nExample: 1000 TC=1m,1u\nExample: 1000 Lot=10%"
19041, "Description: Diode area multiplier, plus optional OFF keyword, plus optional initial condition.\nSyntax: [area][OFF][IC=<vd>][M=value]\nExample: 2 OFF IC=2"
19042, "Description: Optional area multiplier, OFF keyword, and initial conditions.\nSyntax: [area][M=value][OFF][IC=<vbe>[,vce]]\nExample: 2 OFF IC=1,4"
19043, "Description: Optional area multiplier, OFF keyword, and initial conditions.\nSyntax: [area][M=value][OFF][IC=<vds>[,vgs]]\nExample: 3 OFF IC=6,2"
19044, "Description: Voltage value\nSyntax: <value>\nExample: 2.0"
19045, "Description: Optional frequency-dependent expression for use in AC and Stability only. Replaces VALUE above in AC and Stability only.\nSyntax: [expr]\nExample: 1e-4*(1+F/1e9)"
19046, "Description: Switch type keyword, Ron, Roff, On Level, Off Level\nSyntax: <[V]|[T]|[I]>,<n1,n2>[,<ron>[,<roff>]]\nExample: T,1m,5m\nExample: V,3,0,1m,1e6"
19047, "Description: Line parameters may be entered here or as a model (below).\nSyntax: [LEN=<val> R=<val> L=<val> C=<val> G=<val>] | \nZO=<val> [TD=<val>] | [F=<val> [NL=<val>]]\nExample: LEN=100 R=3m C=1p L=1.2n"
19048, "Description: This attribute defines the clock frequency for the Z expression.\nSyntax: <value>\nExample: 10k"
19049, "Description: The Z transfer function expression.\nSyntax: <expression using the Z variable>\nExample: (z*z+z)/pow(z-1,3)"
19050, "Description: DC value, AC magnitude, AC phase, transient analysis format parameters\nSyntax: [[DC]<value>] [AC<mag>[phase]] [PULSE] | [SIN] | [EXP] | [PWL] | [SFFM] [parameters]\nExample: DC 1.5 AC 1 SIN 0 5 60"
19051, "Description: The expression whose value is to be sampled.\nSyntax: <input expression>\nExamples: V(OUT), V(10)*I(V2)."
19052, "Description: The sampling period.\nSyntax: <value>\nExample: 5ns"
19053, "Description: Package type for PCB netlists. Click on the arrow in the VALUE field for a list of packages.\nSyntax: [Package Type]\nExample: DIP16"
19054, "<Gate Identifier>"
19055, "<Component Name for Layout>"
19056, "Description: Expression for calculating a frequency (F) dependent noise current in AC\nSyntax: <noise expression>\nExample: .026e-9/(1+F/1e10)"
19057, "Description: Controls the time precision of the transition.  Recommended range is 1m to 1u.\nSyntax: <expr>\nExample: 1e-4"
19059, "Description: Waveform expression from selected user waveform file\nSyntax: <expr>\nExample: V(1) vs T"
19060, "Description: Power consumption for Bill of Materials calculation of total circuit power used.\nSyntax: [value]\nExample: .07"
19061, "Description: Unit cost for Bill of Materials calculation of total circuit cost.\nSyntax: [value]\nExample: .07"
19062, "Description: Value or expression for computing capacitance value, plus an optional initial condition.\nSyntax: <value | expression> [LOT[/#][/GAUSS|/UNIFORM|/WCASE]=<tolvalue>[%]] [IC=<initial value>]\nExamples: 1u IC=6, 1u*(1+abs(V(C1)/100))\nExample: 1u LOT=10%"
19063, "Description: Transducer gain\nSyntax: <value>\nExample: 10.0"
19064, "Description: Value or expression for computing inductance value, plus an optional initial condition.\nSyntax: <value | expression> [LOT[/#][/GAUSS|/UNIFORM|/WCASE]=<tolvalue>[%]] [IC=<initial value>]\nExamples: .1 IC=2.3, .5*(1+atan(I(L1)/50))\nExample: .1 LOT=10%"
19065, "Description: User waveform file name\nSyntax: <name>\nExample: AMP1.USR"
19066, "Description: Keyword selects data format\nSyntax: [ [MAG|DB] | [RAD|DEG]] | [R_I]\nExample: MAG RAD"
19067, "Description: Voltage value\nSyntax: <value> [LOT[/#][/GAUSS|/UNIFORM|/WCASE]=<tolvalue>[%]]\nExample: 5.0"
19068, "Description: Current value\nSyntax: <value> [LOT[/#][/GAUSS|/UNIFORM|/WCASE]=<tolvalue>[%]]\nExample: 1.0"
19069, "Description: Tie name. Connects to other ties with the same name.\nSyntax: <name>\nExample: VCC"
19070, "Description: Digital state\nSyntax: <0|1|R|F|Z|X>\nExample: X"
19071, "To Add Help for a macro parameter add a .HELP %s  \"text\" to the macro file."
19072, "Syntax: [L=val] [W=val] [NF=val] [SA=val] [SB=val] [SD=val] [SCA=val] [SCB=val] [SCC=val] [SC=val] [MIN=val] [AD=val] [AS=val] [PD=val] [PS=val] [NRD=val] [NRS=val] [RBDB=val] [RBSB=val] [RBPB=val] [RBPS=val] [RBPD=val] [DELVTO=val] [XGW=val] [NGCON=val] [TRNQSMOD=val] [ACNQSMOD=val] [RBODYMOD=val] [RGATEMOD=val] [GEOMOD=val] [RGEOMOD=val]  [OFF] [TEMP=val] [IC=vds[,vgs[,vbs]]]\nExample: M=2 L=100u W=100u IC=6,2,.5"
19073, "Desc: length (m), width (m), drain/source areas (m*m) and peripheries (m), drain/source/gate/body squares, # of parallel devices, # of series devices, Scale parameter, Geometry parameter, device temperature, OFF keyword, ICs.\nSyntax: [M=val] [L=val] [W=val] [AD=val] [AS=val] [PD=val] [PS=val] [NRD=val] [NRS=val] [NRG=val] [NRB=val] [NP|M=val] [NS|N=val] [SCALE=val] [GEO=val] [TEMP=val] [OFF] [IC=vds[,vgs[,vbs]]]\nExample: M=2 L=100u W=100u IC=6,2,.5"
19074, "Sets the derivative method to be used for the individual function source.  Default uses the Global Settings value."
19075, "This is the number of times to repeat the user file waveform."
19076, "Defines a trigger expression that will initiate the start of the user waveform."
19077, "Description: Multiplier, length (m), width (m), drain and source areas (m*m) and peripheries (m), number of drain, source, gate, and body squares, OFF keyword, initial conditions.\nSyntax: [M=val] [L=val] [W=val] [AD=val] [AS=val] [PD=val] [PS=val] [NRD=val] [NRS=val] [NRG=val] [NRB=val] [NQSMOD=val] [ACNQSMOD=val] [OFF] [IC=vds[,vgs[,vbs]]]\nExample: M=2 L=100u W=100u IC=6,2,.5"
19078, "Description: Expression for computing charge value.\nSyntax: [expression] \nExample: SQRT(1+V(C1)^2)/V(C1)"
19079, "Description: Expression for computing flux value.\nSyntax: [expression] \nExample: 1u*ATAN(I(L2))"
19080, "Sets the number of data points used for the convolution method in transient analysis."
19081, "Sets the TMax for the convolution method in transient analysis where 1/TMax is the frequency sampling."
19103, "Defines the default font used as Grid Text."
19108, "Defines the color for components."
19109, "Defines the default font used as Attribute Text."
19110, "Description: Name of the file to be used for the Fit To Standard Values command\nSyntax: <file name>\nExample: standard.res"
19111, "Defines the color for wires."
19112, "Defines the color for Bus."
19113, "Defines the color for selected objects in Standard Select mode."
19114, "Defines the color for selected objects in Block Select mode."
19115, "Defines the color and font used for node numbers."
19116, "Defines the color for the Anchor."
19117, "Defines the color used for node voltages."
19118, "Defines the background color used for voltages in Dynamic AC."
19119, "Defines the color used for disabled objects."
19120, "Defines the color and font used for pin connections."
19121, "Defines the color used for Pin Markers, which are shown by double clicking on a component and checking 'Pin Markers'."
19122, "Defines the color of the box region."
19123, "Defines the color a path will be traced in a digital path operation."
19124, "Defines the highlight color of a node if Node Highlight in the Preferences is enabled."
19125, "Defines the color of an analysis grid."
19126, "Defines the color of the baseline."
19127, "Defines the color of an analysis background."
19128, "Defines the color and font used for analysis text."
19129, "Defines the color of any keyword used within the text page."
19130, "Defines the color of any text that creates an error within the text page."
19131, "Defines the background color used to highlight text that matches the search criteria."
19132, "Defines the waveform's graphical properties."
19133, "Description: Optional area multiplier, model parameters, OFF keyword, and initial conditions.\nSyntax: [AREA=<value>] [WB=<value>] [AGD=<value>] [KP=<value>] [TAU=<value>] [OFF] [IC=vgs[,vae[,vds[,veb]]]]\nExample: AREA=2 WB=120u OFF IC=10,5"
19134, "Defines the default color of the Curve Fit curve."
19135, "Defines the color of the encrypted text."
19148, "Digital 0 color."
19149, "Digital R color."
19150, "Digital F color."
19151, "Digital 1 color."
19152, "Digital X color."
19153, "Digital Z color."
19155, "Defines the color of text page comments denoted by the * or ; characters."
19156, "Defines the color of the associated background."
19157, "Defines the font used in text pages."
19158, "Defines the font color."
19159, "Defines the grid color."
19160, "Defines the wire color."
19161, "Defines the X background color."
19162, "Defines the Y background color."
19163, "Defines the Z background color."
19164, "Sets the high value color of the 3D plot when the User Patch Color is selected."
19165, "Sets the low value color of the 3D plot when the User Patch Color is selected."
19172, "Defines the text color used in text banners (as in Dynamic AC and DC)."
19173, "Defines the text background color used in text banners (as in Dynamic AC and DC)."
19174, "Defines the schematic grid color."
19175, "Defines title block border color."
19176, "Defines the schematic graph paper grid color."
19178, "Defines the font color."
19179, "Defines the grid color."
19180, "Defines the bar front color."
19181, "Defines the bar top/side color."
19182, "Defines the default background color."
19183, "Defines the color used for currents."
19184, "Defines the color used for power."
19185, "Description: The <input expression> is sampled whenever this <sample expression> is true\nSyntax: <sample expression>\nExample: (V(5,4) > 1.1) && (V(3) < 1.2)"
19186, "Controls the color of the waveform that the left cursor is on."
19187, "Controls the color of the waveform that the right cursor is on."
19188, "Sets the tracker color."
19189, "Sets the data point label color."
19190, "Applies any edits to all curves."
19191, "On state (High or Low) required to light the segments in a seven-segment display."
19192, "When the input expression is true, an event occurs. Elapsed time is set to zero and the count is incremented."
19193, "The voltage on the ELAPSED pin is equal to the elapsed time multiplied by this value."
19195, "This is the amount the counter is incremented each time an event occurs. It may be positive or negative."
19196, "This is the value on the COUNT pin when the RESET pin goes positive."
19197, "This is the minimum value on the COUNT pin."
19198, "This is the maximum value on the COUNT pin."
19199, "The state of the switch."
19200, "Scroll to first page tab."
19201, "Scroll page tabs to the left."
19202, "Scroll page tabs to the right."
19203, "Scroll to last page tab."
19204, "Scroll to first section tab."
19205, "Scroll section tabs to the left."
19206, "Scroll page tabs to the right."
19207, "Scroll to last section tab."
19208, "Sets the color and properties of the phase and gain margin lines."
19209, "Sets the color and properties of the phase and gain margin arrows."
19210, "Motor revolutions per second per volt across the control pins."
19211, "Motor series resistance."
19212, "Motor series inductance."
19213, "Relay series inductance."
19214, "Input current required to close the relay contacts."
19215, "Input current required to open the relay contacts."
19216, "This is the on resistance of the relay."
19217, "This is the off resistance of the relay."
19218, "This is the voltage required to turn the traffic lights on."
19219, "This is the color, voltage, current, resistance, and capacitance of the LED."
19220, "This is the low scale value of the meter."
19221, "This is the high scale value of the meter."
19222, "This is the scale factor(T,G,Meg,K,m,u,n,p,f) of the meter.\nThis option works only when Autoscale is Off."
19223, "If On this causes the meter to automatically adjust the scale.\nThis option is available only for analog meters."
19224, "This selects an analog or a digital display."
19225, "This selects whether the meter measures current or voltage."
19226, "This sets the voltage for the minimum height of the bar."
19227, "This sets the voltage for the maximum height of the bar."
19228, "This is the seed for random (?) values. The seed must be >0 to produce a repeatable sequence."
19229, "This is the DC input resistance of the meter:\nAmmeter default = .001.\nVoltmeter default = 1/GMIN."
19230, "Switch ON resistance."
19231, "Switch OFF resistance."
19232, "Description: All switches with the same group name are linked and behave the same. If NOT or ! precedes the name the behavior is reversed.\nSyntax: [[! | NOT] group_name].\nExample: group2\nExample: NOT grp3"
19233, "Input resistance of the relay coil."
19234, "If BIDIRECTIONAL is Yes, then the absolute (rather than the actual) value of the input current determines relay behavior.\n"
19236, "Specifies the name of the .WAV file to be used."
19237, "Specifies the channel number of the .WAV file to be used."
19238, "This is the number of times to repeat the wave file waveform."
19239, "Defines a trigger expression that will initiate the start of the wave waveform."
19240, "Scales the voltage of the wave file waveform."
19241, "Description: List of optional node connections.  Must connect to a node with a global node name ($G_name). \nSyntax: <<optional node>=<global node>>*\nExample: VDD=$G_VDD4000"
19242, "Defines color of label background."
19243, "Sets the color and properties of the phase and gain margin text."
19300, "Sets the grid color in the Model plots."
19301, "Sets the background color of the Model plot."
19302, "Sets the color of the Model plot curve"
19303, "Sets the color of the data points in the Model plot."
19304, "Sets the color and font of the X and Y scale text."
19305, "Description: Optional frequency-dependent expression for use in AC only. Replaces RESISTANCE above in AC only.\nSyntax: [expr]\nExample: 1e-4*(1+F/1e9)"
19306, "Description: Optional frequency-dependent expression for use in AC only. Replaces INDUCTANCE above in AC only.\nSyntax: [expr]\nExample: 1e-4*(1+F/1e9)"
19307, "Description: Optional frequency-dependent expression for use in AC only. Replaces CAPACITANCE above in AC only.\nSyntax: [expr]\nExample: 1e-4*(1+F/1e9)"
19520, "Specifies time where output is retained and plotted to the screen and/or printed to the numeric output."
19521, "Specifies the maximum time step for the run."
19522, "Determines the number of points to be printed in numeric output."
19523, "Specifies temperature values to be used for analysis. To[,From[,Step]]"
19524, "Specifies how many Retrace runs to do. The total run time will be this number times the Time Range."
19525, "Specifies ending time of the simulation."
19530, "Specifies frequency range of the simulation. fmax[,fmin]"
19531, "Determines the number of points for numeric output and analysis."
19533, "Specifies a limit on the rate of change of the first waveform."
19534, "Specifies the name of the source where input noise is calculated."
19535, "Specifies the nodes at which output noise is calculated. node1[,node2]"
19540, "Sets the secondary source sweep. Final[,Initial[,Step]]"
19541, "Specifies the name of the secondary source."
19542, "Sets the primary source sweep. Final[,Initial[,MaxStep]]"
19543, "Specifies the name of the primary source."
19544, "Determines the number of points calculated for numeric output."
19546, "Specifies a limit on the rate of change of the first waveform."
19547, "Specifies the part name of the Loop Gain Probe that will be used for the analysis."
19548, "Selects the method that will be used for the loop gain calculations."
19550, "Defines whether the X-axis is a linear or log scale."
19551, "Defines whether the Y-axis is a linear or log scale."
19552, "Defines the color of the waveform."
19553, "Places the waveform in the numeric output file."
19554, "Selects rectangular, polar, or Smith chart plot type."
19555, "Sets the waveform display status to one of three states: Green: Plot, Yellow: Save waveform but don't show  Red: Don't plot."
19556, "Allows moving, deleting, copying, pasting, and inserting waveforms."
19560, "Fundamental frequency for Fourier analysis and actual frequency of the input sine source."
19561, "Part name of the input source to be used in the analysis."
19562, "Amplitude of the input source to be used in the analysis. Format is High[,Low[,Step]]"
19563, "Name of load resistor."
19564, "Frequency range that the noise voltage will be calculated over for THD+N plots."
19566, "Simulation run time in terms of the number of fundamental cycles."
19567, "Tolerance used to stop the simulation as the waveform is assumed to have reached steady state."
19568, "Ratio used with the fundamental frequency to determine the maximum timestep."
19569, "Number of harmonics that will be used to calculate the total harmonic distortion values."
19571, "Smallest of two frequencies used in the Intermodulation Distortion calculation."
19572, "Largest of two frequencies used in the Intermodulation Distortion calculation."
19573, "Amplitude of the F1 input source to be used in the analysis. Linear/log format is High[,Low[,Step]]"
19574, "Amplitude of the F2 input source to be used in the analysis. Linear/log format is High[,Low[,Step]]"
19575, "Displays the combination of standard value elements needed to produce the current value.\nExample:1K+(100 | 47.5) means 1K in series with a parallel combination of 100 and 47.5."
19577, "Sets the Shape group from which the component will obtain its schematic shape."
19578, "Determines the number of points to be printed in numeric output for all time-domain waveforms."
19579, "Determines the number of points to be printed in numeric output for all frequency-domain waveforms."
19580, "Description: Touchstone File Name\nSyntax: <file name>\nExample: NEC5000.S2P"
19581, "Name of LO or clock source."
19582, "Smoke display text font and color"
19583, "Smoke display grid color"
19584, "Smoke display text pass color"
19585, "Smoke display text marginal color"
19586, "Smoke display text fail color"
19587, "Smoke display text invalid color"
19588, "Yes or No turns smoothing on or off. Inherit From Preferences uses the settings from the Preferences (Ctrl+Shift+P) dialog box."
19589, "For limit functions, the fraction of the interval between high and low values where smoothing begins. For TABLE functions, the fraction of the interval between X,Y points where smoothing begins. The fraction can be entered as a decimal(0.1) or a percent (10%)"
19590, "Determines whether smoothing interpolation is to be done logarithmically or linearly on each axis."
19591, "These are the %s parameters. Editing makes the parameters local to this circuit and saves them as a model statement in the text area."
19600, "Creates a SPICE text file description suitable for external SPICE simulators.\nCreate SPICE Netlist"
19601, "Creates a netlist suitable for SPICE2 compatible simulators."
19602, "Creates a netlist suitable for PSPICE compatible simulators."
19603, "Creates a netlist suitable for SPICE3 compatible simulators."
19604, "Creates a netlist suitable for HSPICE compatible simulators."
19605, "This is the PSPICE format with a few extensions unique to Micro-Cap."
19606, "Defines the file as an ambiguous SPICE format."
19607, "Defines the file as not being in any SPICE format."
19627, "Options"
19628, "Preferences"
19697, "Enables the Quick-help in-line assistance when entering analysis limits X and Y expressions."
19698, "Pixel width of the window splitter / drag bar. Use 15 or more with touch screens."
19699, "Enables the use of sound for illegal operations that don't invoke an error/warning dialog."
19700, "Enables the use of sound to denote when a simulation has finished running."
19701, "Enables the use of sound for warnings and errors."
19702, "Displays the toolbar bitmap, if defined, next to the command for items within a menu."
19703, "Adds a pair of parentheses to .DEFINE arguments. For example, .DEFINE A 1+2 becomes .DEFINE A (1+2)."
19705, "This option increments node text added as a result of a paste, step, drag copy, or mirror operation.\nIncrements Node text"
19706, "Reverts to Select mode in the schematic editor after any other action."
19707, "Shows the text area when a model statement is added."
19708, "Reverts to Select mode in the analysis after any other action."
19709, "Printouts would use the specified background color rather than the paper."
19710, "This option extends wires during drag operations to maintain connections.\nRubberbanding"
19711, "This option enables inertial cancellation in digital delays."
19712, "Sets the threshold limit that a symbolic derivative can hit before the numeric derivative is called as an alternative."
19713, "Adds a DC path to ground at all nodes."
19714, "Sets the cursor to the shape of the selected component in component mode."
19715, "Places the time in plots and other output files."
19716, "Places the date in plots and other output files."
19717, "The maximum number of parts in a Component menu column before it wraps to a new column. If 0 then don't wrap."
19718, "Automatically adds VCC and VEE power supplies and wires the OPAMP pins to the supplies."
19719, "Selects the Block Select display mode. In this mode the selected objects backgrounds are drawn."
19720, "Enables the Convergence Assistance routines."
19721, "Forces objects to originate on the nearest node.\nNode Snap"
19722, "When saving an EMF or WMF image file the background will be transparent."
19723, "Changes the curve that the cursor is on to the select color."
19724, "If the number of components in the schematic exceeds this value, the node numbers will only be recalculated when an analysis is entered."
19725, "Controls the maximum number of files shown in the File menu."
19726, "Controls the length of time that warnings will be displayed. The length is limited between 0 and 30 seconds."
19727, "Enables the analysis window to always be on top in probe."
19728, "Enables the progress display in the status bar."
19729, "Sets Tool bar icons to large size."
19730, "Restores default preferences."
19731, "Controls the maximum number of components in the recent component list."
19732, "Enables an automatic run when a circuit is edited when in an analysis mode.\nAuto Run"
19733, "Specifies the user name substituted for the $USER variable."
19734, "Specifies the company name substituted for the $COMPANY variable."
19735, "Enables the display of shapes when browsing the Component menu."
19736, "Highlights the wire and node name for a node when the mouse passes over it."
19737, "Imports components from a circuit file if those parts do not exist or are different than in the library."
19738, "Displays the full file path for each file reference in the Title bar."
19739, "Displays basic element information when the mouse is over the part."
19740, "When a part is cut/copied and then pasted, any associated Macro, Subckt, Localized File, model or define statement will also be moved with it."
19741, "Expands the information displayed for the element under the mouse cursor."
19742, "When enabled, all model parameters will be placed in alphabetical order when listed."
19743, "When enabled, the probe will drill down into a macro or subcircuit where waveforms can then be recalled."
19745, "When enabled, estimated entries will automatically be placed in the Stepping dialog box when a parameter is selected."
19746, "When enabled, the Help file will always stay on top of the Micro-Cap window."
19747, "Sets the number of data points that are calculated into a buffer prior to plotting. (max 127)"
19748, "When enabled, the group names in the Component panel are bolded."
19749, "When enabled, the Attribute dialog box will be automatically invoked as needed when a component is placed in the schematic."
19750, "Automatically loads each of the last used files, each time the program is run."
19751, "If checked, smoothing is enabled for Nonlinear Function and Table sources if Inherit From Preferences is selected in the Attribute dialog box for the source."
19752, "For limit functions, the fraction of the interval between high and low values where smoothing begins. For TABLE sources, the default fraction of the interval between X,Y points where smoothing begins. This is used for TABLE sources if Inherit From Preferences is selected for the source. The fraction can be entered as a decimal(0.1) or a percent (10%)."
19753, "Maximum number of recently used files to be auto-loaded when starting the program (0=no limit)."
19754, "Check .Define, .Func and .Array statements for Mismatched Parentheses and Braces."
19778, "Transparent"
19779, "Specifies the numeric format for optimized parameters."
19781, "Specifies the numeric format for analysis X scales."
19782, "Specifies the numeric format for analysis Y scales."
19783, "Specifies the numeric format for analysis Z scales."
19784, "Specifies numeric format for X values in Cursor mode tables and trackers."
19785, "Specifies numeric format for Y values in Cursor mode tables and trackers."
19786, "Specifies numeric format for Z values in Cursor mode tables and trackers."
19795, "Specifies the numeric format for any watch variables."
19796, "No Pattern"
19797, "No Fill"
19798, "No Color"
19800, "Black"
19801, "Maroon"
19802, "Green"
19803, "Olive"
19804, "Navy"
19805, "Purple"
19806, "Teal"
19807, "Light gray"
19808, "Dark gray"
19809, "Red"
19810, "Lime"
19811, "Yellow"
19812, "Blue"
19813, "Fuchsia"
19814, "Aqua"
19815, "White"
19816, "User defined color"
19865, "Current color of the object. Click to customize a color."
19999, "Restores the default color palette."
20026, "Tool Bar"
20027, "Defaults all buttons on the tool bar."
20028, "Defaults the selected button."
20104, "Places all buttons onto the tool bar."
20105, "Removes all buttons from the tool bar."
20110, "Places the tool bar at the top of the window."
20111, "Places the tool bar on the left side of the window."
20112, "Places the tool bar at the right side of the window."
20113, "Places the tool bar on the bottom of the window."
20115, "This lets you browse for the name of a component to add to the tool bar."
20117, "This lets type in the name of a component to add to the tool bar."
20199, "When wildcard names are used this enables a spectrum of colors to be used for the plots."
20202, "List of available waveforms."
20203, "Controls whether the waveform will be plotted or not."
20204, "Determines which graph the waveform will appear in."
20205, "Sets the waveform line thickness."
20206, "For stepped waveforms, enables a spectrum of colors to be used."
20207, "X expression of selected waveform."
20208, "Y expression of selected curve."
20210, "Automatically creates the title from the selected performance function."
20211, "List of available waveforms"
20212, "Sets the low range for the X axis."
20213, "Sets the low range for the Y axis."
20214, "Sets the high range for the X axis."
20215, "Sets the high range for the Y axis."
20216, "Auto scales the X axis."
20217, "Auto scales the Y axis."
20218, "If enabled, all curves in each plot group share a common Y scale.\nSame Y Scales"
20219, "Copies current X and Y scale and value formats to all waveforms."
20220, "If checked, all range edits are retained (copied to the Analysis Limits dialog box)."
20221, "Selects a log scale for the X axis."
20222, "Selects a log scale for the Y axis."
20223, "Slope calculation method for Cursor mode table."
20224, "Sets the X and Y grids to a static location in the plot window."
20225, "Spacing between X grids"
20226, "Spacing between Y grids"
20227, "Spacing between X bold grids"
20228, "Spacing between Y bold grids"
20229, "Sets the number of grids to be used when auto scaling the X range."
20230, "Sets the number of grids to be used when auto scaling the Y range."
20231, "Sets the Y scale of all waveforms in the plot group to the current Y values."
20300, "Title field"
20301, "Automatically creates the title."
20400, "Invokes the Package editor.\nPackage editor"
20402, "Defines the number of pins in the package."
20404, "Displays the component name for the selected package."
20406, "Adds a basic package where only one instance of the component is within the package."
20409, "Displays a list of all of the packages that are in the Package library."
20411, "Adds a complex package where more than one instance of the component is within the package."
20412, "Deletes the selected package."
20414, "Duplicates the selected package as a template for a new package."
20416, "Selects the first character of packages that will be displayed in the Package list."
20420, "Defines the package name specified for the component."
20421, "Package Name used when creating an Accel netlist file.  If blank, the Package field will be used."
20422, "Package Name used when creating an OrCad netlist file.  If blank, the Package field will be used."
20423, "Package Name used when creating a Protel netlist file.  If blank, the Package field will be used."
20424, "Package Name used when creating a PADS netlist file.  If blank, the Package field will be used."
20425, "Finds a package name within the Package library."
20426, "Creates a new file and adds it to the Package library.\nNew File"
20427, "Adds an existing file to the Package library.\nOpen File"
20428, "Merges a Package file on disk into the current Package file.\nMerge File"
20429, "Removes selected file from the Package library.\nRemove File"
20430, "Saves Package library.\nSave File"
20431, "Saves Package library under a new name.\nSave File As"
20433, "Displays the model information of the selected part."
20436, "Save Package Editor changes\nfor %s?"
20440, "Defines the component instance in the package that this pin is assigned to."
20441, "Defines the name of the pin that is used within Micro-Cap."
20442, "Defines the name of the pin that is used within the PCB netlist."
20443, "Total Packages %d"
20444, "Remove '%s' package file from the list?\n\nThe packages within the file will no longer be available to use in the schematic."
20492, "Monte Carlo choise."
20495, "Selects the input voltage branch that the window will be created for."
20497, "Selects the waveform branch that the operation will be performed on."
20499, "Selects the waveform branch that the operation will be performed on."
20501, "Temperature choice."
20552, "Stepped parameter choice."
20603, "Stepped parameter choice for X axis."
20613, "Performance function selector."
20614, "Performance function expression."
20615, "The low Y value for measuring rise time"
20616, "The high Y value for measuring rise time"
20617, "The low Y value for measuring fall time"
20618, "The high Y value for measuring fall time"
20619, "The Y value at which the width will be measured"
20620, "The Y value at which the X level will be measured"
20621, "The X value at which the Y level will be measured"
20622, "The low Y value at which the X delta will be measured"
20623, "The high Y value at which the X delta will be measured"
20624, "The low X value at which the Y delta will be measured"
20625, "The high X value at which the Y delta will be measured"
20626, "The low Y value at which the X range will be measured"
20627, "The high Y value at which the X range will be measured"
20628, "The low X value at which the Y range will be measured"
20629, "The high X value at which the Y range will be measured"
20630, "The X value at which the slope will be measured"
20631, "The starting point over which the function is measured"
20632, "The ending point over which the function is measured"
20633, "Specifies the instance to measure and plot"
20640, "Lets you review or edit the model parameter limit values.\nModel Parameter Limits Editor"
20700, "Automatically creates the title from the selected performance function."
20800, "&Expand..."
20801, "&Expand Lists"
20802, "Variables"
20803, "&Analysis Variables"
20804, "&Global Settings"
20807, "&Constants"
20808, "Symbolics"
20809, "&Functions"
20810, "&Operators"
20811, "Curve"
20812, "Buffers..."
20813, "Rename All Pages"
20814, "Renumber All Plots"
20850, "None"
20851, "Sort By Page"
20852, "Enable All for this Page"
20853, "Hide All for this Page"
20854, "Disable All for this Page"
20855, "Sort By Plot"
20856, "Enable All for this Plot"
20857, "Hide All for this Plot"
20858, "Disable All for this Plot"
20900, "Writing numeric output."
20901, "Conductance"
20902, "Capacitance"
20903, "Current"
20904, "Resistance"
20905, "Voltage"
20906, "Charge"
20907, "External Voltage"
20908, "Internal Voltage"
20909, "Power"
20910, "Beta"
20911, "Frequency"
20912, "Noise"
20913, "Transistor Gain"
20914, "Geometry"
20915, "Terms:"
20916, "Operating Point for Devices of Type %s"
20917, "AC values for %s (%s)"
20918, "DC Operating Point Voltages"
20919, "AC Voltages at Frequency=%g (%s)"
20920, "Variable 1 Method"
20921, "Variable 1 Name"
20922, "Variable 1 Range"
20923, "Variable 2 Method"
20924, "Variable 2 Name"
20925, "Variable 2 Range"
20961, "Run"
20963, "All"
20964, "Case"
20965, "DC Variable 2"
20985, "Nodes"
20986, "Voltages"
20987, "Inductors"
20988, "Currents"
20989, "Levels"
20990, "Conditions"
20991, "Power Terms"
20992, "Energy"
21200, "Starts the optimizer.\nOptimize"
21210, "Deletes this parameter."
21220, "Adds a new parameter to optimize."
21230, "Selects a parameter to optimize"
21240, "Sets whether the parameter will be optimized or not."
21250, "The parameter to be optimized"
21260, "The lowest acceptable value for the optimized parameter"
21270, "Displays the initial value of the parameter prior to the optimization."
21280, "The highest acceptable value for the optimized parameter"
21290, "The current value of the parameter"
21300, "The optimized value of the parameter"
21410, "Maximizes, minimizes, or equates the selected performance function."
21420, "Deletes this optimizing criterion."
21430, "Adds a new optimizing criterion."
21440, "Selects the performance function that is to be optimized."
21450, "The performance function to be optimized"
21460, "Specifies the branch that the optimizer is to work on."
21470, "Displays the branch that the optimizer is working on."
21480, "The value to match the performance function to if the Equates method is selected"
21490, "The current value of the performance function"
21500, "The optimized value of the performance function"
21510, "The error of the individual criterion."
21521, "When a new optimization routine starts, it will use the initial parameter values to start with."
21522, "When a new optimization routine starts, it will use the last values from the previous routine to start with."
21523, "Selects the Random mode. In this mode the program does a random search at each grid point."
21524, "Selects the Step All mode. In this mode the program evaluates once at each grid point."
21525, "Selects a starting point method."
21526, "Use a logarithmic grid for Step All and Random modes"
21527, "Keeps a text log of optimization results."
21530, "Imports values from a file to be used as Equate values with the Y_Level performance operator."
21531, "Clears all entries from the That fields."
21533, "Initial"
21534, "Existing"
21535, "Minimizes the dialog box during an optimization to better view the plot being updated."
21536, "Changes the plot values in the background to match the current optimized values."
21539, "Optimizer run time"
21541, "RMS measure of the total error."
21543, "Average percentage error of the model versus the datapoints."
21545, "Starts the optimizer."
21546, "Stops the optimizer."
21547, "Changes the circuit parameter values to the optimized values."
21548, "Sets the numeric format for values displayed in the optimizer dialog box."
21549, "Specifies success criteria for optimizer."
21550, "Invokes a dialog box that lets constraints be entered as Boolean expressions such as V(VCC)*I(VCC)<=100mW."
21551, "Get"
21552, "Random"
21553, "Step All"
21555, "Specifies the number grids to be used in the Random mode."
21558, "Specifies the number of trys at each grid point in Random mode."
21561, "Constraint specified as a Boolean expression such as V(VCC)*I(VCC)<=100mW"
23000, "This page controls which warnings will be displayed in Micro-Cap."
23001, "Enables all warnings."
23002, "Generates a warning if an edited file is closed without saving it."
23003, "Asks for permission before quitting."
23004, "Issues a warning when OPAMP supplies are added."
23005, "Issues a warning when adding GMIN resistors to resolve DC path to ground problems."
23006, "Issues a warning when the Time Range/Maximum Time Step ratio is excessively large."
23007, "Issues a warning when the number of Data Points calculated is excessively large."
23008, "Issues a warning when the Revert command is used."
23009, "Issues a warning when no AC signals are in the circuit and an AC analysis is attempted."
23010, "Issues a warning when a source is creating an excessive number of points."
23011, "Issues a warning when a part name and a node name share the same name."
23012, "Issues a warning when the SPICE3 Temp parameter is used as a device attribute."
23013, "Issues a warning when a component's Level parameter is changed where the model parameters would need to change."
23014, "Issues a warning when both TNOM and T_MEASURED have been specified for a component."
23015, "Issues a warning when a time varying expression and a model attribute are defined for a component."
23016, "Issues a warning when changing device part names that use invalid characters."
23017, "Issues a warning when multiple devices share the same part name."
23018, "Issues a warning that threads are disabled when a Leave or Retrace run is selected."
23019, "Issues a warning when generating .IC or .NODDESET statements from the State Variables Editor."
23020, "Issues a warning if an S or F variable is used in the transmission line when running any analysis besides AC analysis."
23021, "Issues a warning when one of the temperature coefficients in an R, L, or C is set to an excessive value."
23022, "Issues a warning when there are any duplicate component names after exiting the Component editor."
23023, "Enables or disables digital warnings."
23024, "Disables all warnings."
23025, "Issues a warning when the final ')' is missing."
23026, "Issues a warning when there is a purely numeric node name which could be confused with a node number."
23027, "Issues a warning about improper FFT X variables."
23028, "Issues a warning before creating a Monte Carlo circuit for the case."
23029, "Issues a warning when you make a pervasive change in Smoke."
23030, "Igrnores unknown Model Parameters."
23031, "Check for misuse of M multipiler (should use MEG multipler)"
24101, "Displays the Thumbnail Plot.\nThumbnail Plot"
24153, "This page displays general Micro-Cap option preferences."
24154, "This page displays analysis option preferences."
24155, "This page displays circuit option preferences."
24210, "Invokes the Measurements dialog box which displays results from Performance Functions or .Measure statements.\nMeasurements"
24214, "\nOptions"
24215, "\nAutosize"
24216, "\nExcel"
24217, "\nText"
24218, "\nAdd Item"
24219, "\nRemove Item"
24222, "\nDisable Item"
24223, "\nEnable Item"
24300, "Enables X Axis scaling. If disabled the X axis scale can not be changed.\nEnables X Axis scaling."
24301, "Enables Y Axis scaling. If disabled the Y axis scale can not be changed.\nEnables Y Axis scaling."
24302, "Keeps the X Axis scales of waveforms in different plot groups the same for panning, zooming, and scaling.\nKeep X Scales the Same"
24493, "Tolerance Low"
57345, "  "
57601, "Opens an existing schematic, SPICE, model library, or document file.\nOpen"
57602, "Closes the Front Window.\nClose"
57603, "Saves the active file to disk.\nSave"
57604, "Saves the active file to disk under a new name.\nSave As"
57606, "Selects print options.\nPrinter Setup"
57607, "Prints the active file.\nPrint"
57609, "Shows how the printed schematic or plot will look.\nPrint Preview"
57632, "Deletes the selected region or object without copying it to the clipboard.\nDelete"
57634, "Copies the selected region or object to the clipboard.\nCopy"
57635, "Deletes the selected region or object and copies it to the clipboard.\nCut"
57637, "Pastes the region or object in clipboard to the open window.\nPaste"
57642, "Selects everything in window or text field.\nSelect All"
57643, "Undoes the last operation.\nUndo"
57644, "Restores the last undo operation.\nRedo"
57649, "Arrange icons at the bottom of the window.\nArrange Icons"
57650, "Arrange windows so they overlap\nCascade Windows"
57651, "Arrange windows horizontally as non-overlapping tiles.\nTile Horizontal"
57652, "Arrange windows vertically as non-overlapping tiles.\nTile Vertical"
57653, "Split the active window into panes\nSplit"
59143, "Clock"
59144, "XXXXXXXXXXXXXXXXX"
59145, "LnXXXXXX"
59146, "    "
59147, "100%"
59148, "xxxxxxxxxxx"
59149, "Threads=1024"
61184, "Change the window size"
61185, "Change the window position"
61186, "Reduce the window to an icon"
61187, "Enlarge the window to full size"
61188, "Switch to the next document window"
61189, "Switch to the previous document window"
61190, "Close the active window and prompts to save the documents"
61202, "Restore the window to normal size"
61203, "Activate Task List"
61215, "Activate this window"
61402, "Open the selected item"
61440, "Open"
61441, "Save As"
61442, "All Files (*.*)"
61443, "Untitled"
61445, "Close print preview mode\nCancel Preview"
61457, "&Hide"
61472, "No error message is available."
61473, "Attempted an unsupported operation."
61474, "A required resource was unavailable."
61475, "Out of memory."
61476, "An unknown error has occurred."
61477, "Encountered an improper argument."
61696, "Incorrect filename."
61697, "Failed to open document."
61698, "Failed to save document."
61699, "Save changes to %1?"
61700, "Failed to create empty document."
61701, "The file is too large to open."
61702, "Could not start print job."
61703, "Failed to launch help."
61704, "Internal application error."
61705, "Command failed."
61706, "Insufficient memory to perform operation."
61707, "System registry entries have been removed and the INI file (if any) was deleted."
61708, "Not all of the system registry entries (or INI file) were removed."
61709, "This program requires the file %s, which was not found on this system."
61710, "This program is linked to the missing export %s in the file %s. This machine may have an incompatible version of %s."
61712, "Enter an integer."
61713, "Enter a number."
61714, "Enter an integer between %1 and %2."
61715, "Enter a number between %1 and %2."
61716, "Enter no more than %1 characters."
61717, "Select a button."
61718, "Enter an integer between 0 and 255."
61719, "Enter a positive integer."
61720, "Enter a date and/or time."
61721, "Enter a currency."
61722, "Enter a GUID."
61723, "Enter a time."
61724, "Enter a date."
61744, "%1: %2\nContinue running script?"
61745, "Dispatch exception: %1"
61836, "Unable to read write-only property."
61837, "Unable to write read-only property."
61872, "No error occurred."
61873, "An unknown error occurred while accessing %1."
61874, "Attempted to write to the reading %1."
61875, "Attempted to access %1 past its end."
61876, "Attempted to read from the writing %1."
61877, "%1 has a bad format."
61878, "%1 contained an unexpected object."
61879, "%1 contains an incorrect schema."
61888, "pixels"
62177, "Uncheck"
62178, "Check"
62179, "Mixed"
62180, "One or more auto-saved documents were found."
62181, "These are more recently saved than the currently open documents and contain changes that were made before the application closed."
62182, "Do you want to recover these auto-saved documents?"
62183, "Note that if you choose to recover the auto-saved documents, you must explicitly save them to overwrite the original documents.  If you choose to not recover the auto-saved versions, they will be deleted."
62184, "Recover the auto-saved documents\nOpen the auto-saved versions instead of the explicitly saved versions"
62185, "Don't recover the auto-saved documents\nUse the last explicitly saved versions of the documents"
62186, "%s [Recovered]"
65049, "Regular"
65050, "Bold"
65051, "Italic"
65052, "Bold Italic"
}


// Ðåñóðñ ÑÒÐÎÊÀ
//
// Êàæäàÿ ñòðîêà â ðåñóðñå ñòðîê ñîñòîèò èç ÈÄÅÍÒÈÔÈÊÀÒÎÐÀ è, ñëåäóþùåé çà çàïÿòîé,
// ôàêòè÷åñêîé ñòðîêîé.
// ÈÄÅÍÒÈÔÈÊÀÒÎÐ ñëóæèò ññûëêîé äëÿ ïðîãðàììû è Âû íå äîëæíû èçìåíÿòü åãî.
// Êàæäàÿ ñòðîêà äîëæíà áûòü â îäíîé ñòðîêå è çàêëþ÷åíà â êàâû÷êè.
//
// Ñïåöèàëüíûå ñèìâîëû, âðîäå êàâû÷åê (") è íàêëîííîé ÷åðòû âëåâî (\) íóæíî âûâîäèòü
// çà íàêëîííóþ ÷åðòó âëåâî.
// Ïðèìåð öèòèðóåìîãî ñëîâà:
//   1538, "Florian \"Bome\" Bömers"
//
// Äëÿ êîíöà ñòðîêè, âêëþ÷èòå \n. \t çàìåíÿåò òàáóëÿöèþ.
// ----------------------------------------------------------------------------
// Äëÿ ïîëó÷åíèÿ äîïîëíèòåëüíîé èíôîðìàöèè, ñì. èíòåðàêòèâíóþ ñïðàâî÷íóþ Microsoft:
// http://msdn.microsoft.com/library/default.asp?url=/library/en-us/tools/tools/stringtable_resource.asp